Macros
Turn the peripherals off during WFI/WFE
Peripheral Driver » LL Driver » CGC » Defines » CGC Exported Constants

## Macros
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_UART_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART0
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_UART_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART1
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_SPI_M_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_SPIM
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_SPI_S_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_SPIS
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_PWM_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_PWM0
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_PWM_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_PWM1
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C0
#define | LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C1
#define | LL_CGC_MCU_PERIPH_SERIALS_SLP_OFF ((uint32_t)0x00003CC3UL)
#define | LL_CGC_MCU_PERIPH_SERIALS_SLP_ALL ((uint32_t)0x00003CC3UL)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_0_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C0

Turn the i2c0 off during WFI/WFE

Definition at line 162 of file gr533x_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_1_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_I2C1

Turn the i2c1 off during WFI/WFE

Definition at line 163 of file gr533x_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_PWM_0_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_PWM_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_PWM0

Turn the pwm0 off during WFI/WFE

Definition at line 160 of file gr533x_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_PWM_1_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_PWM_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_PWM1

Turn the pwm1 off during WFI/WFE

Definition at line 161 of file gr533x_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_SPI_M_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_SPI_M_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_SPIM

Turn the spi_m off during WFI/WFE

Definition at line 158 of file gr533x_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_SPI_S_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_SPI_S_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_SPIS

Turn the spi_s off during WFI/WFE

Definition at line 159 of file gr533x_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_UART_0_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_UART_0_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART0

Turn the uart0 off during WFI/WFE

Definition at line 156 of file gr533x_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_CG_LP_EN_UART_1_SLP_OFF

#define LL_CGC_MCU_PERIPH_CG_LP_EN_UART_1_SLP_OFF MCU_SUB_PERIPH_CLK_SLP_OFF_UART1

Turn the uart1 off during WFI/WFE

Definition at line 157 of file gr533x_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_SERIALS_SLP_ALL

#define LL_CGC_MCU_PERIPH_SERIALS_SLP_ALL ((uint32_t)0x00003CC3UL)

Serial blocks

Definition at line 166 of file gr533x_ll_cgc.h.

## ◆ LL_CGC_MCU_PERIPH_SERIALS_SLP_OFF

#define LL_CGC_MCU_PERIPH_SERIALS_SLP_OFF ((uint32_t)0x00003CC3UL)

Serial blocks

Definition at line 165 of file gr533x_ll_cgc.h.