Public Attributes | List of all members
_exflash_timing_param Struct Reference
Peripheral Driver » HAL Driver » EXFLASH » Structures

exFlash AC characteristics More...

`#include <gr533x_hal_exflash.h>`

## Public Attributes
uint8_t | flash_tVSL
uint8_t | flash_tESL
uint8_t | flash_tPSL
uint8_t | flash_tPRS
uint8_t | flash_tERS
uint8_t | flash_tDP
uint8_t | flash_tRES2
uint8_t | flash_tRDINT

## Detailed Description

exFlash AC characteristics

Definition at line 211 of file gr533x_hal_exflash.h.

## Member Data Documentation

## ◆ flash_tDP

uint8_t _exflash_timing_param::flash_tDP

CS# High to Deep Power-down Mode. Uint: 5us

Definition at line 223 of file gr533x_hal_exflash.h.

## ◆ flash_tERS

uint8_t _exflash_timing_param::flash_tERS

Latency between erase resume and next suspend. Uint: 5us

Definition at line 221 of file gr533x_hal_exflash.h.

## ◆ flash_tESL

uint8_t _exflash_timing_param::flash_tESL

Erase suspend latency. Uint: 5us

Definition at line 215 of file gr533x_hal_exflash.h.

## ◆ flash_tPRS

uint8_t _exflash_timing_param::flash_tPRS

Latency between program resume and next suspend. Uint: 5us

Definition at line 219 of file gr533x_hal_exflash.h.

## ◆ flash_tPSL

uint8_t _exflash_timing_param::flash_tPSL

Program suspend latency. Uint: 5us

Definition at line 217 of file gr533x_hal_exflash.h.

## ◆ flash_tRDINT

uint8_t _exflash_timing_param::flash_tRDINT

Read status register interval when wait busy. Uint: 5us

Definition at line 227 of file gr533x_hal_exflash.h.

## ◆ flash_tRES2

uint8_t _exflash_timing_param::flash_tRES2

CS# High To Standby Mode With Electronic Signature Read. Uint: 5us

Definition at line 225 of file gr533x_hal_exflash.h.

## ◆ flash_tVSL

uint8_t _exflash_timing_param::flash_tVSL

VCC(min.) to device operation. Uint: 10us

Definition at line 213 of file gr533x_hal_exflash.h.

The documentation for this struct was generated from the following file:

- gr533x_hal_exflash.h