Enumerations
HAL DMA state
Peripheral Driver » HAL Driver » DMA » Enumerations

## Enumerations
enum | hal_dma_state_t { HAL_DMA_STATE_RESET = 0x00U, HAL_DMA_STATE_READY = 0x01U, HAL_DMA_STATE_BUSY = 0x02U, HAL_DMA_STATE_TIMEOUT = 0x03U, HAL_DMA_STATE_ERROR = 0x04U }
| HAL DMA State Enumerations definition. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ hal_dma_state_t

enum hal_dma_state_t

HAL DMA State Enumerations definition.

Enumerator
HAL_DMA_STATE_RESET | DMA not yet initialized or disabled
HAL_DMA_STATE_READY | DMA process success and ready for use
HAL_DMA_STATE_BUSY | DMA process is ongoing
HAL_DMA_STATE_TIMEOUT | DMA timeout state
HAL_DMA_STATE_ERROR | DMA error state

Definition at line 76 of file gr533x_hal_dma.h.