Functions
Functions
Peripheral Driver » LL Driver » CGC

## Functions
__STATIC_INLINE void | ll_cgc_set_wfi_off_hclk_0 (uint32_t clk_mask)
| Some peripherals automatic turn off clock during WFI. (Include: Security/SIM/HTB/PWM/ ROM/SNSADC/GPIO/DMA/BLE_BRG/APB_SUB/SERIAL/I2S) More...
__STATIC_INLINE uint32_t | ll_cgc_get_wfi_off_hclk_0 (void)
| Return to clock blocks that is turned off during WFI.(Include: Security/SIM/HTB/PWM/ ROM/SNSADC/GPIO/DMA/BLE_BRG/APB_SUB/SERIAL/I2S) More...
__STATIC_INLINE void | ll_cgc_set_wfi_off_hclk_1 (uint32_t clk_mask)
| Some peripherals automatic turn off clock during WFI. (Include: AON_MCUSUB/XF_XQSPI/SRAM) More...
__STATIC_INLINE uint32_t | ll_cgc_get_wfi_off_hclk_1 (void)
| Return to clock blocks that is turned off during WFI.(Include: AON_MCUSUB/XF_XQSPI/SRAM) More...
__STATIC_INLINE void | ll_cgc_set_wfi_off_hclk_2 (uint32_t clk_mask)
| Some peripherals automatic turn off clock during WFI. (Include: SECU_DIV4/XQSPI_DIV4) More...
__STATIC_INLINE uint32_t | ll_cgc_get_wfi_off_hclk_2 (void)
| Return to clock blocks that is turned off during WFI.(Include: AON_MCUSUB/XF_XQSPI/SRAM) More...
__STATIC_INLINE void | ll_cgc_set_wfi_off_hclk_3 (uint32_t clk_mask)
| Some peripherals automatic turn off clock during WFI. (Include: UART/DSPI.I2C/QSPI.etc) More...
__STATIC_INLINE uint32_t | ll_cgc_get_wfi_off_hclk_3 (void)
| Return to clock blocks that is turned off during WFI.(Include: UART/DSPI.I2C/QSPI.etc) More...
__STATIC_INLINE void | ll_cgc_set_wfi_off_hclk_4 (uint32_t clk_mask)
| Some peripherals automatic turn off clock during WFI. (Include: AES/HMAC/PKC/RNG.etc) More...
__STATIC_INLINE uint32_t | ll_cgc_get_wfi_off_hclk_4 (void)
| Return to clock blocks that is turned off during WFI.(Include: AES/HMAC/PKC/RNG.etc) More...
__STATIC_INLINE void | ll_cgc_set_force_off_hclk_0 (uint32_t clk_mask)
| Some peripherals force turn off clock. (Include: Security/SIM/HTB/PWM/ROM/SNSADC/GPIO/ DMA/BLE_BRG/APB_SUB/SERIAL/I2S) More...
__STATIC_INLINE uint32_t | ll_cgc_get_force_off_hclk_0 (void)
| Return to clock blocks that was forcibly closed.(Include: Security/SIM/HTB/ ROM/SNSADC/GPIO/DMA/BLE_BRG/APB_SUB/SERIAL/I2S) More...
__STATIC_INLINE void | ll_cgc_set_force_off_hclk_1 (uint32_t clk_mask)
| Some peripherals force turn off clock. (Include: AON_MCUSUB/XF_XQSPI/SRAM) More...
__STATIC_INLINE uint32_t | ll_cgc_get_force_off_hclk_1 (void)
| Return to clock blocks that was forcibly closed.(Include: AON_MCUSUB/XF_XQSPI/SRAM) More...
__STATIC_INLINE void | ll_cgc_set_force_off_hclk_2 (uint32_t clk_mask)
| Some peripherals force turn off clock. (Include: UART0_HCLK/UART1_HCLK/UART2_HCLK/UART3_HCLK/UART4_HCLK/UART5_HCLK/ I2C0_HCLK/I2C1_HCLK/SPIM_HCLK/SPIS_HCLK/QSPI0_HCLK/QSPI1_HCLK/I2S_HCLK/SECU_DIV4_PCLK/XQSPI_DIV4_PCLK/PWM0/PWM1) More...
__STATIC_INLINE uint32_t | ll_cgc_get_force_off_hclk_2 (void)
| Return to clock blocks that was forcibly closed.(Include: UART0_HCLK/UART1_HCLK/UART2_HCLK/UART3_HCLK/UART4_HCLK/UART5_HCLK/ I2C0_HCLK/I2C1_HCLK/SPIM_HCLK/SPIS_HCLK/QSPI0_HCLK/QSPI1_HCLK/I2S_HCLK/SECU_DIV4_PCLK/XQSPI_DIV4_PCLK/PWM0/PWM1) More...
__STATIC_INLINE void | ll_cgc_set_force_off_hclk_3 (uint32_t clk_mask)
| Some peripherals automatic turn off clock. (Include: AES/HMAC/PKC/RNG.etc) More...
__STATIC_INLINE uint32_t | ll_cgc_get_force_off_hclk_3 (void)
| Return to clock blocks that is turned off.(Include: AES/HMAC/PKC/RNG.etc) More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_secu_hclk (void)
| Enable security blocks(including AES, PKC, Present, HMAC) automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_secu_hclk (void)
| Disable security blocks(including AES, PKC, Present, HMAC) automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_secu_hclk (void)
| Indicate whether the security blocks(including AES, PKC, Present, HMAC) automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_sim_hclk (void)
| Enable SIM automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_sim_hclk (void)
| Disable SIM automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_sim_hclk (void)
| Indicate whether the SIM automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_htb_hclk (void)
| Enable Hopping Table automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_htb_hclk (void)
| Disable Hopping Table automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_htb_hclk (void)
| Indicate whether the Hopping Table automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_pwm_hclk (void)
| Enable PWM automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_pwm_hclk (void)
| Disable PWM automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_pwm_hclk (void)
| Indicate whether the PWM automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_rom_hclk (void)
| Enable ROM automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_rom_hclk (void)
| Disable ROM automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_rom_hclk (void)
| Indicate whether the ROM automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_snsadc_hclk (void)
| Enable SNSADC automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_snsadc_hclk (void)
| Disable SNSADC automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_snsadc_hclk (void)
| Indicate whether the SNSADC automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_gpio_hclk (void)
| Enable GPIO automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_gpio_hclk (void)
| Disable GPIO automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_gpio_hclk (void)
| Indicate whether the GPIO automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_dma_hclk (void)
| Enable DMA automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_dma_hclk (void)
| Disable DMA automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_dma_hclk (void)
| Indicate whether the DMA automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_ble_brg_hclk (void)
| Enable BLE Bridge automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_ble_brg_hclk (void)
| Disable BLE Bridge automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_ble_brg_hclk (void)
| Indicate whether the BLE Bridge automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_apb_sub_hclk (void)
| Enable APB Subsystem automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_apb_sub_hclk (void)
| Disable APB Subsystem automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_apb_sub_hclk (void)
| Indicate whether the APB Subsystem automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_serial_hclk (void)
| Enable serial blocks(including I2C, UART, QSPI, I2S, SPI) automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_serial_hclk (void)
| Disable serial blocks(including I2C, UART, QSPI, I2S, SPI) automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_serial_hclk (void)
| Indicate whether the serial blocks(including I2C, UART, QSPI, I2S, SPI) automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_aon_mcusub_hclk (void)
| Enable AON_MUCSUB automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_aon_mcusub_hclk (void)
| Disable AON_MUCSUB automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_aon_mcusub_hclk (void)
| Indicate whether the AON_MUCSUB automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_xqspi_hclk (void)
| Enable XQSPI automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_xqspi_hclk (void)
| Disable XQSPI automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_xqspi_hclk (void)
| Indicate whether the XQSPI automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_sram_hclk (void)
| Enable SRAM automatic turn off clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_sram_hclk (void)
| Disable SRAM automatic turn off clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_sram_hclk (void)
| Indicate whether the SRAM automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_secu_div4_hclk (void)
| Enable security blocks automatic turn off div4 clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_secu_div4_hclk (void)
| Disable security blocks automatic turn off div4 clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_secu_div4_hclk (void)
| Indicate whether the security blocks automatic turn off div4 clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_xqspi_div4_hclk (void)
| Enable XQSPI automatic turn off div4 clock during WFI. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_xqspi_div4_hclk (void)
| Disable XQSPI automatic turn off div4 clock during WFI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_xqspi_div4_hclk (void)
| Indicate whether the XQSPI automatic turn off div4 clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_secu_hclk (void)
| Enabling force to turn off the clock for security blocks(including AES, PKC, Present, HMAC). More...
__STATIC_INLINE void | ll_cgc_disable_force_off_secu_hclk (void)
| Disabling force to turn off the clock for security blocks(including AES, PKC, Present, HMAC). More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_secu_hclk (void)
| Indicate whether the clock for security blocks(including AES, PKC, Present, HMAC) is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_htb_hclk (void)
| Enabling force to turn off the clock for Hopping Table. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_htb_hclk (void)
| Disabling force to turn off the clock for Hopping Table. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_htb_hclk (void)
| Indicate whether the clock for Hopping Table is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_rom_hclk (void)
| Enabling force to turn off the clock for ROM. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_rom_hclk (void)
| Disabling force to turn off the clock for ROM. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_rom_hclk (void)
| Indicate whether the clock for ROM is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_snsadc_hclk (void)
| Enabling force to turn off the clock for SNSADC. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_snsadc_hclk (void)
| Disabling force to turn off the clock for SNSADC. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_snsadc_hclk (void)
| Indicate whether the clock for SNSADC is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_gpio_hclk (void)
| Enabling force to turn off the clock for GPIO. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_gpio_hclk (void)
| Disabling force to turn off the clock for GPIO. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_gpio_hclk (void)
| Indicate whether the clock for GPIO is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_ble_brg_hclk (void)
| Enabling force to turn off the clock for BLE Bridge. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_ble_brg_hclk (void)
| Disabling force to turn off the clock for BLE Bridge. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_ble_brg_hclk (void)
| Indicate whether the clock for BLE Bridge is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_apb_sub_hclk (void)
| Enabling force to turn off the clock for APB Subsystem. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_apb_sub_hclk (void)
| Disabling force to turn off the clock for APB Subsystem. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_apb_sub_hclk (void)
| Indicate whether the clock for APB Subsystem is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_serial_hclk (void)
| Enabling force to turn off the clock for serial blocks(including I2C, UART, QSPI, I2S, SPI). More...
__STATIC_INLINE void | ll_cgc_disable_force_off_serial_hclk (void)
| Disabling force to turn off the clock for serial blocks(including I2C, UART, QSPI, I2S, SPI). More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_serial_hclk (void)
| Indicate whether the clock for serial blocks(including I2C, UART, QSPI, I2S, SPI) is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_aon_mcusub_hclk (void)
| Enabling force to turn off the clock for AON_MUCSUB. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_aon_mcusub_hclk (void)
| Disabling force to turn off the clock for AON_MUCSUB. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_aon_mcusub_hclk (void)
| Indicate whether the clock for AON_MUCSUB is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_xqspi_hclk (void)
| Enabling force to turn off the clock for XQSPI. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_xqspi_hclk (void)
| Disabling force to turn off the clock for XQSPI. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_xqspi_hclk (void)
| Indicate whether the clock for XQSPI is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_sram_hclk (void)
| Enabling force to turn off the clock for SRAM. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_sram_hclk (void)
| Disabling force to turn off the clock for SRAM. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_sram_hclk (void)
| Indicate whether the clock for SRAM is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_uart0_hclk (void)
| Enabling force to turn off the clock for UART0. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_uart0_hclk (void)
| Disabling force to turn off the clock for UART0. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_uart0_hclk (void)
| Indicate whether the clock for UART0 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_uart1_hclk (void)
| Enabling force to turn off the clock for UART1. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_uart1_hclk (void)
| Disabling force to turn off the clock for UART1. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_uart1_hclk (void)
| Indicate whether the clock for UART1 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_uart2_hclk (void)
| Enabling force to turn off the clock for UART2. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_uart2_hclk (void)
| Disabling force to turn off the clock for UART2. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_uart2_hclk (void)
| Indicate whether the clock for UART2 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_uart3_hclk (void)
| Enabling force to turn off the clock for UART3. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_uart3_hclk (void)
| Disabling force to turn off the clock for UART3. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_uart3_hclk (void)
| Indicate whether the clock for UART3 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_uart4_hclk (void)
| Enabling force to turn off the clock for UART4. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_uart4_hclk (void)
| Disabling force to turn off the clock for UART4. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_uart4_hclk (void)
| Indicate whether the clock for UART4 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_uart5_hclk (void)
| Enabling force to turn off the clock for UART5. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_uart5_hclk (void)
| Disabling force to turn off the clock for UART5. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_uart5_hclk (void)
| Indicate whether the clock for UART5 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_i2c0_hclk (void)
| Enabling force to turn off the clock for I2C0. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_i2c0_hclk (void)
| Disabling force to turn off the clock for I2C0. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_i2c0_hclk (void)
| Indicate whether the clock for I2C0 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_i2c1_hclk (void)
| Enabling force to turn off the clock for I2C1. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_i2c1_hclk (void)
| Disabling force to turn off the clock for I2C1. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_i2c1_hclk (void)
| Indicate whether the clock for I2C1 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_i2c2_hclk (void)
| Enabling force to turn off the clock for I2C2. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_i2c2_hclk (void)
| Disabling force to turn off the clock for I2C2. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_i2c2_hclk (void)
| Indicate whether the clock for I2C2 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_i2c3_hclk (void)
| Enabling force to turn off the clock for I2C3. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_i2c3_hclk (void)
| Disabling force to turn off the clock for I2C3. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_i2c3_hclk (void)
| Indicate whether the clock for I2C3 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_i2c4_hclk (void)
| Enabling force to turn off the clock for I2C4. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_i2c4_hclk (void)
| Disabling force to turn off the clock for I2C4. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_i2c4_hclk (void)
| Indicate whether the clock for I2C4 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_i2c5_hclk (void)
| Enabling force to turn off the clock for I2C5. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_i2c5_hclk (void)
| Disabling force to turn off the clock for I2C5. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_i2c5_hclk (void)
| Indicate whether the clock for I2C5 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_spim_hclk (void)
| Enabling force to turn off the clock for SPIM. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_spim_hclk (void)
| Disabling force to turn off the clock for SPIM. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_spim_hclk (void)
| Indicate whether the clock for SPIM is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_spis_hclk (void)
| Enabling force to turn off the clock for SPIS. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_spis_hclk (void)
| Disabling force to turn off the clock for SPIS. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_spis_hclk (void)
| Indicate whether the clock for SPIS is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_qspi0_hclk (void)
| Enabling force to turn off the clock for QSPI0. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_qspi0_hclk (void)
| Disabling force to turn off the clock for QSPI0. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_qspi0_hclk (void)
| Indicate whether the clock for QSPI0 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_qspi1_hclk (void)
| Enabling force to turn off the clock for QSPI1. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_qspi1_hclk (void)
| Disabling force to turn off the clock for QSPI1. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_qspi1_hclk (void)
| Indicate whether the clock for QSPI1 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_qspi2_hclk (void)
| Enabling force to turn off the clock for QSPI2. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_qspi2_hclk (void)
| Disabling force to turn off the clock for QSPI2. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_qspi2_hclk (void)
| Indicate whether the clock for QSPI2 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_i2s_m_hclk (void)
| Enabling force to turn off the clock for I2S master. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_i2s_m_hclk (void)
| Disabling force to turn off the clock for I2S master. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_i2s_m_hclk (void)
| Indicate whether the clock for I2S master is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_i2s_s_p_hclk (void)
| Enabling force to turn off the clock for I2S slave. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_i2s_s_p_hclk (void)
| Disabling force to turn off the clock for I2S slave. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_i2s_s_p_hclk (void)
| Indicate whether the clock for I2S slave is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_dspi_hclk (void)
| Enabling force to turn off the clock for DSPI slave. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_dspi_hclk (void)
| Disabling force to turn off the clock for DSPI slave. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_dspi_hclk (void)
| Indicate whether the clock for DSPI is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_pdm_hclk (void)
| Enabling force to turn off the clock for PDM slave. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_pdm_hclk (void)
| Disabling force to turn off the clock for PDM slave. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_pdm_hclk (void)
| Indicate whether the clock for PDM is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_secu_div4_pclk (void)
| Enabling force to turn off the div4 clock for security blocks. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_secu_div4_pclk (void)
| Disabling force to turn off the div4 clock for security blocks. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_secu_div4_pclk (void)
| Indicate whether the div4 clock for security blocks is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_xf_xqspi_div4_pclk (void)
| Enabling force to turn off the div4 clock for xf qspi blocks. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_xf_xqspi_div4_pclk (void)
| Disabling force to turn off the div4 clock for xf qspi blocks. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_xf_xqspi_div4_pclk (void)
| Indicate whether the div4 clock for xf qspi blocks is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_pwm0_hclk (void)
| Enabling force to turn off the clock for PWM0. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_pwm0_hclk (void)
| Disabling force to turn off the clock for PWM0. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_pwm0_hclk (void)
| Indicate whether the clock for PWM0 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_pwm1_hclk (void)
| Enabling force to turn off the clock for PWM1. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_pwm1_hclk (void)
| Disabling force to turn off the clock for PWM1. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_pwm1_hclk (void)
| Indicate whether the clock for PWM1 is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_vttbl_hclk (void)
| Enabling force to turn off the clock for VTTBL. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_vttbl_hclk (void)
| Disabling force to turn off the clock for VTTBL. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_vttbl_hclk (void)
| Indicate whether the clock for VTTBL is forced to close. More...
__STATIC_INLINE void | ll_cgc_set_mcu_periph_low_power (uint32_t clk_mask)
| Some peripherals has low power feature. (Include: UART/I2S/SPIM/SPIS/I2C/AHB BUS) More...
__STATIC_INLINE uint32_t | ll_cgc_get_mcu_periph_low_power (void)
| Return to clock blocks that has low power feature. (Include: UART/I2S/SPIM/SPIS/I2C/AHB BUS) More...
__STATIC_INLINE void | ll_cgc_enable_uart_sclk_low_power (void)
| Enable uart sclk low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_uart_sclk_low_power (void)
| Disable uart sclk low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_uart_sclk_low_power (void)
| Indicate whether the uart sclk low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_uart_pclk_low_power (void)
| Enable uart pclk low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_uart_pclk_low_power (void)
| Disable uart pclk low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_uart_pclk_low_power (void)
| Indicate whether the uart pclk low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2s_low_power (void)
| Enable i2s low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_i2s_low_power (void)
| Disable i2s low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2s_low_power (void)
| Indicate whether the i2s low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_spim_sclk_low_power (void)
| Enable spim sclk low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_spim_sclk_low_power (void)
| Disable spim sclk low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_spim_sclk_low_power (void)
| Indicate whether the spim sclk low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_spis_sclk_low_power (void)
| Enable spis sclk low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_spis_sclk_low_power (void)
| Disable spis sclk low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_spis_sclk_low_power (void)
| Indicate whether the spis sclk low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2c_sclk_low_power (void)
| Enable i2c sclk low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_i2c_sclk_low_power (void)
| Disable i2c sclk low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2c_sclk_low_power (void)
| Indicate whether the i2c sclk low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_ahb_bus_low_power (void)
| Enable ahb bus low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_ahb_bus_low_power (void)
| Disable ahb bus low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_ahb_bus_low_power (void)
| Indicate whether the ahb bus low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_qspim_low_power (void)
| Enable QSPIM low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_qspim_low_power (void)
| Disable QSPIM low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_qspim_low_power (void)
| Indicate whether the QSPIM low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_ahb2apb_sync_bus_low_power (void)
| Enable AHB2APB bus low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_ahb2apb_sync_bus_low_power (void)
| Disable AHB2APB bus low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_ahb2apb_sync_bus_low_power (void)
| Indicate whether the AHB2APB bus low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_ahb2apb_async_bus_low_power (void)
| Enable ahb bus low-power feature. More...
__STATIC_INLINE void | ll_cgc_disable_ahb2apb_async_bus_low_power (void)
| Disable ahb bus low-power feature. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_ahb2apb_async_bus_low_power (void)
| Indicate whether the ahb bus low-power is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_uart0_slp_wfi (void)
| Enable turn UART0 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_uart0_slp_wfi (void)
| Disable turn UART0 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_uart0_slp_wfi (void)
| Indicate whether turn UART0 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_uart1_slp_wfi (void)
| Enable turn UART1 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_uart1_slp_wfi (void)
| Disable turn UART1 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_uart1_slp_wfi (void)
| Indicate whether turn UART1 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_uart2_slp_wfi (void)
| Enable turn UART2 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_uart2_slp_wfi (void)
| Disable turn UART2 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_uart2_slp_wfi (void)
| Indicate whether turn UART2 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_uart3_slp_wfi (void)
| Enable turn UART3 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_uart3_slp_wfi (void)
| Disable turn UART3 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_uart3_slp_wfi (void)
| Indicate whether turn UART3 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_uart4_slp_wfi (void)
| Enable turn UART4 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_uart4_slp_wfi (void)
| Disable turn UART4 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_uart4_slp_wfi (void)
| Indicate whether turn UART4 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_uart5_slp_wfi (void)
| Enable turn UART5 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_uart5_slp_wfi (void)
| Disable turn UART5 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_uart5_slp_wfi (void)
| Indicate whether turn UART5 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2c0_slp_wfi (void)
| Enable turn I2C0 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_i2c0_slp_wfi (void)
| Disable turn I2C0 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2c0_slp_wfi (void)
| Indicate whether turn I2C0 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2c1_slp_wfi (void)
| Enable turn I2C1 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_i2c1_slp_wfi (void)
| Disable turn I2C1 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2c1_slp_wfi (void)
| Indicate whether turn I2C1 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2c2_slp_wfi (void)
| Enable turn I2C2 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_i2c2_slp_wfi (void)
| Disable turn I2C2 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2c2_slp_wfi (void)
| Indicate whether turn I2C2 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2c3_slp_wfi (void)
| Enable turn I2C3 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_i2c3_slp_wfi (void)
| Disable turn I2C3 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2c3_slp_wfi (void)
| Indicate whether turn I2C3 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2c4_slp_wfi (void)
| Enable turn I2C4 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_i2c4_slp_wfi (void)
| Disable turn I2C4 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2c4_slp_wfi (void)
| Indicate whether turn I2C4 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2c5_slp_wfi (void)
| Enable turn I2C5 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_i2c5_slp_wfi (void)
| Disable turn I2C5 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2c5_slp_wfi (void)
| Indicate whether turn I2C5 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2s_m_slp_wfi (void)
| Enable turn I2S_M off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_i2s_m_slp_wfi (void)
| Disable turn I2S_M off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2s_m_slp_wfi (void)
| Indicate whether turn I2S_M off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_i2s_s_slp_wfi (void)
| Enable turn I2S_S off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_i2s_s_slp_wfi (void)
| Disable turn I2S_S off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_i2s_s_slp_wfi (void)
| Indicate whether turn I2S_S off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_spi_m_slp_wfi (void)
| Enable turn SPI_M off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_spi_m_slp_wfi (void)
| Disable turn SPI_M off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_spi_m_slp_wfi (void)
| Indicate whether turn SPI_M off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_spi_s_slp_wfi (void)
| Enable turn SPI_S off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_spi_s_slp_wfi (void)
| Disable turn SPI_S off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_spi_s_slp_wfi (void)
| Indicate whether turn SPI_S off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_pwm0_slp_wfi (void)
| Enable turn pwm0 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_pwm0_slp_wfi (void)
| Disable turn pwm0 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_pwm0_slp_wfi (void)
| Indicate whether turn pwm0 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_pwm1_slp_wfi (void)
| Enable turn pwm1 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_pwm1_slp_wfi (void)
| Disable turn pwm1 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_pwm1_slp_wfi (void)
| Indicate whether turn pwm1 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_qspim0_slp_wfi (void)
| Enable turn QSPIM0 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_qspim0_slp_wfi (void)
| Disable turn QSPIM0 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_qspim0_slp_wfi (void)
| Indicate whether turn QSPIM0 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_qspim1_slp_wfi (void)
| Enable turn QSPIM1 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_qspim1_slp_wfi (void)
| Disable turn QSPIM1 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_qspim1_slp_wfi (void)
| Indicate whether turn QSPIM1 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_qspim2_slp_wfi (void)
| Enable turn QSPIM2 off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_qspim2_slp_wfi (void)
| Disable turn QSPIM2 off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_qspim2_slp_wfi (void)
| Indicate whether turn QSPIM2 off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_dspi_slp_wfi (void)
| Enable turn DSPI off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_dspi_slp_wfi (void)
| Disable turn DSPI off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_dspi_slp_wfi (void)
| Indicate whether turn DSPI off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_pdm_slp_wfi (void)
| Enable turn PDM off during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_pdm_slp_wfi (void)
| Disable turn PDM off during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_pdm_slp_wfi (void)
| Indicate whether turn PDM off during WFI/WFE is enabled. More...
__STATIC_INLINE void | ll_cgc_set_force_off_hclk_secu (uint32_t clk_mask)
| Individual block's clock control inside security system which was forced to turn off (Include: AES/HMAC/PKC/PRESENT/RAMKAY/RNG/EFUSE) More...
__STATIC_INLINE uint32_t | ll_cgc_get_force_off_secu (void)
| Return to clock blocks that was forcibly closed inside security system.(Include: AES/HMAC/PKC/PRESENT/RAMKAY/RNG/EFUSE) More...
__STATIC_INLINE void | ll_cgc_set_slp_off_hclk_secu (uint32_t clk_mask)
| Some security blocks automatic turn off clock during WFI/WFE. (Include: AES/HMAC/PKC/PRESENT/RAMKAY/RNG/EFUSE) More...
__STATIC_INLINE uint32_t | ll_cgc_get_slp_off_secu (void)
| Return to security clock blocks that is turned off during WFI/WFE.(Include: AES/HMAC/PKC/PRESENT/RAMKAY/RNG/EFUSE) More...
__STATIC_INLINE void | ll_cgc_enable_force_off_aes_hclk (void)
| Enabling force to turn off the clock for AES. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_aes_hclk (void)
| Disabling force to turn off the clock for AES. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_aes_hclk (void)
| Indicate whether the clock for AES is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_hmac_hclk (void)
| Enabling force to turn off the clock for HMAC. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_hmac_hclk (void)
| Disabling force to turn off the clock for HMAC. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_hmac_hclk (void)
| Indicate whether the clock for HMAC is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_pkc_hclk (void)
| Enabling force to turn off the clock for PKC. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_pkc_hclk (void)
| Disabling force to turn off the clock for PKC. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_pkc_hclk (void)
| Indicate whether the clock for PKC is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_present_hclk (void)
| Enabling force to turn off the clock for PRESENT. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_present_hclk (void)
| Disabling force to turn off the clock for PRESENT. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_present_hclk (void)
| Indicate whether the clock for PRESENT is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_ramkey_hclk (void)
| Enabling force to turn off the clock for RAMKEY. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_ramkey_hclk (void)
| Disabling force to turn off the clock for RAMKEY. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_ramkey_hclk (void)
| Indicate whether the clock for RAMKEY is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_rng_hclk (void)
| Enabling force to turn off the clock for RNG. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_rng_hclk (void)
| Disabling force to turn off the clock for RNG. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_rng_hclk (void)
| Indicate whether the clock for RNG is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_efuse_hclk (void)
| Enabling force to turn off the clock for EFUSE. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_efuse_hclk (void)
| Disabling force to turn off the clock for EFUSE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_efuse_hclk (void)
| Indicate whether the clock for EFUSE is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_aes_hclk (void)
| Enable AES automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_aes_hclk (void)
| Disable AES automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_aes_hclk (void)
| Indicate whether the AES automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_hmac_hclk (void)
| Enable HMAC automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_hmac_hclk (void)
| Disable HMAC automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_hmac_hclk (void)
| Indicate whether the HMAC automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_pkc_hclk (void)
| Enable PKC automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_pkc_hclk (void)
| Disable PKC automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_pkc_hclk (void)
| Indicate whether the PKC automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_present_hclk (void)
| Enable PRESENT automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_present_hclk (void)
| Disable PRESENT automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_present_hclk (void)
| Indicate whether the PRESENT automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_ramkey_hclk (void)
| Enable RAMKEY automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_ramkey_hclk (void)
| Disable RAMKEY automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_ramkey_hclk (void)
| Indicate whether the RAMKEY automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_rng_hclk (void)
| Enable RNG automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_rng_hclk (void)
| Disable RNG automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_rng_hclk (void)
| Indicate whether the RNG automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_efuse_hclk (void)
| Enable EFUSE automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_efuse_hclk (void)
| Disable EFUSE automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_efuse_hclk (void)
| Indicate whether the EFUSE automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_set_misc_clk (uint32_t clk_mask)
| Some MISC_CLK blocks turn off clock. (Include: GPADC/XQSPI/DMA0) More...
__STATIC_INLINE uint32_t | ll_cgc_get_misc_clk (void)
| Return to MISC_CLK clock blocks that is turned off.(Include: GPADC/XQSPI/DMA0) More...
__STATIC_INLINE void | ll_cgc_enable_force_off_gpadc_hclk (void)
| Enabling force to turn off the clock for GPADC. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_gpadc_hclk (void)
| Disabling force to turn off the clock for GPADC. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_gpadc_hclk (void)
| Indicate whether the clock for GPADC is forced to close. More...
__STATIC_INLINE void | ll_cgc_enable_wfi_off_gpadc_hclk (void)
| Enable GPADC automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE void | ll_cgc_disable_wfi_off_gpadc_hclk (void)
| Disable GPADC automatic turn off clock during WFI/WFE. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_wfi_off_gpadc_hclk (void)
| Indicate whether the GPADC automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_xqspi_sck (void)
| Enable XQSPI SCK CLK turn off. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_xqspi_sck (void)
| Disable XQSPI SCK CLK turn off. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_xqspi_sck (void)
| Indicate whether the XQSPI SCK CLK automatic turn off clock is enabled. More...
__STATIC_INLINE void | ll_cgc_enable_force_off_dma0_hclk (void)
| Enable DMA0 turn off. More...
__STATIC_INLINE void | ll_cgc_disable_force_off_dma0_hclk (void)
| Disable DMA0 turn off. More...
__STATIC_INLINE uint32_t | ll_cgc_is_enabled_force_off_dma0_hclk (void)
| Indicate whether the DMA0 automatic turn off clock is enabled. More...

## Detailed Description

## Function Documentation

## ◆ ll_cgc_disable_ahb2apb_async_bus_low_power()

__STATIC_INLINE void ll_cgc_disable_ahb2apb_async_bus_low_power | ( | void |  | ) |

Disable ahb bus low-power feature.

Register | BitsName ---------|-------- CG_LP_EN | AHB_BUS_LP

Return values

  None |

Definition at line 3296 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_ahb2apb_sync_bus_low_power()

__STATIC_INLINE void ll_cgc_disable_ahb2apb_sync_bus_low_power | ( | void |  | ) |

Disable AHB2APB bus low-power feature.

Register | BitsName ---------|-------- CG_LP_EN | AHB2APB_BUS_LP

Return values

  None |

Definition at line 3254 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_ahb_bus_low_power()

__STATIC_INLINE void ll_cgc_disable_ahb_bus_low_power | ( | void |  | ) |

Disable ahb bus low-power feature.

Register | BitsName ---------|-------- CG_LP_EN | AHB_BUS_LP

Return values

  None |

Definition at line 3172 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_dspi_slp_wfi()

__STATIC_INLINE void ll_cgc_disable_dspi_slp_wfi | ( | void |  | ) |

Disable turn DSPI off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | DSPI_SLP

Return values

  None |

Definition at line 4193 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_force_off_aes_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_aes_hclk | ( | void |  | ) |

Disabling force to turn off the clock for AES.

Register | BitsName ----------|-------- SECU_CLK_CTRL | AES_HCLK_FRC_OFF

Return values

  None |

Definition at line 4361 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_force_off_aon_mcusub_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_aon_mcusub_hclk | ( | void |  | ) |

Disabling force to turn off the clock for AON_MUCSUB.

Register | BitsName ----------|-------- CG_CTRL_2 | AON_MCUSUB_HCLK

Return values

  None |

Definition at line 1684 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_force_off_apb_sub_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_apb_sub_hclk | ( | void |  | ) |

Disabling force to turn off the clock for APB Subsystem.

Register | BitsName ----------|-------- CG_CTRL_1 | APB_SUB_HCLK

Return values

  None |

Definition at line 1601 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_force_off_ble_brg_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_ble_brg_hclk | ( | void |  | ) |

Disabling force to turn off the clock for BLE Bridge.

Register | BitsName ----------|-------- CG_CTRL_1 | BLE_BRG_HCLK

Return values

  None |

Definition at line 1559 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_force_off_dma0_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_dma0_hclk | ( | void |  | ) |

Disable DMA0 turn off.

Register | BitsName ----------|-------- MCU_MISC_CLK | DMA0_OFF

Return values

  None |

Definition at line 5079 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_force_off_dspi_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_dspi_hclk | ( | void |  | ) |

Disabling force to turn off the clock for DSPI slave.

Register | BitsName ----------|-------- PERIPH_GC | DSPI_PCLK

Return values

  None |

Definition at line 2581 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_force_off_efuse_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_efuse_hclk | ( | void |  | ) |

Disabling force to turn off the clock for EFUSE.

Register | BitsName ----------|-------- SECU_CLK_CTRL | EFUSE_HCLK_FRC_OFF

Return values

  None |

Definition at line 4605 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_force_off_gpadc_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_gpadc_hclk | ( | void |  | ) |

Disabling force to turn off the clock for GPADC.

Register | BitsName ----------|-------- MCU_MISC_CLK | GPADC_HCLK_FRC_OFF

Return values

  None |

Definition at line 4956 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_force_off_gpio_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_gpio_hclk | ( | void |  | ) |

Disabling force to turn off the clock for GPIO.

Register | BitsName ----------|-------- CG_CTRL_1 | GPIO_HCLK

Return values

  None |

Definition at line 1517 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_force_off_hmac_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_hmac_hclk | ( | void |  | ) |

Disabling force to turn off the clock for HMAC.

Register | BitsName ----------|-------- SECU_CLK_CTRL | HMAC_HCLK_FRC_OFF

Return values

  None |

Definition at line 4401 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_force_off_htb_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_htb_hclk | ( | void |  | ) |

Disabling force to turn off the clock for Hopping Table.

Register | BitsName ----------|-------- CG_CTRL_1 | HTB_HCLK

Return values

  None |

Definition at line 1391 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_force_off_i2c0_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_i2c0_hclk | ( | void |  | ) |

Disabling force to turn off the clock for I2C0.

Register | BitsName ----------|-------- PERIPH_GC | I2C0_HCLK

Return values

  None |

Definition at line 2053 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_force_off_i2c1_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_i2c1_hclk | ( | void |  | ) |

Disabling force to turn off the clock for I2C1.

Register | BitsName ----------|-------- PERIPH_GC | I2C1_HCLK

Return values

  None |

Definition at line 2095 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_force_off_i2c2_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_i2c2_hclk | ( | void |  | ) |

Disabling force to turn off the clock for I2C2.

Register | BitsName ----------|-------- PERIPH_GC | I2C2_HCLK

Return values

  None |

Definition at line 2136 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_force_off_i2c3_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_i2c3_hclk | ( | void |  | ) |

Disabling force to turn off the clock for I2C3.

Register | BitsName ----------|-------- PERIPH_GC | I2C3_HCLK

Return values

  None |

Definition at line 2176 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_force_off_i2c4_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_i2c4_hclk | ( | void |  | ) |

Disabling force to turn off the clock for I2C4.

Register | BitsName ----------|-------- PERIPH_GC | I2C4_HCLK

Return values

  None |

Definition at line 2216 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_force_off_i2c5_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_i2c5_hclk | ( | void |  | ) |

Disabling force to turn off the clock for I2C5.

Register | BitsName ----------|-------- PERIPH_GC | I2C5_HCLK

Return values

  None |

Definition at line 2256 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_force_off_i2s_m_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_i2s_m_hclk | ( | void |  | ) |

Disabling force to turn off the clock for I2S master.

Register | BitsName ----------|-------- PERIPH_GC | I2S_HCLK

Return values

  None |

Definition at line 2501 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_force_off_i2s_s_p_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_i2s_s_p_hclk | ( | void |  | ) |

Disabling force to turn off the clock for I2S slave.

Register | BitsName ----------|-------- PERIPH_GC | I2S_S_PCLK

Return values

  None |

Definition at line 2541 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_force_off_pdm_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_pdm_hclk | ( | void |  | ) |

Disabling force to turn off the clock for PDM slave.

Register | BitsName ----------|-------- PERIPH_GC | PDM_PCLK

Return values

  None |

Definition at line 2621 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_force_off_pkc_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_pkc_hclk | ( | void |  | ) |

Disabling force to turn off the clock for PKC.

Register | BitsName ----------|-------- SECU_CLK_CTRL | PKC_HCLK_FRC_OFF

Return values

  None |

Definition at line 4441 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_force_off_present_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_present_hclk | ( | void |  | ) |

Disabling force to turn off the clock for PRESENT.

Register | BitsName ----------|-------- SECU_CLK_CTRL | PRESENT_HCLK_FRC_OFF

Return values

  None |

Definition at line 4481 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_force_off_pwm0_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_pwm0_hclk | ( | void |  | ) |

Disabling force to turn off the clock for PWM0.

Register | BitsName ----------|-------- PERIPH_GC | PWM0_PCLK

Return values

  None |

Definition at line 2741 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_force_off_pwm1_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_pwm1_hclk | ( | void |  | ) |

Disabling force to turn off the clock for PWM1.

Register | BitsName ----------|-------- PERIPH_GC | PWM1_PCLK

Return values

  None |

Definition at line 2783 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_force_off_qspi0_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_qspi0_hclk | ( | void |  | ) |

Disabling force to turn off the clock for QSPI0.

Register | BitsName ----------|-------- PERIPH_GC | QSPI0_HCLK

Return values

  None |

Definition at line 2380 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_force_off_qspi1_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_qspi1_hclk | ( | void |  | ) |

Disabling force to turn off the clock for QSPI1.

Register | BitsName ----------|-------- PERIPH_GC | QSPI1_HCLK

Return values

  None |

Definition at line 2420 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_force_off_qspi2_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_qspi2_hclk | ( | void |  | ) |

Disabling force to turn off the clock for QSPI2.

Register | BitsName ----------|-------- PERIPH_GC | QSPI2_HCLK

Return values

  None |

Definition at line 2460 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_force_off_ramkey_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_ramkey_hclk | ( | void |  | ) |

Disabling force to turn off the clock for RAMKEY.

Register | BitsName ----------|-------- SECU_CLK_CTRL | RAMKEY_HCLK_FRC_OFF

Return values

  None |

Definition at line 4521 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_force_off_rng_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_rng_hclk | ( | void |  | ) |

Disabling force to turn off the clock for RNG.

Register | BitsName ----------|-------- SECU_CLK_CTRL | RNG_HCLK_FRC_OFF

Return values

  None |

Definition at line 4563 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_force_off_rom_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_rom_hclk | ( | void |  | ) |

Disabling force to turn off the clock for ROM.

Register | BitsName ----------|-------- CG_CTRL_1 | ROM_HCLK

Return values

  None |

Definition at line 1433 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_force_off_secu_div4_pclk()

__STATIC_INLINE void ll_cgc_disable_force_off_secu_div4_pclk | ( | void |  | ) |

Disabling force to turn off the div4 clock for security blocks.

Register | BitsName ----------|-------- PERIPH_GC | I2S_HCLK

Return values

  None |

Definition at line 2661 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_force_off_secu_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_secu_hclk | ( | void |  | ) |

Disabling force to turn off the clock for security blocks(including AES, PKC, Present, HMAC).

Register | BitsName ----------|-------- CG_CTRL_1 | SECU_HCLK

Return values

  None |

Definition at line 1349 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_force_off_serial_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_serial_hclk | ( | void |  | ) |

Disabling force to turn off the clock for serial blocks(including I2C, UART, QSPI, I2S, SPI).

Register | BitsName ----------|-------- CG_CTRL_1 | SERIAL_HCLK

Return values

  None |

Definition at line 1643 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_force_off_snsadc_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_snsadc_hclk | ( | void |  | ) |

Disabling force to turn off the clock for SNSADC.

Register | BitsName ----------|-------- CG_CTRL_1 | SNSADC_HCLK

Return values

  None |

Definition at line 1475 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_force_off_spim_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_spim_hclk | ( | void |  | ) |

Disabling force to turn off the clock for SPIM.

Register | BitsName ----------|-------- PERIPH_GC | SPIM_HCLK

Return values

  None |

Definition at line 2297 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_force_off_spis_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_spis_hclk | ( | void |  | ) |

Disabling force to turn off the clock for SPIS.

Register | BitsName ----------|-------- PERIPH_GC | SPIS_HCLK

Return values

  None |

Definition at line 2339 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_force_off_sram_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_sram_hclk | ( | void |  | ) |

Disabling force to turn off the clock for SRAM.

Register | BitsName ----------|-------- CG_CTRL_2 | SRAM_HCLK

Return values

  None |

Definition at line 1767 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_force_off_uart0_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_uart0_hclk | ( | void |  | ) |

Disabling force to turn off the clock for UART0.

Register | BitsName ----------|-------- PERIPH_GC | UART0_HCLK

Return values

  None |

Definition at line 1809 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_force_off_uart1_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_uart1_hclk | ( | void |  | ) |

Disabling force to turn off the clock for UART1.

Register | BitsName ----------|-------- PERIPH_GC | UART1_HCLK

Return values

  None |

Definition at line 1851 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_force_off_uart2_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_uart2_hclk | ( | void |  | ) |

Disabling force to turn off the clock for UART2.

Register | BitsName ----------|-------- PERIPH_GC | UART2_HCLK

Return values

  None |

Definition at line 1892 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_force_off_uart3_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_uart3_hclk | ( | void |  | ) |

Disabling force to turn off the clock for UART3.

Register | BitsName ----------|-------- PERIPH_GC | UART3_HCLK

Return values

  None |

Definition at line 1932 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_force_off_uart4_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_uart4_hclk | ( | void |  | ) |

Disabling force to turn off the clock for UART4.

Register | BitsName ----------|-------- PERIPH_GC | UART4_HCLK

Return values

  None |

Definition at line 1972 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_force_off_uart5_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_uart5_hclk | ( | void |  | ) |

Disabling force to turn off the clock for UART5.

Register | BitsName ----------|-------- PERIPH_GC | UART5_HCLK

Return values

  None |

Definition at line 2012 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_force_off_vttbl_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_vttbl_hclk | ( | void |  | ) |

Disabling force to turn off the clock for VTTBL.

Register | BitsName ----------|-------- PERIPH_GC | VTTBL_PCLK

Return values

  None |

Definition at line 2824 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_force_off_xf_xqspi_div4_pclk()

__STATIC_INLINE void ll_cgc_disable_force_off_xf_xqspi_div4_pclk | ( | void |  | ) |

Disabling force to turn off the div4 clock for xf qspi blocks.

Register | BitsName ----------|-------- PERIPH_GC | XQSPI_HCLK

Return values

  None |

Definition at line 2700 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_force_off_xqspi_hclk()

__STATIC_INLINE void ll_cgc_disable_force_off_xqspi_hclk | ( | void |  | ) |

Disabling force to turn off the clock for XQSPI.

Register | BitsName ----------|-------- CG_CTRL_2 | XF_XQSPI_HCLK

Return values

  None |

Definition at line 1725 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_force_off_xqspi_sck()

__STATIC_INLINE void ll_cgc_disable_force_off_xqspi_sck | ( | void |  | ) |

Disable XQSPI SCK CLK turn off.

Register | BitsName ----------|-------- MCU_MISC_CLK | XQSPI SCK CLK_OFF

Return values

  None |

Definition at line 5037 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_i2c0_slp_wfi()

__STATIC_INLINE void ll_cgc_disable_i2c0_slp_wfi | ( | void |  | ) |

Disable turn I2C0 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | I2C0_SLP

Return values

  None |

Definition at line 3582 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_i2c1_slp_wfi()

__STATIC_INLINE void ll_cgc_disable_i2c1_slp_wfi | ( | void |  | ) |

Disable turn I2C1 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | I2C1_SLP

Return values

  None |

Definition at line 3624 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_i2c2_slp_wfi()

__STATIC_INLINE void ll_cgc_disable_i2c2_slp_wfi | ( | void |  | ) |

Disable turn I2C2 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | I2C2_SLP

Return values

  None |

Definition at line 3665 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_i2c3_slp_wfi()

__STATIC_INLINE void ll_cgc_disable_i2c3_slp_wfi | ( | void |  | ) |

Disable turn I2C3 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | I2C3_SLP

Return values

  None |

Definition at line 3705 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_i2c4_slp_wfi()

__STATIC_INLINE void ll_cgc_disable_i2c4_slp_wfi | ( | void |  | ) |

Disable turn I2C4 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | I2C4_SLP

Return values

  None |

Definition at line 3745 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_i2c5_slp_wfi()

__STATIC_INLINE void ll_cgc_disable_i2c5_slp_wfi | ( | void |  | ) |

Disable turn I2C5 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | I2C5_SLP

Return values

  None |

Definition at line 3785 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_i2c_sclk_low_power()

__STATIC_INLINE void ll_cgc_disable_i2c_sclk_low_power | ( | void |  | ) |

Disable i2c sclk low-power feature.

Register | BitsName ---------|-------- CG_LP_EN | I2C_LP_SCLK

Return values

  None |

Definition at line 3130 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_i2s_low_power()

__STATIC_INLINE void ll_cgc_disable_i2s_low_power | ( | void |  | ) |

Disable i2s low-power feature.

Register | BitsName ---------|-------- CG_LP_EN | I2S_LP

Return values

  None |

Definition at line 3005 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_i2s_m_slp_wfi()

__STATIC_INLINE void ll_cgc_disable_i2s_m_slp_wfi | ( | void |  | ) |

Disable turn I2S_M off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | I2SM_SLP

Return values

  None |

Definition at line 3825 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_i2s_s_slp_wfi()

__STATIC_INLINE void ll_cgc_disable_i2s_s_slp_wfi | ( | void |  | ) |

Disable turn I2S_S off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | I2SS_SLP

Return values

  None |

Definition at line 3865 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_pdm_slp_wfi()

__STATIC_INLINE void ll_cgc_disable_pdm_slp_wfi | ( | void |  | ) |

Disable turn PDM off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | PDM_SLP

Return values

  None |

Definition at line 4233 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_pwm0_slp_wfi()

__STATIC_INLINE void ll_cgc_disable_pwm0_slp_wfi | ( | void |  | ) |

Disable turn pwm0 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | PWM0_SLP

Return values

  None |

Definition at line 3990 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_pwm1_slp_wfi()

__STATIC_INLINE void ll_cgc_disable_pwm1_slp_wfi | ( | void |  | ) |

Disable turn pwm1 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | PWM1_SLP

Return values

  None |

Definition at line 4032 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_qspim0_slp_wfi()

__STATIC_INLINE void ll_cgc_disable_qspim0_slp_wfi | ( | void |  | ) |

Disable turn QSPIM0 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | QSPIM0_SLP

Return values

  None |

Definition at line 4073 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_qspim1_slp_wfi()

__STATIC_INLINE void ll_cgc_disable_qspim1_slp_wfi | ( | void |  | ) |

Disable turn QSPIM1 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | QSPIM1_SLP

Return values

  None |

Definition at line 4113 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_qspim2_slp_wfi()

__STATIC_INLINE void ll_cgc_disable_qspim2_slp_wfi | ( | void |  | ) |

Disable turn QSPIM2 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | QSPIM2_SLP

Return values

  None |

Definition at line 4153 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_qspim_low_power()

__STATIC_INLINE void ll_cgc_disable_qspim_low_power | ( | void |  | ) |

Disable QSPIM low-power feature.

Register | BitsName ---------|-------- CG_LP_EN | QSPIM_LP

Return values

  None |

Definition at line 3213 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_spi_m_slp_wfi()

__STATIC_INLINE void ll_cgc_disable_spi_m_slp_wfi | ( | void |  | ) |

Disable turn SPI_M off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | SPIM_SLP

Return values

  None |

Definition at line 3906 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_spi_s_slp_wfi()

__STATIC_INLINE void ll_cgc_disable_spi_s_slp_wfi | ( | void |  | ) |

Disable turn SPI_S off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | SPIS_SLP

Return values

  None |

Definition at line 3948 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_spim_sclk_low_power()

__STATIC_INLINE void ll_cgc_disable_spim_sclk_low_power | ( | void |  | ) |

Disable spim sclk low-power feature.

Register | BitsName ---------|-------- CG_LP_EN | SPIM_LP_SCLK

Return values

  None |

Definition at line 3046 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_spis_sclk_low_power()

__STATIC_INLINE void ll_cgc_disable_spis_sclk_low_power | ( | void |  | ) |

Disable spis sclk low-power feature.

Register | BitsName ---------|-------- CG_LP_EN | SPIS_LP_SCLK

Return values

  None |

Definition at line 3088 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_uart0_slp_wfi()

__STATIC_INLINE void ll_cgc_disable_uart0_slp_wfi | ( | void |  | ) |

Disable turn UART0 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | UART0_SLP

Return values

  None |

Definition at line 3338 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_uart1_slp_wfi()

__STATIC_INLINE void ll_cgc_disable_uart1_slp_wfi | ( | void |  | ) |

Disable turn UART1 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | UART1_SLP

Return values

  None |

Definition at line 3380 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_uart2_slp_wfi()

__STATIC_INLINE void ll_cgc_disable_uart2_slp_wfi | ( | void |  | ) |

Disable turn UART2 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | UART2_SLP

Return values

  None |

Definition at line 3421 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_uart3_slp_wfi()

__STATIC_INLINE void ll_cgc_disable_uart3_slp_wfi | ( | void |  | ) |

Disable turn UART3 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | UART3_SLP

Return values

  None |

Definition at line 3461 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_uart4_slp_wfi()

__STATIC_INLINE void ll_cgc_disable_uart4_slp_wfi | ( | void |  | ) |

Disable turn UART4 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | UART4_SLP

Return values

  None |

Definition at line 3501 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_uart5_slp_wfi()

__STATIC_INLINE void ll_cgc_disable_uart5_slp_wfi | ( | void |  | ) |

Disable turn UART5 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | UART5_SLP

Return values

  None |

Definition at line 3541 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_uart_pclk_low_power()

__STATIC_INLINE void ll_cgc_disable_uart_pclk_low_power | ( | void |  | ) |

Disable uart pclk low-power feature.

Register | BitsName ---------|-------- CG_LP_EN | UART_LP_PCLK

Return values

  None |

Definition at line 2964 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_uart_sclk_low_power()

__STATIC_INLINE void ll_cgc_disable_uart_sclk_low_power | ( | void |  | ) |

Disable uart sclk low-power feature.

Register | BitsName ---------|-------- CG_LP_EN | UART_LP_SCLK

Return values

  None |

Definition at line 2922 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_wfi_off_aes_hclk()

__STATIC_INLINE void ll_cgc_disable_wfi_off_aes_hclk | ( | void |  | ) |

Disable AES automatic turn off clock during WFI/WFE.

Register | BitsName ----------|-------- SECU_CLK_CTRL | AES_HCLK_SLP_OFF

Return values

  None |

Definition at line 4646 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_wfi_off_aon_mcusub_hclk()

__STATIC_INLINE void ll_cgc_disable_wfi_off_aon_mcusub_hclk | ( | void |  | ) |

Disable AON_MUCSUB automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_2 | AON_MCUSUB_HCLK

Return values

  None |

Definition at line 1142 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_wfi_off_apb_sub_hclk()

__STATIC_INLINE void ll_cgc_disable_wfi_off_apb_sub_hclk | ( | void |  | ) |

Disable APB Subsystem automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_0 | APB_SUB_HCLK

Return values

  None |

Definition at line 1057 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_wfi_off_ble_brg_hclk()

__STATIC_INLINE void ll_cgc_disable_wfi_off_ble_brg_hclk | ( | void |  | ) |

Disable BLE Bridge automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_0 | BLE_BRG_HCLK

Return values

  None |

Definition at line 1015 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_wfi_off_dma_hclk()

__STATIC_INLINE void ll_cgc_disable_wfi_off_dma_hclk | ( | void |  | ) |

Disable DMA automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_0 | DMA_HCLK

Return values

  None |

Definition at line 974 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_wfi_off_efuse_hclk()

__STATIC_INLINE void ll_cgc_disable_wfi_off_efuse_hclk | ( | void |  | ) |

Disable EFUSE automatic turn off clock during WFI/WFE.

Register | BitsName ----------|-------- SECU_CLK_CTRL | EFUSE_HCLK_SLP_OFF

Return values

  None |

Definition at line 4889 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_wfi_off_gpadc_hclk()

__STATIC_INLINE void ll_cgc_disable_wfi_off_gpadc_hclk | ( | void |  | ) |

Disable GPADC automatic turn off clock during WFI/WFE.

Register | BitsName ----------|-------- MCU_MISC_CLK | GPADC_HCLK_SLP_OFF

Return values

  None |

Definition at line 4996 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_wfi_off_gpio_hclk()

__STATIC_INLINE void ll_cgc_disable_wfi_off_gpio_hclk | ( | void |  | ) |

Disable GPIO automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_0 | GPIO_HCLK

Return values

  None |

Definition at line 933 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_wfi_off_hmac_hclk()

__STATIC_INLINE void ll_cgc_disable_wfi_off_hmac_hclk | ( | void |  | ) |

Disable HMAC automatic turn off clock during WFI/WFE.

Register | BitsName ----------|-------- SECU_CLK_CTRL | HMAC_HCLK_SLP_OFF

Return values

  None |

Definition at line 4686 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_wfi_off_htb_hclk()

__STATIC_INLINE void ll_cgc_disable_wfi_off_htb_hclk | ( | void |  | ) |

Disable Hopping Table automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_0 | HTB_HCLK

Return values

  None |

Definition at line 767 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_wfi_off_pkc_hclk()

__STATIC_INLINE void ll_cgc_disable_wfi_off_pkc_hclk | ( | void |  | ) |

Disable PKC automatic turn off clock during WFI/WFE.

Register | BitsName ----------|-------- SECU_CLK_CTRL | PKC_HCLK_SLP_OFF

Return values

  None |

Definition at line 4726 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_wfi_off_present_hclk()

__STATIC_INLINE void ll_cgc_disable_wfi_off_present_hclk | ( | void |  | ) |

Disable PRESENT automatic turn off clock during WFI/WFE.

Register | BitsName ----------|-------- SECU_CLK_CTRL | PRESENT_HCLK_SLP_OFF

Return values

  None |

Definition at line 4766 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_wfi_off_pwm_hclk()

__STATIC_INLINE void ll_cgc_disable_wfi_off_pwm_hclk | ( | void |  | ) |

Disable PWM automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_0 | PWM_HCLK

Return values

  None |

Definition at line 808 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_wfi_off_ramkey_hclk()

__STATIC_INLINE void ll_cgc_disable_wfi_off_ramkey_hclk | ( | void |  | ) |

Disable RAMKEY automatic turn off clock during WFI/WFE.

Register | BitsName ----------|-------- SECU_CLK_CTRL | RAMKEY_HCLK_SLP_OFF

Return values

  None |

Definition at line 4806 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_wfi_off_rng_hclk()

__STATIC_INLINE void ll_cgc_disable_wfi_off_rng_hclk | ( | void |  | ) |

Disable RNG automatic turn off clock during WFI/WFE.

Register | BitsName ----------|-------- SECU_CLK_CTRL | RNG_HCLK_SLP_OFF

Return values

  None |

Definition at line 4847 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_wfi_off_rom_hclk()

__STATIC_INLINE void ll_cgc_disable_wfi_off_rom_hclk | ( | void |  | ) |

Disable ROM automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_0 | ROM_HCLK

Return values

  None |

Definition at line 849 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_wfi_off_secu_div4_hclk()

__STATIC_INLINE void ll_cgc_disable_wfi_off_secu_div4_hclk | ( | void |  | ) |

Disable security blocks automatic turn off div4 clock during WFI.

Register | BitsName ----------|-------- PERIPH_GC | SECU_DIV4_PCLK

Return values

  None |

Definition at line 1267 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_wfi_off_secu_hclk()

__STATIC_INLINE void ll_cgc_disable_wfi_off_secu_hclk | ( | void |  | ) |

Disable security blocks(including AES, PKC, Present, HMAC) automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_0 | SECU_HCLK

Return values

  None |

Definition at line 685 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_wfi_off_serial_hclk()

__STATIC_INLINE void ll_cgc_disable_wfi_off_serial_hclk | ( | void |  | ) |

Disable serial blocks(including I2C, UART, QSPI, I2S, SPI) automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_0 | SERIAL_HCLK

Return values

  None |

Definition at line 1099 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_wfi_off_sim_hclk()

__STATIC_INLINE void ll_cgc_disable_wfi_off_sim_hclk | ( | void |  | ) |

Disable SIM automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_0 | SIM_HCLK

Return values

  None |

Definition at line 726 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_wfi_off_snsadc_hclk()

__STATIC_INLINE void ll_cgc_disable_wfi_off_snsadc_hclk | ( | void |  | ) |

Disable SNSADC automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_0 | SNSADC_HCLK

Return values

  None |

Definition at line 891 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_wfi_off_sram_hclk()

__STATIC_INLINE void ll_cgc_disable_wfi_off_sram_hclk | ( | void |  | ) |

Disable SRAM automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_2 | SRAM_HCLK

Return values

  None |

Definition at line 1226 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_disable_wfi_off_xqspi_div4_hclk()

__STATIC_INLINE void ll_cgc_disable_wfi_off_xqspi_div4_hclk | ( | void |  | ) |

Disable XQSPI automatic turn off div4 clock during WFI.

Register | BitsName ----------|-------- PERIPH_GC | XQSPI_DIV4_PCLK

Return values

  None |

Definition at line 1308 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_disable_wfi_off_xqspi_hclk()

__STATIC_INLINE void ll_cgc_disable_wfi_off_xqspi_hclk | ( | void |  | ) |

Disable XQSPI automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_2 | XF_XQSPI_HCLK

Return values

  None |

Definition at line 1184 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_DISABLE.

## ◆ ll_cgc_enable_ahb2apb_async_bus_low_power()

__STATIC_INLINE void ll_cgc_enable_ahb2apb_async_bus_low_power | ( | void |  | ) |

Enable ahb bus low-power feature.

Register | BitsName ---------|-------- CG_LP_EN | AHB_BUS_LP

Return values

  None |

Definition at line 3282 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_ahb2apb_sync_bus_low_power()

__STATIC_INLINE void ll_cgc_enable_ahb2apb_sync_bus_low_power | ( | void |  | ) |

Enable AHB2APB bus low-power feature.

Register | BitsName ---------|-------- CG_LP_EN | AHB2APB_BUS_LP

Return values

  None |

Definition at line 3240 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_ahb_bus_low_power()

__STATIC_INLINE void ll_cgc_enable_ahb_bus_low_power | ( | void |  | ) |

Enable ahb bus low-power feature.

Register | BitsName ---------|-------- CG_LP_EN | AHB_BUS_LP

Return values

  None |

Definition at line 3158 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_dspi_slp_wfi()

__STATIC_INLINE void ll_cgc_enable_dspi_slp_wfi | ( | void |  | ) |

Enable turn DSPI off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | DSPI_SLP

Return values

  None |

Definition at line 4180 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_force_off_aes_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_aes_hclk | ( | void |  | ) |

Enabling force to turn off the clock for AES.

Register | BitsName ----------|-------- SECU_CLK_CTRL | AES_HCLK_FRC_OFF

Return values

  None |

Definition at line 4348 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_force_off_aon_mcusub_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_aon_mcusub_hclk | ( | void |  | ) |

Enabling force to turn off the clock for AON_MUCSUB.

Register | BitsName ----------|-------- CG_CTRL_2 | AON_MCUSUB_HCLK

Return values

  None |

Definition at line 1671 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_force_off_apb_sub_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_apb_sub_hclk | ( | void |  | ) |

Enabling force to turn off the clock for APB Subsystem.

Register | BitsName ----------|-------- CG_CTRL_1 | APB_SUB_HCLK

Return values

  None |

Definition at line 1587 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_force_off_ble_brg_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_ble_brg_hclk | ( | void |  | ) |

Enabling force to turn off the clock for BLE Bridge.

Register | BitsName ----------|-------- CG_CTRL_1 | BLE_BRG_HCLK

Return values

  None |

Definition at line 1545 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_force_off_dma0_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_dma0_hclk | ( | void |  | ) |

Enable DMA0 turn off.

Register | BitsName ----------|-------- MCU_MISC_CLK |DMA0_OFF

Return values

  None |

Definition at line 5065 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_force_off_dspi_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_dspi_hclk | ( | void |  | ) |

Enabling force to turn off the clock for DSPI slave.

Register | BitsName ----------|-------- PERIPH_GC | DSPI_PCLK

Return values

  None |

Definition at line 2568 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_force_off_efuse_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_efuse_hclk | ( | void |  | ) |

Enabling force to turn off the clock for EFUSE.

Register | BitsName ----------|-------- SECU_CLK_CTRL | EFUSE_HCLK_FRC_OFF

Return values

  None |

Definition at line 4591 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_force_off_gpadc_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_gpadc_hclk | ( | void |  | ) |

Enabling force to turn off the clock for GPADC.

Register | BitsName ----------|-------- MCU_MISC_CLK | GPADC_HCLK_FRC_OFF

Return values

  None |

Definition at line 4943 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_force_off_gpio_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_gpio_hclk | ( | void |  | ) |

Enabling force to turn off the clock for GPIO.

Register | BitsName ----------|-------- CG_CTRL_1 | GPIO_HCLK

Return values

  None |

Definition at line 1503 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_force_off_hmac_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_hmac_hclk | ( | void |  | ) |

Enabling force to turn off the clock for HMAC.

Register | BitsName ----------|-------- SECU_CLK_CTRL | HMAC_HCLK_FRC_OFF

Return values

  None |

Definition at line 4388 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_force_off_htb_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_htb_hclk | ( | void |  | ) |

Enabling force to turn off the clock for Hopping Table.

Register | BitsName ----------|-------- CG_CTRL_1 | HTB_HCLK

Return values

  None |

Definition at line 1377 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_force_off_i2c0_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_i2c0_hclk | ( | void |  | ) |

Enabling force to turn off the clock for I2C0.

Register | BitsName ----------|-------- PERIPH_GC | I2C0_HCLK

Return values

  None |

Definition at line 2039 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_force_off_i2c1_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_i2c1_hclk | ( | void |  | ) |

Enabling force to turn off the clock for I2C1.

Register | BitsName ----------|-------- PERIPH_GC | I2C1_HCLK

Return values

  None |

Definition at line 2081 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_force_off_i2c2_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_i2c2_hclk | ( | void |  | ) |

Enabling force to turn off the clock for I2C2.

Register | BitsName ----------|-------- PERIPH_GC | I2C2_HCLK

Return values

  None |

Definition at line 2123 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_force_off_i2c3_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_i2c3_hclk | ( | void |  | ) |

Enabling force to turn off the clock for I2C3.

Register | BitsName ----------|-------- PERIPH_GC | I2C3_HCLK

Return values

  None |

Definition at line 2163 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_force_off_i2c4_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_i2c4_hclk | ( | void |  | ) |

Enabling force to turn off the clock for I2C4.

Register | BitsName ----------|-------- PERIPH_GC | I2C4_HCLK

Return values

  None |

Definition at line 2203 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_force_off_i2c5_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_i2c5_hclk | ( | void |  | ) |

Enabling force to turn off the clock for I2C5.

Register | BitsName ----------|-------- PERIPH_GC | I2C5_HCLK

Return values

  None |

Definition at line 2243 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_force_off_i2s_m_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_i2s_m_hclk | ( | void |  | ) |

Enabling force to turn off the clock for I2S master.

Register | BitsName ----------|-------- PERIPH_GC | I2S_HCLK

Return values

  None |

Definition at line 2488 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_force_off_i2s_s_p_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_i2s_s_p_hclk | ( | void |  | ) |

Enabling force to turn off the clock for I2S slave.

Register | BitsName ----------|-------- PERIPH_GC | I2S_S_PCLK

Return values

  None |

Definition at line 2528 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_force_off_pdm_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_pdm_hclk | ( | void |  | ) |

Enabling force to turn off the clock for PDM slave.

Register | BitsName ----------|-------- PERIPH_GC | PDM_PCLK

Return values

  None |

Definition at line 2608 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_force_off_pkc_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_pkc_hclk | ( | void |  | ) |

Enabling force to turn off the clock for PKC.

Register | BitsName ----------|-------- SECU_CLK_CTRL | PKC_HCLK_FRC_OFF

Return values

  None |

Definition at line 4428 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_force_off_present_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_present_hclk | ( | void |  | ) |

Enabling force to turn off the clock for PRESENT.

Register | BitsName ----------|-------- SECU_CLK_CTRL | PRESENT_HCLK_FRC_OFF

Return values

  None |

Definition at line 4468 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_force_off_pwm0_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_pwm0_hclk | ( | void |  | ) |

Enabling force to turn off the clock for PWM0.

Register | BitsName ----------|-------- PERIPH_GC | PWM0_PCLK

Return values

  None |

Definition at line 2727 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_force_off_pwm1_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_pwm1_hclk | ( | void |  | ) |

Enabling force to turn off the clock for PWM1.

Register | BitsName ----------|-------- PERIPH_GC | PWM1_PCLK

Return values

  None |

Definition at line 2769 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_force_off_qspi0_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_qspi0_hclk | ( | void |  | ) |

Enabling force to turn off the clock for QSPI0.

Register | BitsName ----------|-------- PERIPH_GC | QSPI0_HCLK

Return values

  None |

Definition at line 2367 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_force_off_qspi1_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_qspi1_hclk | ( | void |  | ) |

Enabling force to turn off the clock for QSPI1.

Register | BitsName ----------|-------- PERIPH_GC | QSPI1_HCLK

Return values

  None |

Definition at line 2407 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_force_off_qspi2_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_qspi2_hclk | ( | void |  | ) |

Enabling force to turn off the clock for QSPI2.

Register | BitsName ----------|-------- PERIPH_GC | QSPI2_HCLK

Return values

  None |

Definition at line 2447 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_force_off_ramkey_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_ramkey_hclk | ( | void |  | ) |

Enabling force to turn off the clock for RAMKEY.

Register | BitsName ----------|-------- SECU_CLK_CTRL | RAMKEY_HCLK_FRC_OFF

Return values

  None |

Definition at line 4508 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_force_off_rng_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_rng_hclk | ( | void |  | ) |

Enabling force to turn off the clock for RNG.

Register | BitsName ----------|-------- SECU_CLK_CTRL | RNG_HCLK_FRC_OFF

Return values

  None |

Definition at line 4549 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_force_off_rom_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_rom_hclk | ( | void |  | ) |

Enabling force to turn off the clock for ROM.

Register | BitsName ----------|-------- CG_CTRL_1 | ROM_HCLK

Return values

  None |

Definition at line 1419 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_force_off_secu_div4_pclk()

__STATIC_INLINE void ll_cgc_enable_force_off_secu_div4_pclk | ( | void |  | ) |

Enabling force to turn off the div4 clock for security blocks.

Register | BitsName ----------|-------- PERIPH_GC | I2S_HCLK

Return values

  None |

Definition at line 2648 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_force_off_secu_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_secu_hclk | ( | void |  | ) |

Enabling force to turn off the clock for security blocks(including AES, PKC, Present, HMAC).

Register | BitsName ----------|-------- CG_CTRL_1 | SECU_HCLK

Return values

  None |

Definition at line 1335 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_force_off_serial_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_serial_hclk | ( | void |  | ) |

Enabling force to turn off the clock for serial blocks(including I2C, UART, QSPI, I2S, SPI).

Register | BitsName ----------|-------- CG_CTRL_1 | SERIAL_HCLK

Return values

  None |

Definition at line 1629 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_force_off_snsadc_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_snsadc_hclk | ( | void |  | ) |

Enabling force to turn off the clock for SNSADC.

Register | BitsName ----------|-------- CG_CTRL_1 | SNSADC_HCLK

Return values

  None |

Definition at line 1461 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_force_off_spim_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_spim_hclk | ( | void |  | ) |

Enabling force to turn off the clock for SPIM.

Register | BitsName ----------|-------- PERIPH_GC | SPIM_HCLK

Return values

  None |

Definition at line 2283 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_force_off_spis_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_spis_hclk | ( | void |  | ) |

Enabling force to turn off the clock for SPIS.

Register | BitsName ----------|-------- PERIPH_GC | SPIS_HCLK

Return values

  None |

Definition at line 2325 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_force_off_sram_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_sram_hclk | ( | void |  | ) |

Enabling force to turn off the clock for SRAM.

Register | BitsName ----------|-------- CG_CTRL_2 | SRAM_HCLK

Return values

  None |

Definition at line 1753 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_force_off_uart0_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_uart0_hclk | ( | void |  | ) |

Enabling force to turn off the clock for UART0.

Register | BitsName ----------|-------- PERIPH_GC | UART0_HCLK

Return values

  None |

Definition at line 1795 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_force_off_uart1_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_uart1_hclk | ( | void |  | ) |

Enabling force to turn off the clock for UART1.

Register | BitsName ----------|-------- PERIPH_GC | UART1_HCLK

Return values

  None |

Definition at line 1837 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_force_off_uart2_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_uart2_hclk | ( | void |  | ) |

Enabling force to turn off the clock for UART2.

Register | BitsName ----------|-------- PERIPH_GC | UART2_HCLK

Return values

  None |

Definition at line 1879 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_force_off_uart3_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_uart3_hclk | ( | void |  | ) |

Enabling force to turn off the clock for UART3.

Register | BitsName ----------|-------- PERIPH_GC | UART3_HCLK

Return values

  None |

Definition at line 1919 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_force_off_uart4_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_uart4_hclk | ( | void |  | ) |

Enabling force to turn off the clock for UART4.

Register | BitsName ----------|-------- PERIPH_GC | UART4_HCLK

Return values

  None |

Definition at line 1959 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_force_off_uart5_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_uart5_hclk | ( | void |  | ) |

Enabling force to turn off the clock for UART5.

Register | BitsName ----------|-------- PERIPH_GC | UART5_HCLK

Return values

  None |

Definition at line 1999 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_force_off_vttbl_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_vttbl_hclk | ( | void |  | ) |

Enabling force to turn off the clock for VTTBL.

Register | BitsName ----------|-------- PERIPH_GC | VTTBL_PCLK

Return values

  None |

Definition at line 2811 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_force_off_xf_xqspi_div4_pclk()

__STATIC_INLINE void ll_cgc_enable_force_off_xf_xqspi_div4_pclk | ( | void |  | ) |

Enabling force to turn off the div4 clock for xf qspi blocks.

Register | BitsName ----------|-------- PERIPH_GC | XQSPI_HCLK

Return values

  None |

Definition at line 2687 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_force_off_xqspi_hclk()

__STATIC_INLINE void ll_cgc_enable_force_off_xqspi_hclk | ( | void |  | ) |

Enabling force to turn off the clock for XQSPI.

Register | BitsName ----------|-------- CG_CTRL_2 | XF_XQSPI_HCLK

Return values

  None |

Definition at line 1711 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_force_off_xqspi_sck()

__STATIC_INLINE void ll_cgc_enable_force_off_xqspi_sck | ( | void |  | ) |

Enable XQSPI SCK CLK turn off.

Register | BitsName ----------|-------- MCU_MISC_CLK |XQSPI SCK CLK_OFF

Return values

  None |

Definition at line 5023 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_i2c0_slp_wfi()

__STATIC_INLINE void ll_cgc_enable_i2c0_slp_wfi | ( | void |  | ) |

Enable turn I2C0 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | I2C0_SLP

Return values

  None |

Definition at line 3568 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_i2c1_slp_wfi()

__STATIC_INLINE void ll_cgc_enable_i2c1_slp_wfi | ( | void |  | ) |

Enable turn I2C1 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | I2C1_SLP

Return values

  None |

Definition at line 3610 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_i2c2_slp_wfi()

__STATIC_INLINE void ll_cgc_enable_i2c2_slp_wfi | ( | void |  | ) |

Enable turn I2C2 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | I2C2_SLP

Return values

  None |

Definition at line 3652 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_i2c3_slp_wfi()

__STATIC_INLINE void ll_cgc_enable_i2c3_slp_wfi | ( | void |  | ) |

Enable turn I2C3 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | I2C3_SLP

Return values

  None |

Definition at line 3692 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_i2c4_slp_wfi()

__STATIC_INLINE void ll_cgc_enable_i2c4_slp_wfi | ( | void |  | ) |

Enable turn I2C4 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | I2C4_SLP

Return values

  None |

Definition at line 3732 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_i2c5_slp_wfi()

__STATIC_INLINE void ll_cgc_enable_i2c5_slp_wfi | ( | void |  | ) |

Enable turn I2C5 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | I2C5_SLP

Return values

  None |

Definition at line 3772 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_i2c_sclk_low_power()

__STATIC_INLINE void ll_cgc_enable_i2c_sclk_low_power | ( | void |  | ) |

Enable i2c sclk low-power feature.

Register | BitsName ---------|-------- CG_LP_EN | I2C_LP_SCLK

Return values

  None |

Definition at line 3116 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_i2s_low_power()

__STATIC_INLINE void ll_cgc_enable_i2s_low_power | ( | void |  | ) |

Enable i2s low-power feature.

Register | BitsName ---------|-------- CG_LP_EN | I2S_LP

Return values

  None |

Definition at line 2992 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_i2s_m_slp_wfi()

__STATIC_INLINE void ll_cgc_enable_i2s_m_slp_wfi | ( | void |  | ) |

Enable turn I2S_M off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | I2SM_SLP

Return values

  None |

Definition at line 3812 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_i2s_s_slp_wfi()

__STATIC_INLINE void ll_cgc_enable_i2s_s_slp_wfi | ( | void |  | ) |

Enable turn I2S_S off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | I2SS_SLP

Return values

  None |

Definition at line 3852 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_pdm_slp_wfi()

__STATIC_INLINE void ll_cgc_enable_pdm_slp_wfi | ( | void |  | ) |

Enable turn PDM off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | PDM_SLP

Return values

  None |

Definition at line 4220 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_pwm0_slp_wfi()

__STATIC_INLINE void ll_cgc_enable_pwm0_slp_wfi | ( | void |  | ) |

Enable turn pwm0 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | PWM0_SLP

Return values

  None |

Definition at line 3976 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_pwm1_slp_wfi()

__STATIC_INLINE void ll_cgc_enable_pwm1_slp_wfi | ( | void |  | ) |

Enable turn pwm1 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | PWM1_SLP

Return values

  None |

Definition at line 4018 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_qspim0_slp_wfi()

__STATIC_INLINE void ll_cgc_enable_qspim0_slp_wfi | ( | void |  | ) |

Enable turn QSPIM0 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | QSPIM0_SLP

Return values

  None |

Definition at line 4060 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_qspim1_slp_wfi()

__STATIC_INLINE void ll_cgc_enable_qspim1_slp_wfi | ( | void |  | ) |

Enable turn QSPIM1 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | QSPIM1_SLP

Return values

  None |

Definition at line 4100 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_qspim2_slp_wfi()

__STATIC_INLINE void ll_cgc_enable_qspim2_slp_wfi | ( | void |  | ) |

Enable turn QSPIM2 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | QSPIM2_SLP

Return values

  None |

Definition at line 4140 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_qspim_low_power()

__STATIC_INLINE void ll_cgc_enable_qspim_low_power | ( | void |  | ) |

Enable QSPIM low-power feature.

Register | BitsName ---------|-------- CG_LP_EN | QSPIM_LP

Return values

  None |

Definition at line 3200 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_spi_m_slp_wfi()

__STATIC_INLINE void ll_cgc_enable_spi_m_slp_wfi | ( | void |  | ) |

Enable turn SPI_M off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | SPIM_SLP

Return values

  None |

Definition at line 3892 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_spi_s_slp_wfi()

__STATIC_INLINE void ll_cgc_enable_spi_s_slp_wfi | ( | void |  | ) |

Enable turn SPI_S off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | SPIS_SLP

Return values

  None |

Definition at line 3934 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_spim_sclk_low_power()

__STATIC_INLINE void ll_cgc_enable_spim_sclk_low_power | ( | void |  | ) |

Enable spim sclk low-power feature.

Register | BitsName ---------|-------- CG_LP_EN | SPIM_LP_SCLK

Return values

  None |

Definition at line 3032 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_spis_sclk_low_power()

__STATIC_INLINE void ll_cgc_enable_spis_sclk_low_power | ( | void |  | ) |

Enable spis sclk low-power feature.

Register | BitsName ---------|-------- CG_LP_EN | SPIS_LP_SCLK

Return values

  None |

Definition at line 3074 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_uart0_slp_wfi()

__STATIC_INLINE void ll_cgc_enable_uart0_slp_wfi | ( | void |  | ) |

Enable turn UART0 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | UART0_SLP

Return values

  None |

Definition at line 3324 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_uart1_slp_wfi()

__STATIC_INLINE void ll_cgc_enable_uart1_slp_wfi | ( | void |  | ) |

Enable turn UART1 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | UART1_SLP

Return values

  None |

Definition at line 3366 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_uart2_slp_wfi()

__STATIC_INLINE void ll_cgc_enable_uart2_slp_wfi | ( | void |  | ) |

Enable turn UART2 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | UART2_SLP

Return values

  None |

Definition at line 3408 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_uart3_slp_wfi()

__STATIC_INLINE void ll_cgc_enable_uart3_slp_wfi | ( | void |  | ) |

Enable turn UART3 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | UART3_SLP

Return values

  None |

Definition at line 3448 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_uart4_slp_wfi()

__STATIC_INLINE void ll_cgc_enable_uart4_slp_wfi | ( | void |  | ) |

Enable turn UART4 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | UART4_SLP

Return values

  None |

Definition at line 3488 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_uart5_slp_wfi()

__STATIC_INLINE void ll_cgc_enable_uart5_slp_wfi | ( | void |  | ) |

Enable turn UART5 off during WFI/WFE.

Register | BitsName ---------|-------- CLK_SLP_OFF | UART5_SLP

Return values

  None |

Definition at line 3528 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_uart_pclk_low_power()

__STATIC_INLINE void ll_cgc_enable_uart_pclk_low_power | ( | void |  | ) |

Enable uart pclk low-power feature.

Register | BitsName ---------|-------- CG_LP_EN | UART_LP_PCLK

Return values

  None |

Definition at line 2950 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_uart_sclk_low_power()

__STATIC_INLINE void ll_cgc_enable_uart_sclk_low_power | ( | void |  | ) |

Enable uart sclk low-power feature.

Register | BitsName ---------|-------- CG_LP_EN | UART_LP_SCLK

Return values

  None |

Definition at line 2908 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_wfi_off_aes_hclk()

__STATIC_INLINE void ll_cgc_enable_wfi_off_aes_hclk | ( | void |  | ) |

Enable AES automatic turn off clock during WFI/WFE.

Register | BitsName ----------|-------- SECU_CLK_CTRL | AES_HCLK_SLP_OFF

Return values

  None |

Definition at line 4633 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_wfi_off_aon_mcusub_hclk()

__STATIC_INLINE void ll_cgc_enable_wfi_off_aon_mcusub_hclk | ( | void |  | ) |

Enable AON_MUCSUB automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_2 | AON_MCUSUB_HCLK

Return values

  None |

Definition at line 1128 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_wfi_off_apb_sub_hclk()

__STATIC_INLINE void ll_cgc_enable_wfi_off_apb_sub_hclk | ( | void |  | ) |

Enable APB Subsystem automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_0 | APB_SUB_HCLK

Return values

  None |

Definition at line 1043 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_wfi_off_ble_brg_hclk()

__STATIC_INLINE void ll_cgc_enable_wfi_off_ble_brg_hclk | ( | void |  | ) |

Enable BLE Bridge automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_0 | BLE_BRG_HCLK

Return values

  None |

Definition at line 1001 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_wfi_off_dma_hclk()

__STATIC_INLINE void ll_cgc_enable_wfi_off_dma_hclk | ( | void |  | ) |

Enable DMA automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_0 | DMA_HCLK

Return values

  None |

Definition at line 961 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_wfi_off_efuse_hclk()

__STATIC_INLINE void ll_cgc_enable_wfi_off_efuse_hclk | ( | void |  | ) |

Enable EFUSE automatic turn off clock during WFI/WFE.

Register | BitsName ----------|-------- SECU_CLK_CTRL | EFUSE_HCLK_SLP_OFF

Return values

  None |

Definition at line 4875 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_wfi_off_gpadc_hclk()

__STATIC_INLINE void ll_cgc_enable_wfi_off_gpadc_hclk | ( | void |  | ) |

Enable GPADC automatic turn off clock during WFI/WFE.

Register | BitsName ----------|-------- MCU_MISC_CLK |GPADC_HCLK_SLP_OFF

Return values

  None |

Definition at line 4983 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_wfi_off_gpio_hclk()

__STATIC_INLINE void ll_cgc_enable_wfi_off_gpio_hclk | ( | void |  | ) |

Enable GPIO automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_0 | GPIO_HCLK

Return values

  None |

Definition at line 919 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_wfi_off_hmac_hclk()

__STATIC_INLINE void ll_cgc_enable_wfi_off_hmac_hclk | ( | void |  | ) |

Enable HMAC automatic turn off clock during WFI/WFE.

Register | BitsName ----------|-------- SECU_CLK_CTRL | HMAC_HCLK_SLP_OFF

Return values

  None |

Definition at line 4673 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_wfi_off_htb_hclk()

__STATIC_INLINE void ll_cgc_enable_wfi_off_htb_hclk | ( | void |  | ) |

Enable Hopping Table automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_0 | HTB_HCLK

Return values

  None |

Definition at line 753 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_wfi_off_pkc_hclk()

__STATIC_INLINE void ll_cgc_enable_wfi_off_pkc_hclk | ( | void |  | ) |

Enable PKC automatic turn off clock during WFI/WFE.

Register | BitsName ----------|-------- SECU_CLK_CTRL | PKC_HCLK_SLP_OFF

Return values

  None |

Definition at line 4713 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_wfi_off_present_hclk()

__STATIC_INLINE void ll_cgc_enable_wfi_off_present_hclk | ( | void |  | ) |

Enable PRESENT automatic turn off clock during WFI/WFE.

Register | BitsName ----------|-------- SECU_CLK_CTRL | PRESENT_HCLK_SLP_OFF

Return values

  None |

Definition at line 4753 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_wfi_off_pwm_hclk()

__STATIC_INLINE void ll_cgc_enable_wfi_off_pwm_hclk | ( | void |  | ) |

Enable PWM automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_0 | PWM_HCLK

Return values

  None |

Definition at line 795 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_wfi_off_ramkey_hclk()

__STATIC_INLINE void ll_cgc_enable_wfi_off_ramkey_hclk | ( | void |  | ) |

Enable RAMKEY automatic turn off clock during WFI/WFE.

Register | BitsName ----------|-------- SECU_CLK_CTRL | RAMKEY_HCLK_SLP_OFF

Return values

  None |

Definition at line 4793 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_wfi_off_rng_hclk()

__STATIC_INLINE void ll_cgc_enable_wfi_off_rng_hclk | ( | void |  | ) |

Enable RNG automatic turn off clock during WFI/WFE.

Register | BitsName ----------|-------- SECU_CLK_CTRL | RNG_HCLK_SLP_OFF

Return values

  None |

Definition at line 4833 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_wfi_off_rom_hclk()

__STATIC_INLINE void ll_cgc_enable_wfi_off_rom_hclk | ( | void |  | ) |

Enable ROM automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_0 | ROM_HCLK

Return values

  None |

Definition at line 835 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_wfi_off_secu_div4_hclk()

__STATIC_INLINE void ll_cgc_enable_wfi_off_secu_div4_hclk | ( | void |  | ) |

Enable security blocks automatic turn off div4 clock during WFI.

Register | BitsName ----------|-------- PERIPH_GC | SECU_DIV4_PCLK

Return values

  None |

Definition at line 1254 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_wfi_off_secu_hclk()

__STATIC_INLINE void ll_cgc_enable_wfi_off_secu_hclk | ( | void |  | ) |

Enable security blocks(including AES, PKC, Present, HMAC) automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_0 | SECU_HCLK

Return values

  None |

Definition at line 671 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_wfi_off_serial_hclk()

__STATIC_INLINE void ll_cgc_enable_wfi_off_serial_hclk | ( | void |  | ) |

Enable serial blocks(including I2C, UART, QSPI, I2S, SPI) automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_0 | SERIAL_HCLK

Return values

  None |

Definition at line 1085 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_wfi_off_sim_hclk()

__STATIC_INLINE void ll_cgc_enable_wfi_off_sim_hclk | ( | void |  | ) |

Enable SIM automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_0 | SIM_HCLK

Return values

  None |

Definition at line 713 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_wfi_off_snsadc_hclk()

__STATIC_INLINE void ll_cgc_enable_wfi_off_snsadc_hclk | ( | void |  | ) |

Enable SNSADC automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_0 | SNSADC_HCLK

Return values

  None |

Definition at line 877 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_wfi_off_sram_hclk()

__STATIC_INLINE void ll_cgc_enable_wfi_off_sram_hclk | ( | void |  | ) |

Enable SRAM automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_2 | SRAM_HCLK

Return values

  None |

Definition at line 1212 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_enable_wfi_off_xqspi_div4_hclk()

__STATIC_INLINE void ll_cgc_enable_wfi_off_xqspi_div4_hclk | ( | void |  | ) |

Enable XQSPI automatic turn off div4 clock during WFI.

Register | BitsName ----------|-------- PERIPH_GC | XQSPI_DIV4_PCLK

Return values

  None |

Definition at line 1295 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_enable_wfi_off_xqspi_hclk()

__STATIC_INLINE void ll_cgc_enable_wfi_off_xqspi_hclk | ( | void |  | ) |

Enable XQSPI automatic turn off clock during WFI.

Register | BitsName ----------|-------- CG_CTRL_2 | XF_XQSPI_HCLK

Return values

  None |

Definition at line 1170 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_get_force_off_hclk_0()

__STATIC_INLINE uint32_t ll_cgc_get_force_off_hclk_0 | ( | void |  | ) |

Return to clock blocks that was forcibly closed.(Include: Security/SIM/HTB/ ROM/SNSADC/GPIO/DMA/BLE_BRG/APB_SUB/SERIAL/I2S)

Register | BitsName ----------|-------- CG_CTRL_1 | SECU_HCLK CG_CTRL_1 | SIM_HCLK CG_CTRL_1 | HTB_HCLK CG_CTRL_1 | ROM_HCLK CG_CTRL_1 | SNSADC_HCLK CG_CTRL_1 | GPIO_HCLK CG_CTRL_1 | DMA_HCLK CG_CTRL_1 | BLE_BRG_HCLK CG_CTRL_1 | APB_SUB_HCLK CG_CTRL_1 | SERIAL_HCLK

Return values

  Returned | value can be a combination of the following values: LL_CGC_FRC_SECU_HCLK LL_CGC_FRC_HTB_HCLK LL_CGC_FRC_ROM_HCLK LL_CGC_FRC_SNSADC_HCLK LL_CGC_FRC_GPIO_HCLK LL_CGC_FRC_BLE_BRG_HCLK LL_CGC_FRC_APB_SUB_HCLK LL_CGC_FRC_SERIAL_HCLK

Definition at line 519 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_get_force_off_hclk_1()

__STATIC_INLINE uint32_t ll_cgc_get_force_off_hclk_1 | ( | void |  | ) |

Return to clock blocks that was forcibly closed.(Include: AON_MCUSUB/XF_XQSPI/SRAM)

Register | BitsName ----------|-------- CG_CTRL_2 | AON_MCUSUB_HCLK CG_CTRL_2 | XF_XQSPI_HCLK CG_CTRL_2 | SRAM_HCLK

Return values

  Returned | value can be a combination of the following values: LL_CGC_FRC_XF_XQSPI_HCLK LL_CGC_FRC_SRAM_HCLK

Definition at line 556 of file gr533x_ll_cgc.h.

References LL_CGC_FRC_ALL_HCLK1.

## ◆ ll_cgc_get_force_off_hclk_2()

__STATIC_INLINE uint32_t ll_cgc_get_force_off_hclk_2 | ( | void |  | ) |

Return to clock blocks that was forcibly closed.(Include: UART0_HCLK/UART1_HCLK/UART2_HCLK/UART3_HCLK/UART4_HCLK/UART5_HCLK/ I2C0_HCLK/I2C1_HCLK/SPIM_HCLK/SPIS_HCLK/QSPI0_HCLK/QSPI1_HCLK/I2S_HCLK/SECU_DIV4_PCLK/XQSPI_DIV4_PCLK/PWM0/PWM1)

Register | BitsName ----------|-------- PERIPH_GC | UART0_HCLK PERIPH_GC | UART1_HCLK PERIPH_GC | I2C0_HCLK PERIPH_GC | I2C1_HCLK PERIPH_GC | SPIM_HCLK PERIPH_GC | SPIS_HCLK PERIPH_GC | XQSPI_DIV4_PCLK PERIPH_GC | PWM0_HCLK PERIPH_GC | PWM1_HCLK

Return values

  Returned | value can be a combination of the following values: LL_CGC_FRC_UART0_PCLK LL_CGC_FRC_UART1_PCLK LL_CGC_FRC_I2C0_PCLK LL_CGC_FRC_I2C1_PCLK LL_CGC_FRC_SPI_M_PCLK LL_CGC_FRC_SPI_S_PCLK LL_CGC_FRC_SERIALS_HCLK2 LL_CGC_FRC_PWM_0_PCLK LL_CGC_FRC_PWM_1_PCLK

Definition at line 622 of file gr533x_ll_cgc.h.

References LL_CGC_FRC_ALL_HCLK2.

## ◆ ll_cgc_get_force_off_hclk_3()

__STATIC_INLINE uint32_t ll_cgc_get_force_off_hclk_3 | ( | void |  | ) |

Return to clock blocks that is turned off.(Include: AES/HMAC/PKC/RNG.etc)

Register | BitsName ----------|-------- PERIPH_GC | AES/HMAC/PKC/RNG/EFUSE

Return values

  Returned | value can be a combination of the following values: LL_CGC_MCU_FRC_RNG_HCLK_OFF_EN ..... LL_CGC_MCU_SLP_EFUSE_HCLK_OFF_EN

Definition at line 657 of file gr533x_ll_cgc.h.

References LL_CGC_MCU_SECU_FRC_OFF_HCLK.

## ◆ ll_cgc_get_force_off_secu()

__STATIC_INLINE uint32_t ll_cgc_get_force_off_secu | ( | void |  | ) |

Return to clock blocks that was forcibly closed inside security system.(Include: AES/HMAC/PKC/PRESENT/RAMKAY/RNG/EFUSE)

Register | BitsName ----------|-------- SECU_CLK_CTRL | AES_HCLK_FRC_OFF SECU_CLK_CTRL | HMAC_HCLK_FRC_OFF SECU_CLK_CTRL | PKC_HCLK_FRC_OFF SECU_CLK_CTRL | PRESENT_HCLK_FRC_OFF SECU_CLK_CTRL | RAMKEY_HCLK_FRC_OFF SECU_CLK_CTRL | RNG_HCLK_FRC_OFF SECU_CLK_CTRL | EFUSE_HCLK_FRC_OFF

Return values

  Returned | value can be a combination of the following values: LL_CGC_MCU_FRC_RNG_HCLK_OFF_EN LL_CGC_MCU_FRC_EFUSE_HCLK_OFF_EN

Definition at line 4291 of file gr533x_ll_cgc.h.

References LL_CGC_MCU_SECU_FRC_OFF_HCLK.

## ◆ ll_cgc_get_mcu_periph_low_power()

__STATIC_INLINE uint32_t ll_cgc_get_mcu_periph_low_power | ( | void |  | ) |

Return to clock blocks that has low power feature. (Include: UART/I2S/SPIM/SPIS/I2C/AHB BUS)

Register | BitsName ---------|-------- CG_LP_EN | UART_LP_SCLK CG_LP_EN | UART_LP_PCLK CG_LP_EN | I2S_LP CG_LP_EN | SPIM_LP_SCLK CG_LP_EN | SPIS_LP_SCLK CG_LP_EN | I2C_LP_SCLK CG_LP_EN | AHB_BUS_LP

Return values

  Returned | value can be a combination of the following values: LL_CGC_MCU_PERIPH_CG_LP_EN_AHB2APB_EN LL_CGC_MCU_PERIPH_CG_LP_EN_AHB2APB_SYNC_EN LL_CGC_MCU_PERIPH_CG_LP_EN_AHB_BUS_LP_EN LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_LP_SCLK_EN LL_CGC_MCU_PERIPH_CG_LP_EN_SPIS_LP_SCLK_EN LL_CGC_MCU_PERIPH_CG_LP_EN_SPIM_LP_SCLK_EN LL_CGC_MCU_PERIPH_CG_LP_EN_UART_LP_PCLK_EN LL_CGC_MCU_PERIPH_CG_LP_EN_UART_LP_SCLK_EN

Definition at line 2894 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_get_misc_clk()

__STATIC_INLINE uint32_t ll_cgc_get_misc_clk | ( | void |  | ) |

Return to MISC_CLK clock blocks that is turned off.(Include: GPADC/XQSPI/DMA0)

Register | BitsName ----------|-------- MCU_MISC_CLK | GPADC/XQSPI/DMA0

Definition at line 4929 of file gr533x_ll_cgc.h.

References LL_CGC_MCU_MISC_CLK.

## ◆ ll_cgc_get_slp_off_secu()

__STATIC_INLINE uint32_t ll_cgc_get_slp_off_secu | ( | void |  | ) |

Return to security clock blocks that is turned off during WFI/WFE.(Include: AES/HMAC/PKC/PRESENT/RAMKAY/RNG/EFUSE)

Register | BitsName ----------|-------- SECU_CLK_CTRL | AES_HCLK_SLP_OFF SECU_CLK_CTRL | HMAC_HCLK_SLP_OFF SECU_CLK_CTRL | PKC_HCLK_SLP_OFF SECU_CLK_CTRL | PRESENT_HCLK_SLP_OFF

Return values

  Returned | value can be a combination of the following values: LL_CGC_MCU_FRC_RNG_HCLK_OFF_EN LL_CGC_MCU_SLP_RNG_HCLK_OFF_EN LL_CGC_MCU_FRC_EFUSE_HCLK_OFF_EN LL_CGC_MCU_SLP_EFUSE_HCLK_OFF_EN

Definition at line 4334 of file gr533x_ll_cgc.h.

References LL_CGC_MCU_SECU_FRC_OFF_WFI_HCLK.

## ◆ ll_cgc_get_wfi_off_hclk_0()

__STATIC_INLINE uint32_t ll_cgc_get_wfi_off_hclk_0 | ( | void |  | ) |

Return to clock blocks that is turned off during WFI.(Include: Security/SIM/HTB/PWM/ ROM/SNSADC/GPIO/DMA/BLE_BRG/APB_SUB/SERIAL/I2S)

Register | BitsName ----------|-------- CG_CTRL_0 | SECU_HCLK CG_CTRL_0 | SIM_HCLK CG_CTRL_0 | HTB_HCLK CG_CTRL_0 | PWM_HCLK CG_CTRL_0 | ROM_HCLK CG_CTRL_0 | SNSADC_HCLK CG_CTRL_0 | GPIO_HCLK CG_CTRL_0 | DMA_HCLK CG_CTRL_0 | BLE_BRG_HCLK CG_CTRL_0 | APB_SUB_HCLK CG_CTRL_0 | SERIAL_HCLK

Return values

  Returned | value can be a combination of the following values: LL_CGC_WFI_SECU_HCLK LL_CGC_WFI_HTB_HCLK LL_CGC_WFI_ROM_HCLK LL_CGC_WFI_SNSADC_HCLK LL_CGC_WFI_GPIO_HCLK LL_CGC_WFI_BLE_BRG_HCLK LL_CGC_WFI_APB_SUB_HCLK LL_CGC_WFI_SERIAL_HCLK

Definition at line 313 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_get_wfi_off_hclk_1()

__STATIC_INLINE uint32_t ll_cgc_get_wfi_off_hclk_1 | ( | void |  | ) |

Return to clock blocks that is turned off during WFI.(Include: AON_MCUSUB/XF_XQSPI/SRAM)

Register | BitsName ----------|-------- CG_CTRL_2 | AON_MCUSUB_HCLK CG_CTRL_2 | XF_XQSPI_HCLK CG_CTRL_2 | SRAM_HCLK

Return values

  Returned | value can be a combination of the following values: LL_CGC_WFI_AON_MCUSUB_HCLK LL_CGC_WFI_XF_XQSPI_HCLK LL_CGC_WFI_SRAM_HCLK

Definition at line 352 of file gr533x_ll_cgc.h.

References LL_CGC_WFI_ALL_HCLK1.

## ◆ ll_cgc_get_wfi_off_hclk_2()

__STATIC_INLINE uint32_t ll_cgc_get_wfi_off_hclk_2 | ( | void |  | ) |

Return to clock blocks that is turned off during WFI.(Include: AON_MCUSUB/XF_XQSPI/SRAM)

Register | BitsName ----------|-------- PERIPH_GC | SECU_DIV4_PCLK PERIPH_GC | XQSPI_DIV4_PCLK

Return values

  Returned | value can be a combination of the following values:

Definition at line 382 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_get_wfi_off_hclk_3()

__STATIC_INLINE uint32_t ll_cgc_get_wfi_off_hclk_3 | ( | void |  | ) |

Return to clock blocks that is turned off during WFI.(Include: UART/DSPI.I2C/QSPI.etc)

Register | BitsName ----------|-------- PERIPH_GC | UART0 - UART5/I2C0 - I2C5 PERIPH_GC | I2SM/I2SS/SPIM/SPIS/PWM0/PWM1//QSPIM0/QSPIM1/QSPIM2/DSPI/PDM

Return values

  Returned | value can be a combination of the following values: LL_CGC_MCU_PERIPH_CG_LP_EN_UART_0_SLP_OFF LL_CGC_MCU_PERIPH_CG_LP_EN_UART_1_SLP_OFF ..... LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_1_SLP_OFF

Definition at line 421 of file gr533x_ll_cgc.h.

References LL_CGC_MCU_PERIPH_SERIALS_SLP_ALL.

## ◆ ll_cgc_get_wfi_off_hclk_4()

__STATIC_INLINE uint32_t ll_cgc_get_wfi_off_hclk_4 | ( | void |  | ) |

Return to clock blocks that is turned off during WFI.(Include: AES/HMAC/PKC/RNG.etc)

Register | BitsName ----------|-------- PERIPH_GC | AES/HMAC/PKC/RNG/EFUSE

Return values

  Returned | value can be a combination of the following values: LL_CGC_MCU_FRC_RNG_HCLK_OFF_EN ..... LL_CGC_MCU_SLP_EFUSE_HCLK_OFF_EN

Definition at line 456 of file gr533x_ll_cgc.h.

References LL_CGC_MCU_SECU_FRC_OFF_WFI_HCLK.

## ◆ ll_cgc_is_enabled_ahb2apb_async_bus_low_power()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_ahb2apb_async_bus_low_power | ( | void |  | ) |

Indicate whether the ahb bus low-power is enabled.

Register | BitsName ---------|-------- CG_LP_EN | AHB_BUS_LP

Return values

  State | of bit (1 or 0).

Definition at line 3310 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_ahb2apb_sync_bus_low_power()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_ahb2apb_sync_bus_low_power | ( | void |  | ) |

Indicate whether the AHB2APB bus low-power is enabled.

Register | BitsName ---------|-------- CG_LP_EN | AHB2APB_BUS_LP

Return values

  State | of bit (1 or 0).

Definition at line 3268 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_ahb_bus_low_power()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_ahb_bus_low_power | ( | void |  | ) |

Indicate whether the ahb bus low-power is enabled.

Register | BitsName ---------|-------- CG_LP_EN | AHB_BUS_LP

Return values

  State | of bit (1 or 0).

Definition at line 3186 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_dspi_slp_wfi()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_dspi_slp_wfi | ( | void |  | ) |

Indicate whether turn DSPI off during WFI/WFE is enabled.

Register | BitsName ---------|-------- CLK_SLP_OFF | DSPI_SLP

Return values

  State | of bit (1 or 0).

Definition at line 4206 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_force_off_aes_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_aes_hclk | ( | void |  | ) |

Indicate whether the clock for AES is forced to close.

Register | BitsName ----------|-------- SECU_CLK_CTRL | AES_HCLK_FRC_OFF

Return values

  State | of bit (1 or 0).

Definition at line 4374 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_force_off_aon_mcusub_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_aon_mcusub_hclk | ( | void |  | ) |

Indicate whether the clock for AON_MUCSUB is forced to close.

Register | BitsName ----------|-------- CG_CTRL_2 | AON_MCUSUB_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 1697 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_force_off_apb_sub_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_apb_sub_hclk | ( | void |  | ) |

Indicate whether the clock for APB Subsystem is forced to close.

Register | BitsName ----------|-------- CG_CTRL_1 | APB_SUB_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 1615 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_force_off_ble_brg_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_ble_brg_hclk | ( | void |  | ) |

Indicate whether the clock for BLE Bridge is forced to close.

Register | BitsName ----------|-------- CG_CTRL_1 | BLE_BRG_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 1573 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_force_off_dma0_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_dma0_hclk | ( | void |  | ) |

Indicate whether the DMA0 automatic turn off clock is enabled.

Register | BitsName ----------|-------- MCU_MISC_CLK | DMA0_OFF

Return values

  State | of bit (1 or 0).

Definition at line 5093 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_force_off_dspi_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_dspi_hclk | ( | void |  | ) |

Indicate whether the clock for DSPI is forced to close.

Register | BitsName ----------|-------- PERIPH_GC | DSPI_PCLK

Return values

  State | of bit (1 or 0).

Definition at line 2594 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_force_off_efuse_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_efuse_hclk | ( | void |  | ) |

Indicate whether the clock for EFUSE is forced to close.

Register | BitsName ----------|-------- SECU_CLK_CTRL | EFUSE_HCLK_FRC_OFF

Return values

  State | of bit (1 or 0).

Definition at line 4619 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_force_off_gpadc_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_gpadc_hclk | ( | void |  | ) |

Indicate whether the clock for GPADC is forced to close.

Register | BitsName ----------|-------- MCU_MISC_CLK | GPADC_HCLK_FRC_OFF

Return values

  State | of bit (1 or 0).

Definition at line 4969 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_force_off_gpio_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_gpio_hclk | ( | void |  | ) |

Indicate whether the clock for GPIO is forced to close.

Register | BitsName ----------|-------- CG_CTRL_1 | GPIO_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 1531 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_force_off_hmac_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_hmac_hclk | ( | void |  | ) |

Indicate whether the clock for HMAC is forced to close.

Register | BitsName ----------|-------- SECU_CLK_CTRL | HMAC_HCLK_FRC_OFF

Return values

  State | of bit (1 or 0).

Definition at line 4414 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_force_off_htb_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_htb_hclk | ( | void |  | ) |

Indicate whether the clock for Hopping Table is forced to close.

Register | BitsName ----------|-------- CG_CTRL_1 | HTB_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 1405 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_force_off_i2c0_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_i2c0_hclk | ( | void |  | ) |

Indicate whether the clock for I2C0 is forced to close.

Register | BitsName ----------|-------- PERIPH_GC | I2C0_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 2067 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_force_off_i2c1_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_i2c1_hclk | ( | void |  | ) |

Indicate whether the clock for I2C1 is forced to close.

Register | BitsName ----------|-------- PERIPH_GC | I2C1_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 2109 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_force_off_i2c2_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_i2c2_hclk | ( | void |  | ) |

Indicate whether the clock for I2C2 is forced to close.

Register | BitsName ----------|-------- PERIPH_GC | I2C2_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 2149 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_force_off_i2c3_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_i2c3_hclk | ( | void |  | ) |

Indicate whether the clock for I2C3 is forced to close.

Register | BitsName ----------|-------- PERIPH_GC | I2C3_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 2189 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_force_off_i2c4_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_i2c4_hclk | ( | void |  | ) |

Indicate whether the clock for I2C4 is forced to close.

Register | BitsName ----------|-------- PERIPH_GC | I2C4_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 2229 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_force_off_i2c5_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_i2c5_hclk | ( | void |  | ) |

Indicate whether the clock for I2C5 is forced to close.

Register | BitsName ----------|-------- PERIPH_GC | I2C5_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 2269 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_force_off_i2s_m_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_i2s_m_hclk | ( | void |  | ) |

Indicate whether the clock for I2S master is forced to close.

Register | BitsName ----------|-------- PERIPH_GC | I2S_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 2514 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_force_off_i2s_s_p_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_i2s_s_p_hclk | ( | void |  | ) |

Indicate whether the clock for I2S slave is forced to close.

Register | BitsName ----------|-------- PERIPH_GC | I2S_S_PCLK

Return values

  State | of bit (1 or 0).

Definition at line 2554 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_force_off_pdm_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_pdm_hclk | ( | void |  | ) |

Indicate whether the clock for PDM is forced to close.

Register | BitsName ----------|-------- PERIPH_GC | PDM_PCLK

Return values

  State | of bit (1 or 0).

Definition at line 2634 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_force_off_pkc_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_pkc_hclk | ( | void |  | ) |

Indicate whether the clock for PKC is forced to close.

Register | BitsName ----------|-------- SECU_CLK_CTRL | PKC_HCLK_FRC_OFF

Return values

  State | of bit (1 or 0).

Definition at line 4454 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_force_off_present_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_present_hclk | ( | void |  | ) |

Indicate whether the clock for PRESENT is forced to close.

Register | BitsName ----------|-------- SECU_CLK_CTRL | PRESENT_HCLK_FRC_OFF

Return values

  State | of bit (1 or 0).

Definition at line 4494 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_force_off_pwm0_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_pwm0_hclk | ( | void |  | ) |

Indicate whether the clock for PWM0 is forced to close.

Register | BitsName ----------|-------- PERIPH_GC | PWM0_PCLK

Return values

  State | of bit (1 or 0).

Definition at line 2755 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_force_off_pwm1_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_pwm1_hclk | ( | void |  | ) |

Indicate whether the clock for PWM1 is forced to close.

Register | BitsName ----------|-------- PERIPH_GC | PWM1_PCLK

Return values

  State | of bit (1 or 0).

Definition at line 2797 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_force_off_qspi0_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_qspi0_hclk | ( | void |  | ) |

Indicate whether the clock for QSPI0 is forced to close.

Register | BitsName ----------|-------- PERIPH_GC | QSPI0_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 2393 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_force_off_qspi1_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_qspi1_hclk | ( | void |  | ) |

Indicate whether the clock for QSPI1 is forced to close.

Register | BitsName ----------|-------- PERIPH_GC | QSPI1_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 2433 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_force_off_qspi2_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_qspi2_hclk | ( | void |  | ) |

Indicate whether the clock for QSPI2 is forced to close.

Register | BitsName ----------|-------- PERIPH_GC | QSPI2_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 2473 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_force_off_ramkey_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_ramkey_hclk | ( | void |  | ) |

Indicate whether the clock for RAMKEY is forced to close.

Register | BitsName ----------|-------- SECU_CLK_CTRL | RAMKEY_HCLK_FRC_OFF

Return values

  State | of bit (1 or 0).

Definition at line 4534 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_force_off_rng_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_rng_hclk | ( | void |  | ) |

Indicate whether the clock for RNG is forced to close.

Register | BitsName ----------|-------- SECU_CLK_CTRL | RNG_HCLK_FRC_OFF

Return values

  State | of bit (1 or 0).

Definition at line 4577 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_force_off_rom_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_rom_hclk | ( | void |  | ) |

Indicate whether the clock for ROM is forced to close.

Register | BitsName ----------|-------- CG_CTRL_1 | ROM_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 1447 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_force_off_secu_div4_pclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_secu_div4_pclk | ( | void |  | ) |

Indicate whether the div4 clock for security blocks is forced to close.

Register | BitsName ----------|-------- PERIPH_GC | I2S_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 2674 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_force_off_secu_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_secu_hclk | ( | void |  | ) |

Indicate whether the clock for security blocks(including AES, PKC, Present, HMAC) is forced to close.

Register | BitsName ----------|-------- CG_CTRL_1 | SECU_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 1363 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_force_off_serial_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_serial_hclk | ( | void |  | ) |

Indicate whether the clock for serial blocks(including I2C, UART, QSPI, I2S, SPI) is forced to close.

Register | BitsName ----------|-------- CG_CTRL_1 | SERIAL_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 1657 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_force_off_snsadc_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_snsadc_hclk | ( | void |  | ) |

Indicate whether the clock for SNSADC is forced to close.

Register | BitsName ----------|-------- CG_CTRL_1 | SNSADC_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 1489 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_force_off_spim_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_spim_hclk | ( | void |  | ) |

Indicate whether the clock for SPIM is forced to close.

Register | BitsName ----------|-------- PERIPH_GC | SPIM_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 2311 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_force_off_spis_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_spis_hclk | ( | void |  | ) |

Indicate whether the clock for SPIS is forced to close.

Register | BitsName ----------|-------- PERIPH_GC | SPIS_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 2353 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_force_off_sram_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_sram_hclk | ( | void |  | ) |

Indicate whether the clock for SRAM is forced to close.

Register | BitsName ----------|-------- CG_CTRL_2 | SRAM_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 1781 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_force_off_uart0_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_uart0_hclk | ( | void |  | ) |

Indicate whether the clock for UART0 is forced to close.

Register | BitsName ----------|-------- PERIPH_GC | UART0_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 1823 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_force_off_uart1_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_uart1_hclk | ( | void |  | ) |

Indicate whether the clock for UART1 is forced to close.

Register | BitsName ----------|-------- PERIPH_GC | UART1_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 1865 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_force_off_uart2_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_uart2_hclk | ( | void |  | ) |

Indicate whether the clock for UART2 is forced to close.

Register | BitsName ----------|-------- PERIPH_GC | UART2_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 1905 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_force_off_uart3_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_uart3_hclk | ( | void |  | ) |

Indicate whether the clock for UART3 is forced to close.

Register | BitsName ----------|-------- PERIPH_GC | UART3_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 1945 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_force_off_uart4_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_uart4_hclk | ( | void |  | ) |

Indicate whether the clock for UART4 is forced to close.

Register | BitsName ----------|-------- PERIPH_GC | UART4_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 1985 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_force_off_uart5_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_uart5_hclk | ( | void |  | ) |

Indicate whether the clock for UART5 is forced to close.

Register | BitsName ----------|-------- PERIPH_GC | UART5_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 2025 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_force_off_vttbl_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_vttbl_hclk | ( | void |  | ) |

Indicate whether the clock for VTTBL is forced to close.

Register | BitsName ----------|-------- PERIPH_GC | VTTBL_PCLK

Return values

  State | of bit (1 or 0).

Definition at line 2837 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_force_off_xf_xqspi_div4_pclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_xf_xqspi_div4_pclk | ( | void |  | ) |

Indicate whether the div4 clock for xf qspi blocks is forced to close.

Register | BitsName ----------|-------- PERIPH_GC | XQSPI_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 2713 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_force_off_xqspi_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_xqspi_hclk | ( | void |  | ) |

Indicate whether the clock for XQSPI is forced to close.

Register | BitsName ----------|-------- CG_CTRL_2 | XF_XQSPI_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 1739 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_force_off_xqspi_sck()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_force_off_xqspi_sck | ( | void |  | ) |

Indicate whether the XQSPI SCK CLK automatic turn off clock is enabled.

Register | BitsName ----------|-------- MCU_MISC_CLK | XQSPI SCK CLK_OFF

Return values

  State | of bit (1 or 0).

Definition at line 5051 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_i2c0_slp_wfi()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_i2c0_slp_wfi | ( | void |  | ) |

Indicate whether turn I2C0 off during WFI/WFE is enabled.

Register | BitsName ---------|-------- CLK_SLP_OFF | I2C0_SLP

Return values

  State | of bit (1 or 0).

Definition at line 3596 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_i2c1_slp_wfi()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_i2c1_slp_wfi | ( | void |  | ) |

Indicate whether turn I2C1 off during WFI/WFE is enabled.

Register | BitsName ---------|-------- CLK_SLP_OFF | I2C1_SLP

Return values

  State | of bit (1 or 0).

Definition at line 3638 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_i2c2_slp_wfi()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_i2c2_slp_wfi | ( | void |  | ) |

Indicate whether turn I2C2 off during WFI/WFE is enabled.

Register | BitsName ---------|-------- CLK_SLP_OFF | I2C2_SLP

Return values

  State | of bit (1 or 0).

Definition at line 3678 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_i2c3_slp_wfi()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_i2c3_slp_wfi | ( | void |  | ) |

Indicate whether turn I2C3 off during WFI/WFE is enabled.

Register | BitsName ---------|-------- CLK_SLP_OFF | I2C3_SLP

Return values

  State | of bit (1 or 0).

Definition at line 3718 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_i2c4_slp_wfi()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_i2c4_slp_wfi | ( | void |  | ) |

Indicate whether turn I2C4 off during WFI/WFE is enabled.

Register | BitsName ---------|-------- CLK_SLP_OFF | I2C4_SLP

Return values

  State | of bit (1 or 0).

Definition at line 3758 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_i2c5_slp_wfi()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_i2c5_slp_wfi | ( | void |  | ) |

Indicate whether turn I2C5 off during WFI/WFE is enabled.

Register | BitsName ---------|-------- CLK_SLP_OFF | I2C5_SLP

Return values

  State | of bit (1 or 0).

Definition at line 3798 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_i2c_sclk_low_power()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_i2c_sclk_low_power | ( | void |  | ) |

Indicate whether the i2c sclk low-power is enabled.

Register | BitsName ---------|-------- CG_LP_EN | I2C_LP_SCLK

Return values

  State | of bit (1 or 0).

Definition at line 3144 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_i2s_low_power()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_i2s_low_power | ( | void |  | ) |

Indicate whether the i2s low-power is enabled.

Register | BitsName ---------|-------- CG_LP_EN | I2S_LP

Return values

  State | of bit (1 or 0).

Definition at line 3018 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_i2s_m_slp_wfi()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_i2s_m_slp_wfi | ( | void |  | ) |

Indicate whether turn I2S_M off during WFI/WFE is enabled.

Register | BitsName ---------|-------- CLK_SLP_OFF | I2SM_SLP

Return values

  State | of bit (1 or 0).

Definition at line 3838 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_i2s_s_slp_wfi()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_i2s_s_slp_wfi | ( | void |  | ) |

Indicate whether turn I2S_S off during WFI/WFE is enabled.

Register | BitsName ---------|-------- CLK_SLP_OFF | I2SS_SLP

Return values

  State | of bit (1 or 0).

Definition at line 3878 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_pdm_slp_wfi()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_pdm_slp_wfi | ( | void |  | ) |

Indicate whether turn PDM off during WFI/WFE is enabled.

Register | BitsName ---------|-------- CLK_SLP_OFF | PDM_SLP

Return values

  State | of bit (1 or 0).

Definition at line 4246 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_pwm0_slp_wfi()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_pwm0_slp_wfi | ( | void |  | ) |

Indicate whether turn pwm0 off during WFI/WFE is enabled.

Register | BitsName ---------|-------- CLK_SLP_OFF | PWM0_SLP

Return values

  State | of bit (1 or 0).

Definition at line 4004 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_pwm1_slp_wfi()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_pwm1_slp_wfi | ( | void |  | ) |

Indicate whether turn pwm1 off during WFI/WFE is enabled.

Register | BitsName ---------|-------- CLK_SLP_OFF | PWM1_SLP

Return values

  State | of bit (1 or 0).

Definition at line 4046 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_qspim0_slp_wfi()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_qspim0_slp_wfi | ( | void |  | ) |

Indicate whether turn QSPIM0 off during WFI/WFE is enabled.

Register | BitsName ---------|-------- CLK_SLP_OFF | QSPIM0_SLP

Return values

  State | of bit (1 or 0).

Definition at line 4086 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_qspim1_slp_wfi()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_qspim1_slp_wfi | ( | void |  | ) |

Indicate whether turn QSPIM1 off during WFI/WFE is enabled.

Register | BitsName ---------|-------- CLK_SLP_OFF | QSPIM1_SLP

Return values

  State | of bit (1 or 0).

Definition at line 4126 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_qspim2_slp_wfi()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_qspim2_slp_wfi | ( | void |  | ) |

Indicate whether turn QSPIM2 off during WFI/WFE is enabled.

Register | BitsName ---------|-------- CLK_SLP_OFF | QSPIM2_SLP

Return values

  State | of bit (1 or 0).

Definition at line 4166 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_qspim_low_power()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_qspim_low_power | ( | void |  | ) |

Indicate whether the QSPIM low-power is enabled.

Register | BitsName ---------|-------- CG_LP_EN | QSPIM_LP

Return values

  State | of bit (1 or 0).

Definition at line 3226 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_spi_m_slp_wfi()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_spi_m_slp_wfi | ( | void |  | ) |

Indicate whether turn SPI_M off during WFI/WFE is enabled.

Register | BitsName ---------|-------- CLK_SLP_OFF | SPIM_SLP

Return values

  State | of bit (1 or 0).

Definition at line 3920 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_spi_s_slp_wfi()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_spi_s_slp_wfi | ( | void |  | ) |

Indicate whether turn SPI_S off during WFI/WFE is enabled.

Register | BitsName ---------|-------- CLK_SLP_OFF | SPIS_SLP

Return values

  State | of bit (1 or 0).

Definition at line 3962 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_spim_sclk_low_power()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_spim_sclk_low_power | ( | void |  | ) |

Indicate whether the spim sclk low-power is enabled.

Register | BitsName ---------|-------- CG_LP_EN | SPIM_LP_SCLK

Return values

  State | of bit (1 or 0).

Definition at line 3060 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_spis_sclk_low_power()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_spis_sclk_low_power | ( | void |  | ) |

Indicate whether the spis sclk low-power is enabled.

Register | BitsName ---------|-------- CG_LP_EN | SPIS_LP_SCLK

Return values

  State | of bit (1 or 0).

Definition at line 3102 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_uart0_slp_wfi()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_uart0_slp_wfi | ( | void |  | ) |

Indicate whether turn UART0 off during WFI/WFE is enabled.

Register | BitsName ---------|-------- CLK_SLP_OFF | UART0_SLP

Return values

  State | of bit (1 or 0).

Definition at line 3352 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_uart1_slp_wfi()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_uart1_slp_wfi | ( | void |  | ) |

Indicate whether turn UART1 off during WFI/WFE is enabled.

Register | BitsName ---------|-------- CLK_SLP_OFF | UART1_SLP

Return values

  State | of bit (1 or 0).

Definition at line 3394 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_uart2_slp_wfi()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_uart2_slp_wfi | ( | void |  | ) |

Indicate whether turn UART2 off during WFI/WFE is enabled.

Register | BitsName ---------|-------- CLK_SLP_OFF | UART2_SLP

Return values

  State | of bit (1 or 0).

Definition at line 3434 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_uart3_slp_wfi()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_uart3_slp_wfi | ( | void |  | ) |

Indicate whether turn UART3 off during WFI/WFE is enabled.

Register | BitsName ---------|-------- CLK_SLP_OFF | UART3_SLP

Return values

  State | of bit (1 or 0).

Definition at line 3474 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_uart4_slp_wfi()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_uart4_slp_wfi | ( | void |  | ) |

Indicate whether turn UART4 off during WFI/WFE is enabled.

Register | BitsName ---------|-------- CLK_SLP_OFF | UART4_SLP

Return values

  State | of bit (1 or 0).

Definition at line 3514 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_uart5_slp_wfi()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_uart5_slp_wfi | ( | void |  | ) |

Indicate whether turn UART5 off during WFI/WFE is enabled.

Register | BitsName ---------|-------- CLK_SLP_OFF | UART5_SLP

Return values

  State | of bit (1 or 0).

Definition at line 3554 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_uart_pclk_low_power()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_uart_pclk_low_power | ( | void |  | ) |

Indicate whether the uart pclk low-power is enabled.

Register | BitsName ---------|-------- CG_LP_EN | UART_LP_PCLK

Return values

  State | of bit (1 or 0).

Definition at line 2978 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_uart_sclk_low_power()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_uart_sclk_low_power | ( | void |  | ) |

Indicate whether the uart sclk low-power is enabled.

Register | BitsName ---------|-------- CG_LP_EN | UART_LP_SCLK

Return values

  State | of bit (1 or 0).

Definition at line 2936 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_wfi_off_aes_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_wfi_off_aes_hclk | ( | void |  | ) |

Indicate whether the AES automatic turn off clock is enabled.

Register | BitsName ----------|-------- SECU_CLK_CTRL | AES_HCLK_SLP_OFF

Return values

  State | of bit (1 or 0).

Definition at line 4659 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_wfi_off_aon_mcusub_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_wfi_off_aon_mcusub_hclk | ( | void |  | ) |

Indicate whether the AON_MUCSUB automatic turn off clock is enabled.

Register | BitsName ----------|-------- CG_CTRL_2 | AON_MCUSUB_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 1156 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_wfi_off_apb_sub_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_wfi_off_apb_sub_hclk | ( | void |  | ) |

Indicate whether the APB Subsystem automatic turn off clock is enabled.

Register | BitsName ----------|-------- CG_CTRL_0 | APB_SUB_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 1071 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_wfi_off_ble_brg_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_wfi_off_ble_brg_hclk | ( | void |  | ) |

Indicate whether the BLE Bridge automatic turn off clock is enabled.

Register | BitsName ----------|-------- CG_CTRL_0 | BLE_BRG_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 1029 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_wfi_off_dma_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_wfi_off_dma_hclk | ( | void |  | ) |

Indicate whether the DMA automatic turn off clock is enabled.

Register | BitsName ----------|-------- CG_CTRL_0 | DMA_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 987 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_wfi_off_efuse_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_wfi_off_efuse_hclk | ( | void |  | ) |

Indicate whether the EFUSE automatic turn off clock is enabled.

Register | BitsName ----------|-------- SECU_CLK_CTRL | EFUSE_HCLK_SLP_OFF

Return values

  State | of bit (1 or 0).

Definition at line 4903 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_wfi_off_gpadc_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_wfi_off_gpadc_hclk | ( | void |  | ) |

Indicate whether the GPADC automatic turn off clock is enabled.

Register | BitsName ----------|-------- MCU_MISC_CLK | GPADC_HCLK_SLP_OFF

Return values

  State | of bit (1 or 0).

Definition at line 5009 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_wfi_off_gpio_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_wfi_off_gpio_hclk | ( | void |  | ) |

Indicate whether the GPIO automatic turn off clock is enabled.

Register | BitsName ----------|-------- CG_CTRL_0 | GPIO_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 947 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_wfi_off_hmac_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_wfi_off_hmac_hclk | ( | void |  | ) |

Indicate whether the HMAC automatic turn off clock is enabled.

Register | BitsName ----------|-------- SECU_CLK_CTRL | HMAC_HCLK_SLP_OFF

Return values

  State | of bit (1 or 0).

Definition at line 4699 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_wfi_off_htb_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_wfi_off_htb_hclk | ( | void |  | ) |

Indicate whether the Hopping Table automatic turn off clock is enabled.

Register | BitsName ----------|-------- CG_CTRL_0 | HTB_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 781 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_wfi_off_pkc_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_wfi_off_pkc_hclk | ( | void |  | ) |

Indicate whether the PKC automatic turn off clock is enabled.

Register | BitsName ----------|-------- SECU_CLK_CTRL | PKC_HCLK_SLP_OFF

Return values

  State | of bit (1 or 0).

Definition at line 4739 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_wfi_off_present_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_wfi_off_present_hclk | ( | void |  | ) |

Indicate whether the PRESENT automatic turn off clock is enabled.

Register | BitsName ----------|-------- SECU_CLK_CTRL | PRESENT_HCLK_SLP_OFF

Return values

  State | of bit (1 or 0).

Definition at line 4779 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_wfi_off_pwm_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_wfi_off_pwm_hclk | ( | void |  | ) |

Indicate whether the PWM automatic turn off clock is enabled.

Register | BitsName ----------|-------- CG_CTRL_0 | PWM_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 821 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_wfi_off_ramkey_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_wfi_off_ramkey_hclk | ( | void |  | ) |

Indicate whether the RAMKEY automatic turn off clock is enabled.

Register | BitsName ----------|-------- SECU_CLK_CTRL | RAMKEY_HCLK_SLP_OFF

Return values

  State | of bit (1 or 0).

Definition at line 4819 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_wfi_off_rng_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_wfi_off_rng_hclk | ( | void |  | ) |

Indicate whether the RNG automatic turn off clock is enabled.

Register | BitsName ----------|-------- SECU_CLK_CTRL | RNG_HCLK_SLP_OFF

Return values

  State | of bit (1 or 0).

Definition at line 4861 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_wfi_off_rom_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_wfi_off_rom_hclk | ( | void |  | ) |

Indicate whether the ROM automatic turn off clock is enabled.

Register | BitsName ----------|-------- CG_CTRL_0 | ROM_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 863 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_wfi_off_secu_div4_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_wfi_off_secu_div4_hclk | ( | void |  | ) |

Indicate whether the security blocks automatic turn off div4 clock is enabled.

Register | BitsName ----------|-------- PERIPH_GC | SECU_DIV4_PCLK

Return values

  State | of bit (1 or 0).

Definition at line 1281 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_wfi_off_secu_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_wfi_off_secu_hclk | ( | void |  | ) |

Indicate whether the security blocks(including AES, PKC, Present, HMAC) automatic turn off clock is enabled.

Register | BitsName ----------|-------- CG_CTRL_0 | SECU_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 699 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_wfi_off_serial_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_wfi_off_serial_hclk | ( | void |  | ) |

Indicate whether the serial blocks(including I2C, UART, QSPI, I2S, SPI) automatic turn off clock is enabled.

Register | BitsName ----------|-------- CG_CTRL_0 | SERIAL_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 1114 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_wfi_off_sim_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_wfi_off_sim_hclk | ( | void |  | ) |

Indicate whether the SIM automatic turn off clock is enabled.

Register | BitsName ----------|-------- CG_CTRL_0 | SIM_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 739 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_wfi_off_snsadc_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_wfi_off_snsadc_hclk | ( | void |  | ) |

Indicate whether the SNSADC automatic turn off clock is enabled.

Register | BitsName ----------|-------- CG_CTRL_0 | SNSADC_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 905 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_wfi_off_sram_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_wfi_off_sram_hclk | ( | void |  | ) |

Indicate whether the SRAM automatic turn off clock is enabled.

Register | BitsName ----------|-------- CG_CTRL_2 | SRAM_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 1240 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_is_enabled_wfi_off_xqspi_div4_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_wfi_off_xqspi_div4_hclk | ( | void |  | ) |

Indicate whether the XQSPI automatic turn off div4 clock is enabled.

Register | BitsName ----------|-------- PERIPH_GC | XQSPI_DIV4_PCLK

Return values

  State | of bit (1 or 0).

Definition at line 1321 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_is_enabled_wfi_off_xqspi_hclk()

__STATIC_INLINE uint32_t ll_cgc_is_enabled_wfi_off_xqspi_hclk | ( | void |  | ) |

Indicate whether the XQSPI automatic turn off clock is enabled.

Register | BitsName ----------|-------- CG_CTRL_2 | XF_XQSPI_HCLK

Return values

  State | of bit (1 or 0).

Definition at line 1198 of file gr533x_ll_cgc.h.

References BIT_SEGMENT_VALUE, and CGC_CLOCK_ENABLE.

## ◆ ll_cgc_set_force_off_hclk_0()

__STATIC_INLINE void ll_cgc_set_force_off_hclk_0 | ( | uint32_t | clk_mask | ) |

Some peripherals force turn off clock. (Include: Security/SIM/HTB/PWM/ROM/SNSADC/GPIO/ DMA/BLE_BRG/APB_SUB/SERIAL/I2S)

Register | BitsName ----------|-------- CG_CTRL_1 | SECU_HCLK CG_CTRL_1 | SIM_HCLK CG_CTRL_1 | HTB_HCLK CG_CTRL_1 | ROM_HCLK CG_CTRL_1 | SNSADC_HCLK CG_CTRL_1 | GPIO_HCLK CG_CTRL_1 | DMA_HCLK CG_CTRL_1 | BLE_BRG_HCLK CG_CTRL_1 | APB_SUB_HCLK CG_CTRL_1 | SERIAL_HCLK

Parameters

  clk_mask | This parameter can be a combination of the following values: LL_CGC_FRC_SECU_HCLK LL_CGC_FRC_HTB_HCLK LL_CGC_FRC_ROM_HCLK LL_CGC_FRC_SNSADC_HCLK LL_CGC_FRC_GPIO_HCLK LL_CGC_FRC_SERIAL_HCLK

Return values

  None |

Definition at line 487 of file gr533x_ll_cgc.h.

References LL_CGC_FRC_ALL_HCLK0.

## ◆ ll_cgc_set_force_off_hclk_1()

__STATIC_INLINE void ll_cgc_set_force_off_hclk_1 | ( | uint32_t | clk_mask | ) |

Some peripherals force turn off clock. (Include: AON_MCUSUB/XF_XQSPI/SRAM)

Register | BitsName ----------|-------- CG_CTRL_2 | AON_MCUSUB_HCLK CG_CTRL_2 | XF_XQSPI_HCLK CG_CTRL_2 | SRAM_HCLK

Parameters

  clk_mask | This parameter can be a combination of the following values: LL_CGC_FRC_XF_XQSPI_HCLK LL_CGC_FRC_SRAM_HCLK

Return values

  None |

Definition at line 538 of file gr533x_ll_cgc.h.

References LL_CGC_FRC_ALL_HCLK1.

## ◆ ll_cgc_set_force_off_hclk_2()

__STATIC_INLINE void ll_cgc_set_force_off_hclk_2 | ( | uint32_t | clk_mask | ) |

Some peripherals force turn off clock. (Include: UART0_HCLK/UART1_HCLK/UART2_HCLK/UART3_HCLK/UART4_HCLK/UART5_HCLK/ I2C0_HCLK/I2C1_HCLK/SPIM_HCLK/SPIS_HCLK/QSPI0_HCLK/QSPI1_HCLK/I2S_HCLK/SECU_DIV4_PCLK/XQSPI_DIV4_PCLK/PWM0/PWM1)

Register | BitsName ----------|-------- PERIPH_GC | UART0_HCLK PERIPH_GC | UART1_HCLK PERIPH_GC | I2C0_HCLK PERIPH_GC | I2C1_HCLK PERIPH_GC | SPIM_HCLK PERIPH_GC | SPIS_HCLK PERIPH_GC | XQSPI_DIV4_PCLK PERIPH_GC | PWM0_HCLK PERIPH_GC | PWM1_HCLK

Parameters

  clk_mask | This parameter can be a combination of the following values: LL_CGC_FRC_UART0_PCLK LL_CGC_FRC_UART1_PCLK LL_CGC_FRC_I2C0_PCLK LL_CGC_FRC_I2C1_PCLK LL_CGC_FRC_SPI_M_PCLK LL_CGC_FRC_SPI_S_PCLK LL_CGC_FRC_SERIALS_HCLK2 LL_CGC_FRC_PWM_0_PCLK LL_CGC_FRC_PWM_1_PCLK

Return values

  None |

Definition at line 589 of file gr533x_ll_cgc.h.

References LL_CGC_FRC_ALL_HCLK2.

## ◆ ll_cgc_set_force_off_hclk_3()

__STATIC_INLINE void ll_cgc_set_force_off_hclk_3 | ( | uint32_t | clk_mask | ) |

Some peripherals automatic turn off clock. (Include: AES/HMAC/PKC/RNG.etc)

Register | BitsName ----------|-------- PERIPH_GC | AES/HMAC/PKC/RNG/EFUSE

Parameters

  clk_mask | This parameter can be a combination of the following values: LL_CGC_MCU_FRC_RNG_HCLK_OFF_EN ..... LL_CGC_MCU_SLP_EFUSE_HCLK_OFF_EN

Return values

  None |

Definition at line 640 of file gr533x_ll_cgc.h.

References LL_CGC_MCU_SECU_FRC_OFF_HCLK.

## ◆ ll_cgc_set_force_off_hclk_secu()

__STATIC_INLINE void ll_cgc_set_force_off_hclk_secu | ( | uint32_t | clk_mask | ) |

Individual block's clock control inside security system which was forced to turn off (Include: AES/HMAC/PKC/PRESENT/RAMKAY/RNG/EFUSE)

Register | BitsName ----------|-------- SECU_CLK_CTRL | AES_HCLK_FRC_OFF SECU_CLK_CTRL | HMAC_HCLK_FRC_OFF SECU_CLK_CTRL | PKC_HCLK_FRC_OFF SECU_CLK_CTRL | PRESENT_HCLK_FRC_OFF SECU_CLK_CTRL | RAMKEY_HCLK_FRC_OFF SECU_CLK_CTRL | RNG_HCLK_FRC_OFF SECU_CLK_CTRL | EFUSE_HCLK_FRC_OFF

Parameters

  clk_mask | This parameter can be a combination of the following values: LL_CGC_MCU_FRC_RNG_HCLK_OFF_EN LL_CGC_MCU_FRC_EFUSE_HCLK_OFF_EN

Return values

  None |

Definition at line 4269 of file gr533x_ll_cgc.h.

References LL_CGC_MCU_SECU_FRC_OFF_HCLK.

## ◆ ll_cgc_set_mcu_periph_low_power()

__STATIC_INLINE void ll_cgc_set_mcu_periph_low_power | ( | uint32_t | clk_mask | ) |

Some peripherals has low power feature. (Include: UART/I2S/SPIM/SPIS/I2C/AHB BUS)

Register | BitsName ---------|-------- CG_LP_EN | UART_LP_SCLK CG_LP_EN | UART_LP_PCLK CG_LP_EN | I2S_LP CG_LP_EN | SPIM_LP_SCLK CG_LP_EN | SPIS_LP_SCLK CG_LP_EN | I2C_LP_SCLK CG_LP_EN | AHB_BUS_LP

Parameters

  clk_mask | This parameter can be a combination of the following values: LL_CGC_MCU_PERIPH_CG_LP_EN_AHB2APB_EN LL_CGC_MCU_PERIPH_CG_LP_EN_AHB2APB_SYNC_EN LL_CGC_MCU_PERIPH_CG_LP_EN_AHB_BUS_LP_EN LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_LP_SCLK_EN LL_CGC_MCU_PERIPH_CG_LP_EN_SPIS_LP_SCLK_EN LL_CGC_MCU_PERIPH_CG_LP_EN_SPIM_LP_SCLK_EN LL_CGC_MCU_PERIPH_CG_LP_EN_UART_LP_PCLK_EN LL_CGC_MCU_PERIPH_CG_LP_EN_UART_LP_SCLK_EN

Return values

  None |

Definition at line 2866 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_set_misc_clk()

__STATIC_INLINE void ll_cgc_set_misc_clk | ( | uint32_t | clk_mask | ) |

Some MISC_CLK blocks turn off clock. (Include: GPADC/XQSPI/DMA0)

Register | BitsName ----------|-------- MCU_MISC_CLK | GPADC/XQSPI/DMA0

Return values

  None |

Definition at line 4917 of file gr533x_ll_cgc.h.

References LL_CGC_MCU_MISC_CLK.

## ◆ ll_cgc_set_slp_off_hclk_secu()

__STATIC_INLINE void ll_cgc_set_slp_off_hclk_secu | ( | uint32_t | clk_mask | ) |

Some security blocks automatic turn off clock during WFI/WFE. (Include: AES/HMAC/PKC/PRESENT/RAMKAY/RNG/EFUSE)

Register | BitsName ----------|-------- SECU_CLK_CTRL | AES_HCLK_SLP_OFF SECU_CLK_CTRL | HMAC_HCLK_SLP_OFF SECU_CLK_CTRL | PKC_HCLK_SLP_OFF SECU_CLK_CTRL | PRESENT_HCLK_SLP_OFF

Parameters

  clk_mask | This parameter can be a combination of the following values: LL_CGC_MCU_FRC_RNG_HCLK_OFF_EN LL_CGC_MCU_SLP_RNG_HCLK_OFF_EN LL_CGC_MCU_FRC_EFUSE_HCLK_OFF_EN LL_CGC_MCU_SLP_EFUSE_HCLK_OFF_EN

Return values

  None |

Definition at line 4313 of file gr533x_ll_cgc.h.

References LL_CGC_MCU_SECU_FRC_OFF_WFI_HCLK.

## ◆ ll_cgc_set_wfi_off_hclk_0()

__STATIC_INLINE void ll_cgc_set_wfi_off_hclk_0 | ( | uint32_t | clk_mask | ) |

Some peripherals automatic turn off clock during WFI. (Include: Security/SIM/HTB/PWM/ ROM/SNSADC/GPIO/DMA/BLE_BRG/APB_SUB/SERIAL/I2S)

Register | BitsName ----------|-------- CG_CTRL_0 | SECU_HCLK CG_CTRL_0 | SIM_HCLK CG_CTRL_0 | HTB_HCLK CG_CTRL_0 | PWM_HCLK CG_CTRL_0 | ROM_HCLK CG_CTRL_0 | SNSADC_HCLK CG_CTRL_0 | GPIO_HCLK CG_CTRL_0 | DMA_HCLK CG_CTRL_0 | BLE_BRG_HCLK CG_CTRL_0 | APB_SUB_HCLK CG_CTRL_0 | SERIAL_HCLK

Parameters

  clk_mask | This parameter can be a combination of the following values: LL_CGC_WFI_SECU_HCLK LL_CGC_WFI_HTB_HCLK LL_CGC_WFI_ROM_HCLK LL_CGC_WFI_SNSADC_HCLK LL_CGC_WFI_GPIO_HCLK LL_CGC_WFI_BLE_BRG_HCLK LL_CGC_WFI_APB_SUB_HCLK LL_CGC_WFI_SERIAL_HCLK

Return values

  None |

Definition at line 280 of file gr533x_ll_cgc.h.

References LL_CGC_WFI_ALL_HCLK0.

## ◆ ll_cgc_set_wfi_off_hclk_1()

__STATIC_INLINE void ll_cgc_set_wfi_off_hclk_1 | ( | uint32_t | clk_mask | ) |

Some peripherals automatic turn off clock during WFI. (Include: AON_MCUSUB/XF_XQSPI/SRAM)

Register | BitsName ----------|-------- CG_CTRL_2 | AON_MCUSUB_HCLK CG_CTRL_2 | XF_XQSPI_HCLK CG_CTRL_2 | SRAM_HCLK

Parameters

  clk_mask | This parameter can be a combination of the following values: LL_CGC_WFI_AON_MCUSUB_HCLK LL_CGC_WFI_XF_XQSPI_HCLK LL_CGC_WFI_SRAM_HCLK

Return values

  None |

Definition at line 333 of file gr533x_ll_cgc.h.

References LL_CGC_WFI_ALL_HCLK1.

## ◆ ll_cgc_set_wfi_off_hclk_2()

__STATIC_INLINE void ll_cgc_set_wfi_off_hclk_2 | ( | uint32_t | clk_mask | ) |

Some peripherals automatic turn off clock during WFI. (Include: SECU_DIV4/XQSPI_DIV4)

Register | BitsName ----------|-------- PERIPH_GC | SECU_DIV4_PCLK PERIPH_GC | XQSPI_DIV4_PCLK

Parameters

  clk_mask | This parameter can be a combination of the following values:

Return values

  None |

Definition at line 368 of file gr533x_ll_cgc.h.

## ◆ ll_cgc_set_wfi_off_hclk_3()

__STATIC_INLINE void ll_cgc_set_wfi_off_hclk_3 | ( | uint32_t | clk_mask | ) |

Some peripherals automatic turn off clock during WFI. (Include: UART/DSPI.I2C/QSPI.etc)

Register | BitsName ----------|-------- PERIPH_GC | UART0 - UART5/I2C0 - I2C5 PERIPH_GC | I2SM/I2SS/SPIM/SPIS/PWM0/PWM1//QSPIM0/QSPIM1/QSPIM2/DSPI/PDM

Parameters

  clk_mask | This parameter can be a combination of the following values: LL_CGC_MCU_PERIPH_CG_LP_EN_UART_0_SLP_OFF LL_CGC_MCU_PERIPH_CG_LP_EN_UART_1_SLP_OFF ..... LL_CGC_MCU_PERIPH_CG_LP_EN_I2C_1_SLP_OFF

Return values

  None |

Definition at line 402 of file gr533x_ll_cgc.h.

References LL_CGC_MCU_PERIPH_SERIALS_SLP_ALL.

## ◆ ll_cgc_set_wfi_off_hclk_4()

__STATIC_INLINE void ll_cgc_set_wfi_off_hclk_4 | ( | uint32_t | clk_mask | ) |

Some peripherals automatic turn off clock during WFI. (Include: AES/HMAC/PKC/RNG.etc)

Register | BitsName ----------|-------- PERIPH_GC | AES/HMAC/PKC/RNG/EFUSE

Parameters

  clk_mask | This parameter can be a combination of the following values: LL_CGC_MCU_FRC_RNG_HCLK_OFF_EN ..... LL_CGC_MCU_SLP_EFUSE_HCLK_OFF_EN

Return values

  None |

Definition at line 439 of file gr533x_ll_cgc.h.

References LL_CGC_MCU_SECU_FRC_OFF_WFI_HCLK.