### - p -

- PACK_INT : ble_iso.h
- PACK_SEQ : ble_iso.h
- PACKAGE_NONE : gr533x_sys_sdk.h
- PACKAGE_QFN32 : gr533x_sys_sdk.h
- PACKAGE_QFN48 : gr533x_sys_sdk.h
- PARAM_ID_ACTCLK_DRIFT : nvds_tag.h
- PARAM_ID_ACTIVITY_MOVE_CONFIG : nvds_tag.h
- PARAM_ID_BD_ADDRESS : nvds_tag.h
- PARAM_ID_CH_ASS_EN : nvds_tag.h
- PARAM_ID_DEVICE_NAME : nvds_tag.h
- PARAM_ID_DFT_SLAVE_MD : nvds_tag.h
- PARAM_ID_DIAG_BLE_HW : nvds_tag.h
- PARAM_ID_DIAG_DM_HW : nvds_tag.h
- PARAM_ID_DIAG_PLF : nvds_tag.h
- PARAM_ID_DIAG_SW : nvds_tag.h
- PARAM_ID_GDX_ADV_INT : nvds_tag.h
- PARAM_ID_LE_CODED_PHY_500 : nvds_tag.h
- PARAM_ID_LE_DBG_FIXED_P256_KEY : nvds_tag.h
- PARAM_ID_LE_PRIVATE_KEY_P256 : nvds_tag.h
- PARAM_ID_LPCLK_DRIFT : nvds_tag.h
- PARAM_ID_RF_BTIPT_GAIN_SETTING : nvds_tag.h
- PARAM_ID_RF_BTIPT_VERSION : nvds_tag.h
- PARAM_ID_RF_BTIPT_XO_SETTING : nvds_tag.h
- PARAM_ID_RF_XO_OFFSET : nvds_tag.h
- PARAM_ID_RSSI_HIGH_THR : nvds_tag.h
- PARAM_ID_RSSI_INTERF_THR : nvds_tag.h
- PARAM_ID_RSSI_LOW_THR : nvds_tag.h
- PARAM_ID_SCAN_EXT_ADV : nvds_tag.h
- PARAM_ID_SCHED_SCAN_DUR : nvds_tag.h
- PARAM_ID_TRACER_CONFIG : nvds_tag.h
- PASS_C_CTRL_PT_CANCEL_SLIENT_MODE : pass_c.h
- PASS_C_CTRL_PT_MUTE_ONCE : pass_c.h
- PASS_C_CTRL_PT_SILENT_MODE : pass_c.h
- PASS_C_EVT_ALERT_STATUS_NTF_SET_SUCCESS : pass_c.h
- PASS_C_EVT_ALERT_STATUS_RECEIVE : pass_c.h
- PASS_C_EVT_CTRL_POINT_SET_SUCCESS : pass_c.h
- PASS_C_EVT_DISCOVERY_COMPLETE : pass_c.h
- PASS_C_EVT_DISCOVERY_FAIL : pass_c.h
- PASS_C_EVT_INVALID : pass_c.h
- PASS_C_EVT_RINGER_SET_NTF_SET_SUCCESS : pass_c.h
- PASS_C_EVT_RINGER_SET_RECEIVE : pass_c.h
- PASS_C_EVT_WRITE_OP_ERR : pass_c.h
- PASS_CTRL_PT_CANCEL_SLIENT_MODE : pass.h
- PASS_CTRL_PT_MUTE_ONCE : pass.h
- PASS_CTRL_PT_SILENT_MODE : pass.h
- PASS_EVT_ALERT_STATUS_NTF_DISABLE : pass.h
- PASS_EVT_ALERT_STATUS_NTF_ENABLE : pass.h
- PASS_EVT_INVALID : pass.h
- PASS_EVT_MUTE_ONCE_SET : pass.h
- PASS_EVT_RINGER_SET_NTF_DISABLE : pass.h
- PASS_EVT_RINGER_SET_NTF_ENABLE : pass.h
- PASS_EVT_SILENT_MODE_CANCEL : pass.h
- PASS_EVT_SILENT_MODE_SET : pass.h
- PCS_EVT_DISCONNECTED : pcs.h
- PCS_EVT_INVALID : pcs.h
- PCS_EVT_PARAM_SET : pcs.h
- PCS_EVT_SETTING_DISABLE : pcs.h
- PCS_EVT_SETTING_ENABLE : pcs.h
- PCS_EVT_TX_DATA_SENT : pcs.h
- PCS_EVT_TX_DISABLE : pcs.h
- PCS_EVT_TX_ENABLE : pcs.h
- PCS_SETTING_TYPE_ADV_DATA : pcs.h
- PCS_SETTING_TYPE_ADV_INTERVAL : pcs.h
- PCS_SETTING_TYPE_CONN_PARAM : pcs.h
- PCS_SETTING_TYPE_PHY : pcs.h
- PCS_SETTING_TYPE_TX_POWER : pcs.h
- PERIPH_DEVICE_NUM_AES : gr533x_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_CLK_CALIB : gr533x_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_DMA0 : gr533x_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_I2C0 : gr533x_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_I2C1 : gr533x_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_PWM0 : gr533x_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_PWM1 : gr533x_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_RNG : gr533x_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_SNSADC : gr533x_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_SPIM : gr533x_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_SPIS : gr533x_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_UART0 : gr533x_hal_pwr_mgmt.h
- PERIPH_DEVICE_NUM_UART1 : gr533x_hal_pwr_mgmt.h
- PMR_BB_FRAME_ONGOING : gr533x_pwr.h
- PMR_BLE_ACTIVE_MODE : gr533x_pwr.h
- PMR_BT_ACTIVE_MODE : gr533x_pwr.h
- PMR_CRYPT_ONGOING : gr533x_pwr.h
- PMR_CSB_NOT_LPO_ALLOWED : gr533x_pwr.h
- PMR_DEEP_SLEEP : gr533x_pwr.h
- PMR_HOP_CALC_ONGOING : gr533x_pwr.h
- PMR_MGMT_ACTIVE_MODE : gr533x_pwr.h
- PMR_MGMT_IDLE_MODE : gr533x_pwr.h
- PMR_MGMT_SLEEP_MODE : gr533x_pwr.h
- PMR_MWS_WLAN_EVENT_GENERATOR_ACTIVE : gr533x_pwr.h
- PMR_PLF_DEEP_SLEEP_DISABLED : gr533x_pwr.h
- PMR_TL_RX_ONGOING : gr533x_pwr.h
- PMR_TL_TX_ONGOING : gr533x_pwr.h
- PMR_WAKE_UP_ONGOING : gr533x_pwr.h
- PRF_CLI_START_IND : ble_prf_types.h
- PRF_CLI_START_NTF : ble_prf_types.h
- PRF_CLI_STOP_NTFIND : ble_prf_types.h
- PUBLIC : ble_iso.h
- PWM_BREATH_MODE : gr533x_hal_pwm.h
- PWM_CODING_MODE : gr533x_hal_pwm.h
- PWM_FLICKER_MODE : gr533x_hal_pwm.h
- PWM_PWR_ID : app_pwr_mgmt.h
- PWR_ID_MAX : app_pwr_mgmt.h