Public Attributes | List of all members
_ll_pwm_init_t Struct Reference
Peripheral Driver » LL Driver » PWM » Structures » PWM Exported init structures

LL PWM init Structure definition. More...

`#include <gr533x_ll_pwm.h>`

## Public Attributes
ll_pwm_mode_t | ll_mode
uint32_t | ll_prd_cycles
ll_pwm_none_coding_mode_init_t | none_coding_mode_cfg
ll_pwm_coding_mode_init_t | coding_mode_cfg

## Detailed Description

LL PWM init Structure definition.

Definition at line 196 of file gr533x_ll_pwm.h.

## Member Data Documentation

## ◆ coding_mode_cfg

ll_pwm_coding_mode_init_t _ll_pwm_init_t::coding_mode_cfg

Specifies the coding mode config. This parameter can be a value of ll_pwm_coding_mode_init_t.

Definition at line 209 of file gr533x_ll_pwm.h.

## ◆ ll_mode

ll_pwm_mode_t _ll_pwm_init_t::ll_mode

Specifies the PWM output mode. This parameter can be a value of PWM_LL_EC_MODE.

This feature can be modified afterwards using unitary function ll_pwm_set_mode().

Definition at line 198 of file gr533x_ll_pwm.h.

## ◆ ll_prd_cycles

uint32_t _ll_pwm_init_t::ll_prd_cycles

Specifies the number of period cycle in Flicker mode or Coding mode. This parameter control the number of period cycles, when set to 0 will continuously generate waveform.

Definition at line 203 of file gr533x_ll_pwm.h.

## ◆ none_coding_mode_cfg

ll_pwm_none_coding_mode_init_t _ll_pwm_init_t::none_coding_mode_cfg

Specifies the none coding mode config. This parameter can be a value of ll_pwm_none_coding_mode_init_t.

Definition at line 206 of file gr533x_ll_pwm.h.

The documentation for this struct was generated from the following file:

- gr533x_ll_pwm.h