Public Attributes | List of all members
ble_gap_evt_data_length_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

Data Length Updated event for BLE_GAPC_EVT_DATA_LENGTH_UPDATED. More...

`#include <ble_gapc.h>`

## Public Attributes
uint16_t | max_tx_octets
uint16_t | max_tx_time
uint16_t | max_rx_octets
uint16_t | max_rx_time

## Detailed Description

Data Length Updated event for BLE_GAPC_EVT_DATA_LENGTH_UPDATED.

Definition at line 881 of file ble_gapc.h.

## Member Data Documentation

## ◆ max_rx_octets

uint16_t ble_gap_evt_data_length_t::max_rx_octets

The maximum number of payload octets in RX.

Definition at line 885 of file ble_gapc.h.

## ◆ max_rx_time

uint16_t ble_gap_evt_data_length_t::max_rx_time

The maximum time that the local Controller will take to RX.

Definition at line 886 of file ble_gapc.h.

## ◆ max_tx_octets

uint16_t ble_gap_evt_data_length_t::max_tx_octets

The maximum number of payload octets in TX.

Definition at line 883 of file ble_gapc.h.

## ◆ max_tx_time

uint16_t ble_gap_evt_data_length_t::max_tx_time

The maximum time that the local Controller will take to TX.

Definition at line 884 of file ble_gapc.h.

The documentation for this struct was generated from the following file:

- ble_gapc.h