Functions
IRQ Handler and Callbacks
Peripheral Driver » HAL Driver » AON_GPIO » Functions

IRQ Handler and Callbacks functions. More...

## Functions
void | hal_aon_gpio_irq_handler (void)
| Handle AON_GPIO interrupt request. More...
void | hal_aon_gpio_callback (uint16_t aon_gpio_pin)
| AON GPIO pin detection callback. More...

## Detailed Description

IRQ Handler and Callbacks functions.

## Function Documentation

## ◆ hal_aon_gpio_callback()

void hal_aon_gpio_callback | ( | uint16_t | aon_gpio_pin | ) |

AON GPIO pin detection callback.

Note
  This function should not be modified. When the callback is needed, the hal_aon_gpio_callback can be implemented in the user file.

Parameters

  [in] | aon_gpio_pin | Indicate the port pin whose interrupt was triggered. This parameter can be a combination of the following values: AON_GPIO_PIN_0 AON_GPIO_PIN_1 AON_GPIO_PIN_2 AON_GPIO_PIN_3 AON_GPIO_PIN_4 AON_GPIO_PIN_5 AON_GPIO_PIN_ALL

## ◆ hal_aon_gpio_irq_handler()

void hal_aon_gpio_irq_handler | ( | void |  | ) |

Handle AON_GPIO interrupt request.