Enumerations
Enumerations
Peripheral Driver » HAL Driver » PWR_MGMT

## Enumerations
enum | periph_device_number_t { PERIPH_DEVICE_NUM_SPIM = 0, PERIPH_DEVICE_NUM_SPIS, PERIPH_DEVICE_NUM_I2C0, PERIPH_DEVICE_NUM_I2C1, PERIPH_DEVICE_NUM_UART0, PERIPH_DEVICE_NUM_UART1, PERIPH_DEVICE_NUM_PWM0, PERIPH_DEVICE_NUM_PWM1, PERIPH_DEVICE_NUM_DMA0, PERIPH_DEVICE_NUM_AES, PERIPH_DEVICE_NUM_RNG, PERIPH_DEVICE_NUM_SNSADC, PERIPH_DEVICE_NUM_CLK_CALIB, MAX_PERIPH_DEVICE_NUM }
| Peripheral Device ID definition. More...
enum | periph_state_t { IDLE = 0, ACTIVE }
| Peripheral Device State definition. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ periph_device_number_t

enum periph_device_number_t

Peripheral Device ID definition.

Enumerator
PERIPH_DEVICE_NUM_SPIM |
PERIPH_DEVICE_NUM_SPIS |
PERIPH_DEVICE_NUM_I2C0 |
PERIPH_DEVICE_NUM_I2C1 |
PERIPH_DEVICE_NUM_UART0 |
PERIPH_DEVICE_NUM_UART1 |
PERIPH_DEVICE_NUM_PWM0 |
PERIPH_DEVICE_NUM_PWM1 |
PERIPH_DEVICE_NUM_DMA0 |
PERIPH_DEVICE_NUM_AES |
PERIPH_DEVICE_NUM_RNG |
PERIPH_DEVICE_NUM_SNSADC |
PERIPH_DEVICE_NUM_CLK_CALIB |
MAX_PERIPH_DEVICE_NUM |

Definition at line 75 of file gr533x_hal_pwr_mgmt.h.

## ◆ periph_state_t

enum periph_state_t

Peripheral Device State definition.

Enumerator
IDLE |
ACTIVE |

Definition at line 96 of file gr533x_hal_pwr_mgmt.h.