Modules | Macros
XQSPI Exported Constants
Peripheral Driver » HAL Driver » XQSPI » Defines

## Modules
| XQSPI Error Code
| XQSPI in XIP mode
| XQSPI Work Mode
| XQSPI Cache Mode in XIP mode
| XQSPI in XIP mode
| XQSPI in XIP mode
| XQSPI Read Command in XIP mode
| XQSPI Clock Mode
| XQSPI Clock Speed
| XQSPI Data Mode, only in QSPI mode
| XQSPI FIFO Threshold, FIFO depth is 64*4bytes, only in QSPI mode
| XQSPI Instruction Size, only in QSPI mode
| XQSPI Address Size, only in QSPI mode
| XQSPI Instruction and Address Mode, only in QSPI mode
| XQSPI Flags, only in QSPI mode
| Control Present Status, only in XIP mode

## Macros
#define | HAL_XQSPI_RETRY_DEFAULT_VALUE ((uint32_t)1000)
| XQSPI_Retry_definition XQSPI Retry definition. More...

## Detailed Description

## Macro Definition Documentation

## ◆ HAL_XQSPI_RETRY_DEFAULT_VALUE

#define HAL_XQSPI_RETRY_DEFAULT_VALUE ((uint32_t)1000)

XQSPI_Retry_definition XQSPI Retry definition.

1000 times

Definition at line 382 of file gr533x_hal_xqspi.h.