Macros
Defines
Peripheral Driver » APP DRIVER » RTOS CONFIG

## Macros
#define | SEM_WAIT_FOREVER (0xFFFFUL)
#define | SEM_NO_WAIT (0)
#define | MUTEX_WAIT_FOREVER (0xFFFFUL)
#define | MUTEX_NO_WAIT (0)
#define | APP_DRV_SEM_DECL(sem) sem_t sem
#define | APP_DRV_MUTEX_DECL(mutex) mutex_t mutex
#define | APP_DRV_SEM_STATIC(sem) static APP_DRV_SEM_DECL(sem)
#define | APP_DRV_MUTEX_STATIC(mutex) static APP_DRV_MUTEX_DECL(mutex)
#define | app_driver_sem_init(x) (0)
#define | app_driver_sem_deinit(x)
#define | app_driver_sem_pend(x, y) (0)
#define | app_driver_sem_post(x)
#define | app_driver_sem_post_from_isr(x)
#define | app_driver_mutex_init(x) (0)
#define | app_driver_mutex_deinit(x)
#define | app_driver_mutex_pend(x, y)
#define | app_driver_mutex_post(x)

## Detailed Description

## Macro Definition Documentation

## ◆ app_driver_mutex_deinit

#define app_driver_mutex_deinit | ( |  | x | ) |

Deinitialize the mutex.

Definition at line 270 of file app_rtos_cfg.h.

## ◆ app_driver_mutex_init

#define app_driver_mutex_init | ( |  | x | ) | (0)

Initialize the mutex.

Definition at line 269 of file app_rtos_cfg.h.

## ◆ app_driver_mutex_pend

#define app_driver_mutex_pend | ( |  | x,
|  |  | y
| ) |  |

Pend the mutex.

Definition at line 271 of file app_rtos_cfg.h.

## ◆ app_driver_mutex_post

#define app_driver_mutex_post | ( |  | x | ) |

Post the mutex.

Definition at line 272 of file app_rtos_cfg.h.

## ◆ app_driver_sem_deinit

#define app_driver_sem_deinit | ( |  | x | ) |

Deinitialize the semaphore.

Definition at line 264 of file app_rtos_cfg.h.

## ◆ app_driver_sem_init

#define app_driver_sem_init | ( |  | x | ) | (0)

Initialize the semaphore.

Definition at line 263 of file app_rtos_cfg.h.

## ◆ app_driver_sem_pend

#define app_driver_sem_pend | ( |  | x,
|  |  | y
| ) |  | (0)

Pend the semaphore.

Definition at line 265 of file app_rtos_cfg.h.

## ◆ app_driver_sem_post

#define app_driver_sem_post | ( |  | x | ) |

Post the semaphore.

Definition at line 266 of file app_rtos_cfg.h.

## ◆ app_driver_sem_post_from_isr

#define app_driver_sem_post_from_isr | ( |  | x | ) |

Post the semaphore from interrupt.

Definition at line 267 of file app_rtos_cfg.h.

## ◆ APP_DRV_MUTEX_DECL

#define APP_DRV_MUTEX_DECL | ( |  | mutex | ) | mutex_t mutex

Define a mutex instance

Definition at line 135 of file app_rtos_cfg.h.

## ◆ APP_DRV_MUTEX_STATIC

#define APP_DRV_MUTEX_STATIC | ( |  | mutex | ) | static APP_DRV_MUTEX_DECL(mutex)

Define a static mutex instance

Definition at line 138 of file app_rtos_cfg.h.

## ◆ APP_DRV_SEM_DECL

#define APP_DRV_SEM_DECL | ( |  | sem | ) | sem_t sem

Define a semaphore instance

Definition at line 134 of file app_rtos_cfg.h.

## ◆ APP_DRV_SEM_STATIC

#define APP_DRV_SEM_STATIC | ( |  | sem | ) | static APP_DRV_SEM_DECL(sem)

Define a static semaphore instance

Definition at line 137 of file app_rtos_cfg.h.

## ◆ MUTEX_NO_WAIT

#define MUTEX_NO_WAIT (0)

Non-block

Definition at line 126 of file app_rtos_cfg.h.

## ◆ MUTEX_WAIT_FOREVER

#define MUTEX_WAIT_FOREVER (0xFFFFUL)

Wait for the mutex forever

Definition at line 125 of file app_rtos_cfg.h.

## ◆ SEM_NO_WAIT

#define SEM_NO_WAIT (0)

Non-block

Definition at line 123 of file app_rtos_cfg.h.

## ◆ SEM_WAIT_FOREVER

#define SEM_WAIT_FOREVER (0xFFFFUL)

Wait for the semaphore forever.

Definition at line 122 of file app_rtos_cfg.h.