Macros
IT Defines
Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants

Interrupt definitions which can be used with LL_SPI_ReadReg and LL_SPI_WriteReg functions. More...

## Macros
#define | LL_SPI_IM_MST SPI_INT_MASK_MULTI_M_CIM
#define | LL_SPI_IM_RXF SPI_INT_MASK_RX_FIFO_FIM
#define | LL_SPI_IM_RXO SPI_INT_MASK_RX_FIFO_OIM
#define | LL_SPI_IM_RXU SPI_INT_MASK_RX_FIFO_UIM
#define | LL_SPI_IM_TXO SPI_INT_MASK_TX_FIFO_OIM
#define | LL_SPI_IM_TXE SPI_INT_MASK_TX_FIFO_EIM
#define | LL_SPI_IS_MST SPI_INT_STAT_MULTI_M_CIS
#define | LL_SPI_IS_RXF SPI_INT_STAT_RX_FIFO_FIS
#define | LL_SPI_IS_RXO SPI_INT_STAT_RX_FIFO_OIS
#define | LL_SPI_IS_RXU SPI_INT_STAT_RX_FIFO_UIS
#define | LL_SPI_IS_TXO SPI_INT_STAT_TX_FIFO_OIS
#define | LL_SPI_IS_TXE SPI_INT_STAT_TX_FIFO_EIS
#define | LL_SPI_RIS_MST SPI_RAW_INT_STAT_MULTI_M_CRIS
#define | LL_SPI_RIS_RXF SPI_RAW_INT_STAT_RX_FIFO_FRIS
#define | LL_SPI_RIS_RXO SPI_RAW_INT_STAT_RX_FIFO_ORIS
#define | LL_SPI_RIS_RXU SPI_RAW_INT_STAT_RX_FIFO_URIS
#define | LL_SPI_RIS_TXO SPI_RAW_INT_STAT_TX_FIFO_ORIS
#define | LL_SPI_RIS_TXE SPI_RAW_INT_STAT_TX_FIFO_ERIS

## Detailed Description

Interrupt definitions which can be used with LL_SPI_ReadReg and LL_SPI_WriteReg functions.

## Macro Definition Documentation

## ◆ LL_SPI_IM_MST

#define LL_SPI_IM_MST SPI_INT_MASK_MULTI_M_CIM

Multi-Master Contention Interrupt enable

Definition at line 167 of file gr533x_ll_spi.h.

## ◆ LL_SPI_IM_RXF

#define LL_SPI_IM_RXF SPI_INT_MASK_RX_FIFO_FIM

Receive FIFO Full Interrupt enable

Definition at line 168 of file gr533x_ll_spi.h.

## ◆ LL_SPI_IM_RXO

#define LL_SPI_IM_RXO SPI_INT_MASK_RX_FIFO_OIM

Receive FIFO Overflow Interrupt enable

Definition at line 169 of file gr533x_ll_spi.h.

## ◆ LL_SPI_IM_RXU

#define LL_SPI_IM_RXU SPI_INT_MASK_RX_FIFO_UIM

Receive FIFO Underflow Interrupt enable

Definition at line 170 of file gr533x_ll_spi.h.

## ◆ LL_SPI_IM_TXE

#define LL_SPI_IM_TXE SPI_INT_MASK_TX_FIFO_EIM

Transmit FIFO Empty Interrupt enable

Definition at line 172 of file gr533x_ll_spi.h.

## ◆ LL_SPI_IM_TXO

#define LL_SPI_IM_TXO SPI_INT_MASK_TX_FIFO_OIM

Transmit FIFO Overflow Interrupt enable

Definition at line 171 of file gr533x_ll_spi.h.

## ◆ LL_SPI_IS_MST

#define LL_SPI_IS_MST SPI_INT_STAT_MULTI_M_CIS

Multi-Master Contention Interrupt flag

Definition at line 174 of file gr533x_ll_spi.h.

## ◆ LL_SPI_IS_RXF

#define LL_SPI_IS_RXF SPI_INT_STAT_RX_FIFO_FIS

Receive FIFO Full Interrupt flag

Definition at line 175 of file gr533x_ll_spi.h.

## ◆ LL_SPI_IS_RXO

#define LL_SPI_IS_RXO SPI_INT_STAT_RX_FIFO_OIS

Receive FIFO Overflow Interrupt flag

Definition at line 176 of file gr533x_ll_spi.h.

## ◆ LL_SPI_IS_RXU

#define LL_SPI_IS_RXU SPI_INT_STAT_RX_FIFO_UIS

Receive FIFO Underflow Interrupt flag

Definition at line 177 of file gr533x_ll_spi.h.

## ◆ LL_SPI_IS_TXE

#define LL_SPI_IS_TXE SPI_INT_STAT_TX_FIFO_EIS

Transmit FIFO Empty Interrupt flag

Definition at line 179 of file gr533x_ll_spi.h.

## ◆ LL_SPI_IS_TXO

#define LL_SPI_IS_TXO SPI_INT_STAT_TX_FIFO_OIS

Transmit FIFO Overflow Interrupt flag

Definition at line 178 of file gr533x_ll_spi.h.

## ◆ LL_SPI_RIS_MST

#define LL_SPI_RIS_MST SPI_RAW_INT_STAT_MULTI_M_CRIS

Multi-Master Contention RAW Interrupt flag

Definition at line 181 of file gr533x_ll_spi.h.

## ◆ LL_SPI_RIS_RXF

#define LL_SPI_RIS_RXF SPI_RAW_INT_STAT_RX_FIFO_FRIS

Receive FIFO Full RAW Interrupt flag

Definition at line 182 of file gr533x_ll_spi.h.

## ◆ LL_SPI_RIS_RXO

#define LL_SPI_RIS_RXO SPI_RAW_INT_STAT_RX_FIFO_ORIS

Receive FIFO Overflow RAW Interrupt flag

Definition at line 183 of file gr533x_ll_spi.h.

## ◆ LL_SPI_RIS_RXU

#define LL_SPI_RIS_RXU SPI_RAW_INT_STAT_RX_FIFO_URIS

Receive FIFO Underflow RAW Interrupt flag

Definition at line 184 of file gr533x_ll_spi.h.

## ◆ LL_SPI_RIS_TXE

#define LL_SPI_RIS_TXE SPI_RAW_INT_STAT_TX_FIFO_ERIS

Transmit FIFO Empty RAW Interrupt flag

Definition at line 186 of file gr533x_ll_spi.h.

## ◆ LL_SPI_RIS_TXO

#define LL_SPI_RIS_TXO SPI_RAW_INT_STAT_TX_FIFO_ORIS

Transmit FIFO Overflow RAW Interrupt flag

Definition at line 185 of file gr533x_ll_spi.h.