Macros
Defines
BLE Services » Multi Link Multi Role Service (MLMR)

## Macros
#define | MLMR_CONNECTION_MAX 10
#define | MLMR_MAX_DATA_LEN 247
#define | MLMR_FLOW_CTRL_LEN 1
#define | MLMR_SERVICE_UUID

## Detailed Description

## Macro Definition Documentation

## ◆ MLMR_CONNECTION_MAX

#define MLMR_CONNECTION_MAX 10

Maximum number of Multi Link Multi Role Service connections.

Definition at line 71 of file mlmr.h.

## ◆ MLMR_FLOW_CTRL_LEN

#define MLMR_FLOW_CTRL_LEN 1

Maximum length of ble flow control data packet which is transmitted via MLMR.

Definition at line 73 of file mlmr.h.

## ◆ MLMR_MAX_DATA_LEN

#define MLMR_MAX_DATA_LEN 247

Maximum length of application data packet which is transmitted via MLMR.

Definition at line 72 of file mlmr.h.

## ◆ MLMR_SERVICE_UUID

#define MLMR_SERVICE_UUID

Value:
0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x01, 0x02, 0xED, 0xA6

The UUID of Multi Link Multi Role Service for setting advertising data.

Definition at line 75 of file mlmr.h.