Public Attributes | List of all members
iso_set_per_adv_rcv_enable_t Struct Reference
BLE » Core Isochronous Channels | BLE » Logical Link Control and Adaptation Protocol (L2CAP) » Structures

The parameter for setting periodic advertising reciving enable. More...

`#include <ble_iso.h>`

## Public Attributes
uint16_t | sync_hdl
uint8_t | enable

## Detailed Description

The parameter for setting periodic advertising reciving enable.

Definition at line 416 of file ble_iso.h.

## Member Data Documentation

## ◆ enable

uint8_t iso_set_per_adv_rcv_enable_t::enable

0x00: Reporting disabled, 0x01: Reporting enabled.

Definition at line 419 of file ble_iso.h.

## ◆ sync_hdl

uint16_t iso_set_per_adv_rcv_enable_t::sync_hdl

identifying the periodic advertising, (Range: 0x0000 to 0x0EFF).

Definition at line 418 of file ble_iso.h.

The documentation for this struct was generated from the following file:

- ble_iso.h