Macros
QSPI Buad Rate
Peripheral Driver » LL Driver » Defines » XQSPI Exported Constants

## Macros
#define | LL_XQSPI_BAUD_RATE_64M 0x00000000UL
#define | LL_XQSPI_BAUD_RATE_48M (1UL << AON_CTL_FLASH_CACHE_XF_SCK_CLK_SEL_Pos)
#define | LL_XQSPI_BAUD_RATE_32M (2UL << AON_CTL_FLASH_CACHE_XF_SCK_CLK_SEL_Pos)
#define | LL_XQSPI_BAUD_RATE_24M (3UL << AON_CTL_FLASH_CACHE_XF_SCK_CLK_SEL_Pos)
#define | LL_XQSPI_BAUD_RATE_16M (4UL << AON_CTL_FLASH_CACHE_XF_SCK_CLK_SEL_Pos)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_XQSPI_BAUD_RATE_16M

#define LL_XQSPI_BAUD_RATE_16M (4UL << AON_CTL_FLASH_CACHE_XF_SCK_CLK_SEL_Pos)

Clock to 16MHz

Definition at line 314 of file gr533x_ll_xqspi.h.

## ◆ LL_XQSPI_BAUD_RATE_24M

#define LL_XQSPI_BAUD_RATE_24M (3UL << AON_CTL_FLASH_CACHE_XF_SCK_CLK_SEL_Pos)

Clock to 24MHz

Definition at line 313 of file gr533x_ll_xqspi.h.

## ◆ LL_XQSPI_BAUD_RATE_32M

#define LL_XQSPI_BAUD_RATE_32M (2UL << AON_CTL_FLASH_CACHE_XF_SCK_CLK_SEL_Pos)

Clock to 32MHz

Definition at line 312 of file gr533x_ll_xqspi.h.

## ◆ LL_XQSPI_BAUD_RATE_48M

#define LL_XQSPI_BAUD_RATE_48M (1UL << AON_CTL_FLASH_CACHE_XF_SCK_CLK_SEL_Pos)

Clock to 48MHz

Definition at line 311 of file gr533x_ll_xqspi.h.

## ◆ LL_XQSPI_BAUD_RATE_64M

#define LL_XQSPI_BAUD_RATE_64M 0x00000000UL

Clock to 64MHz

Definition at line 310 of file gr533x_ll_xqspi.h.