Data Fields
gatts_read_cfm_t Struct Reference
BLE » Generic Attribute Profile (GATT) » Generic Attribute Profile (GATT) Server » Structures

GATT read attribute result description. More...

`#include <ble_gatts.h>`

## Data Fields
uint16_t | handle
uint16_t | length
uint8_t | status
uint8_t * | value

## Detailed Description

GATT read attribute result description.

## Field Documentation

## ◆ handle

uint16_t gatts_read_cfm_t::handle

Handle of the read attribute.

## ◆ length

uint16_t gatts_read_cfm_t::length

Length of read data.

## ◆ status

uint8_t gatts_read_cfm_t::status

Status of read operation by upper layers. See BLE Stack specific error codes.

## ◆ value

uint8_t* gatts_read_cfm_t::value

Attribute value pointer.

The documentation for this struct was generated from the following file:

- ble_gatts.h