Macros
Defines
BLE Services » Throughput Control Point Client (THSCPS)
Collaboration diagram for Defines:

## Macros
#define | THSCPS_CONNECTION_MAX
| Maximum number of THSCPS connections. More...
#define | THSCPS_CTRL_PT_VAL_LEN 20
| Length of the value of Control Point characteristic.
#define | THSCPS_TEST_SETTING_VAL_LEN 20
| Length of the value of Test Setting characteristic.
#define | THSCPS_TEST_INFO_VAL_LEN 20
| Length of the value of Test Information characteristic.
#define | THSCPS_CONN_INFO_VAL_LEN 20
| Length of the value of Connection Information characteristic.
#define | THSCPS_SERVICE_UUID
| The UUID of THS Control Point Control Point Service for setting advertising data. More...
#define | THSCPS_ACTION_ON 0x01
| Start the action.
#define | THSCPS_ACTION_OFF 0x00
| Stop the action.
#define | THSCPS_CTRL_PT_RSP_CODE 0xff
| Response code.

## Detailed Description

## Macro Definition Documentation

## ◆ THSCPS_CONNECTION_MAX

#define THSCPS_CONNECTION_MAX

Value:
(10 < CFG_MAX_CONNECTIONS ?\
10 : CFG_MAX_CONNECTIONS)

Maximum number of THSCPS connections.

## ◆ THSCPS_SERVICE_UUID

#define THSCPS_SERVICE_UUID

Value:
0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x01, 0x07, 0xED, 0xA6

The UUID of THS Control Point Control Point Service for setting advertising data.