Here is a list of all documented functions, variables, defines, enums, and typedefs with links to the documentation:

### - s -

- SAMPLES_CONNECTION_MAX : sample_service.h
- samples_evt_handler_t : sample_service.h
- samples_evt_type_t : sample_service.h
- SAMPLES_INSTANCE_MAX : sample_service.h
- SAMPLES_MAX_DATA_LEN : sample_service.h
- samples_notify_tx_data() : sample_service.h
- samples_service_init() : sample_service.h
- SAMPLES_SERVICE_UUID : sample_service.h
- sdk_clock_type_t : platform_sdk.h
- SDK_ERR_ADV_DATA_NOT_SET : ble_error.h
- SDK_ERR_APP_ERROR : ble_error.h
- SDK_ERR_BUSY : ble_error.h
- SDK_ERR_DISALLOWED : ble_error.h
- SDK_ERR_DISCONNECTED : ble_error.h
- SDK_ERR_EXT_SCAN_RSP_DATA_NOT_SET : ble_error.h
- SDK_ERR_IND_DISABLED : ble_error.h
- SDK_ERR_INVALID_ADDRESS : ble_error.h
- SDK_ERR_INVALID_ADV_DATA_TYPE : ble_error.h
- SDK_ERR_INVALID_ADV_IDX : ble_error.h
- SDK_ERR_INVALID_ADV_INTERVAL : ble_error.h
- SDK_ERR_INVALID_ADV_PARAM : ble_error.h
- SDK_ERR_INVALID_ADV_PEER_ADDR : ble_error.h
- SDK_ERR_INVALID_ATT_VAL_LEN : ble_error.h
- SDK_ERR_INVALID_BUFF_LENGTH : ble_error.h
- SDK_ERR_INVALID_CHL_NUM : ble_error.h
- SDK_ERR_INVALID_CID : ble_error.h
- SDK_ERR_INVALID_CONN_IDX : ble_error.h
- SDK_ERR_INVALID_DATA_LENGTH : ble_error.h
- SDK_ERR_INVALID_DISVCOVERY_MODE : ble_error.h
- SDK_ERR_INVALID_DURATION_PARAM : ble_error.h
- SDK_ERR_INVALID_HANDLE : ble_error.h
- SDK_ERR_INVALID_OFFSET : ble_error.h
- SDK_ERR_INVALID_PARAM : ble_error.h
- SDK_ERR_INVALID_PER_SYNC_IDX : ble_error.h
- SDK_ERR_INVALID_PERM : ble_error.h
- SDK_ERR_INVALID_PSM_ALREADY_REGISTERED : ble_error.h
- SDK_ERR_INVALID_PSM_EXCEEDED_MAX_PSM_NUM : ble_error.h
- SDK_ERR_INVALID_PSM_NUM : ble_error.h
- SDK_ERR_LIST_FULL : ble_error.h
- SDK_ERR_LIST_ITEM_ALREADY_EXISTED : ble_error.h
- SDK_ERR_LIST_ITEM_NOT_FOUND : ble_error.h
- SDK_ERR_NO_RESOURCES : ble_error.h
- SDK_ERR_NOT_ENOUGH_CREDITS : ble_error.h
- SDK_ERR_NTF_DISABLED : ble_error.h
- SDK_ERR_NVDS_NOT_INIT : ble_error.h
- SDK_ERR_PER_ADV_DATA_NOT_SET : ble_error.h
- SDK_ERR_POINTER_NULL : ble_error.h
- SDK_ERR_PROFILE_COUNT : ble_error.h
- SDK_ERR_REQ_NOT_SUPPORTED : ble_error.h
- SDK_ERR_SDK_INTERNAL : ble_error.h
- sdk_err_t : ble_error.h
- SDK_ERR_TIMER_INSUFFICIENT : ble_error.h
- SDK_SUCCESS : ble_error.h
- SEC_CON : ble_gatts.h
- sec_enc_ind_t : ble_sec.h
- sec_enc_req_type_t : ble_sec.h
- sec_io_cap_t : ble_sec.h
- sec_key_missing_reason_t : ble_sec.h
- sec_keypress_notify_t : ble_sec.h
- SEC_LEVEL_MASK : ble_gatts.h
- SEC_MODE1_LEVEL1 : ble_sec.h
- SEC_MODE1_LEVEL2 : ble_sec.h
- SEC_MODE1_LEVEL3 : ble_sec.h
- SEC_MODE1_LEVEL4 : ble_sec.h
- SEC_MODE2_LEVEL1 : ble_sec.h
- SEC_MODE2_LEVEL2 : ble_sec.h
- sec_mode_level_t : ble_sec.h
- SEC_TK_DISPLAY : ble_sec.h
- SEC_TK_KEY_ENTRY : ble_sec.h
- SEC_TK_OOB : ble_sec.h
- sec_tk_type_t : ble_sec.h
- SEM_NO_WAIT : app_rtos_cfg.h
- SEM_WAIT_FOREVER : app_rtos_cfg.h
- send_signal_carrier_wave() : ble.h
- SERVICE_TABLE_TYPE_128 : ble_gatts.h
- SERVICE_TABLE_TYPE_16 : ble_gatts.h
- SPI_DATASIZE_10BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_11BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_12BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_13BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_14BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_15BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_16BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_17BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_18BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_19BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_20BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_21BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_22BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_23BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_24BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_25BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_26BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_27BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_28BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_29BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_30BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_31BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_32BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_4BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_5BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_6BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_7BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_8BIT : gr55xx_hal_spi.h
- SPI_DATASIZE_9BIT : gr55xx_hal_spi.h
- SPI_DIRECTION_FULL_DUPLEX : gr55xx_hal_spi.h
- SPI_DIRECTION_READ_EEPROM : gr55xx_hal_spi.h
- SPI_DIRECTION_SIMPLEX_RX : gr55xx_hal_spi.h
- SPI_DIRECTION_SIMPLEX_TX : gr55xx_hal_spi.h
- SPI_FLAG_BUSY : gr55xx_hal_spi.h
- SPI_FLAG_DCOL : gr55xx_hal_spi.h
- SPI_FLAG_RFF : gr55xx_hal_spi.h
- SPI_FLAG_RFNE : gr55xx_hal_spi.h
- SPI_FLAG_TFE : gr55xx_hal_spi.h
- SPI_FLAG_TFNF : gr55xx_hal_spi.h
- SPI_FLAG_TXE : gr55xx_hal_spi.h
- spi_handle_t : gr55xx_hal_spi.h
- spi_init_t : gr55xx_hal_spi.h
- SPI_IT_MST : gr55xx_hal_spi.h
- SPI_IT_RXF : gr55xx_hal_spi.h
- SPI_IT_RXO : gr55xx_hal_spi.h
- SPI_IT_RXU : gr55xx_hal_spi.h
- SPI_IT_TXE : gr55xx_hal_spi.h
- SPI_IT_TXO : gr55xx_hal_spi.h
- SPI_PHASE_1EDGE : gr55xx_hal_spi.h
- SPI_PHASE_2EDGE : gr55xx_hal_spi.h
- SPI_POLARITY_HIGH : gr55xx_hal_spi.h
- SPI_POLARITY_LOW : gr55xx_hal_spi.h
- SPI_RX_FIFO_LEVEL_MAX : gr55xx_hal_spi.h
- SPI_SLAVE_SELECT_0 : gr55xx_hal_spi.h
- SPI_SLAVE_SELECT_1 : gr55xx_hal_spi.h
- SPI_SLAVE_SELECT_ALL : gr55xx_hal_spi.h
- SPI_TIMODE_DISABLE : gr55xx_hal_spi.h
- SPI_TIMODE_ENABLE : gr55xx_hal_spi.h
- SPI_TX_FIFO_LEVEL_MAX : gr55xx_hal_spi.h
- SPI_XFER_ADDR_NONE : gr55xx_hal_spi_v2.h
- SPI_XFER_INST_ADDR_NONE : gr55xx_hal_spi_v2.h
- SPI_XFER_INST_NONE : gr55xx_hal_spi_v2.h
- sram_size_t : gr55xx_sys.h
- SRVC_DISABLE : ble_gatts.h
- SRVC_ENCRP_KEY_SIZE_16 : ble_gatts.h
- SRVC_MULTI_ENABLE : ble_gatts.h
- SRVC_PERM : ble_gatts.h
- SRVC_SECONDARY_SET : ble_gatts.h
- SRVC_UUID_TYPE_SET : ble_gatts.h
- svc_func_register() : gr55xx_fpb.h
- SVC_handler_proc() : gr55xx_fpb.h
- svc_table_register() : gr55xx_fpb.h
- sys_adc_trim_get() : gr55xx_sys.h
- sys_app_printf() : gr55xx_sys.h
- sys_assert_cb_register() : gr55xx_sys.h
- sys_attdb_usage_ratio_get() : gr55xx_sys.h
- SYS_BD_ADDR_LEN : gr55xx_sys.h
- sys_ble_heartbeat_period_get() : gr55xx_sys.h
- sys_ble_heartbeat_period_set() : gr55xx_sys.h
- SYS_CHIP_UID_LEN : gr55xx_sys.h
- sys_context_checksum_gen() : gr55xx_sys.h
- sys_context_func_t : gr55xx_sys.h
- sys_context_save() : gr55xx_sys.h
- sys_crystal_trim_get() : gr55xx_sys.h
- sys_delay_ms() : gr55xx_sys.h
- sys_delay_us() : gr55xx_sys.h
- SYS_DEV_SRAM_128K : gr55xx_sys.h
- SYS_DEV_SRAM_256K : gr55xx_sys.h
- SYS_DEV_SRAM_64K : gr55xx_sys.h
- sys_device_addr_get() : gr55xx_sys.h
- sys_device_lp_gain_offset_2m_get() : gr55xx_sys.h
- sys_device_package_get() : gr55xx_sys.h
- sys_device_sram_get() : gr55xx_sys.h
- sys_device_uid_get() : gr55xx_sys.h
- sys_env_usage_ratio_get() : gr55xx_sys.h
- sys_firmware_jump() : gr55xx_sys.h
- sys_free() : gr55xx_sys.h
- SYS_INVALID_TIMER_ID : gr55xx_sys.h
- sys_ke_sleep_check() : gr55xx_sys.h
- sys_link_quality_clear() : gr55xx_sys.h
- sys_link_quality_get() : gr55xx_sys.h
- sys_lld_max_msg_usage_ratio_set() : gr55xx_sys.h
- sys_lpclk_get() : gr55xx_sys.h
- sys_lpclk_set() : gr55xx_sys.h
- sys_lpclk_update_func_register() : gr55xx_sys.h
- sys_lpclk_update_func_with_return_register() : gr55xx_sys.h
- sys_lpcycles_2_hus() : gr55xx_sys.h
- sys_lpper_get() : gr55xx_sys.h
- sys_malloc() : gr55xx_sys.h
- sys_max_msg_usage_ratio_set() : gr55xx_sys.h
- sys_min_sleep_threshold_set() : platform_sdk.h
- sys_msg_usage_ratio_get() : gr55xx_sys.h
- sys_nonret_usage_ratio_get() : gr55xx_sys.h
- sys_pmu_trim_get() : gr55xx_sys.h
- sys_regs_save() : gr55xx_sys.h
- sys_reverse_hword() : gr55xx_sys.h
- sys_reverse_word() : gr55xx_sys.h
- sys_rf_trim_get() : gr55xx_sys.h
- sys_sdk_verison_get() : gr55xx_sys.h
- sys_security_data_use_present() : gr55xx_sys.h
- sys_security_enable_status_check() : gr55xx_sys.h
- SYS_SET_BD_ADDR : gr55xx_sys.h
- sys_signal_handler_register() : gr55xx_sys.h
- sys_swd_disable() : gr55xx_sys.h
- sys_swd_enable() : gr55xx_sys.h
- sys_trim_sum_get() : gr55xx_sys.h
- sys_us_2_lpcycles() : gr55xx_sys.h
- system_lp_counter_set() : platform_sdk.h
- system_pmu_deinit() : platform_sdk.h
- system_pmu_init() : platform_sdk.h
- SYSTICK_CLKSOURCE_HCLK : gr55xx_hal_cortex.h
- SYSTICK_CLKSOURCE_REFCLK : gr55xx_hal_cortex.h
- SYSTICK_CURRENT_VALUE : gr55xx_hal.h
- SYSTICK_RELOAD_VALUE : gr55xx_hal.h