Data Fields
gap_rslv_addr_read_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

Read resolvable address info struct. More...

`#include <ble_gapc.h>`

## Data Fields
uint8_t | op_code
gap_addr_t | gap_addr

## Detailed Description

Read resolvable address info struct.

## Field Documentation

## ◆ gap_addr

gap_addr_t gap_rslv_addr_read_t::gap_addr

Resolvable address info.

## ◆ op_code

uint8_t gap_rslv_addr_read_t::op_code

Operation code.

See also
  enum gap_rslv_addr_read_op_id_t.

The documentation for this struct was generated from the following file:

- ble_gapc.h