Data Fields
gap_conn_info_t Union Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

Connection info. More...

`#include <ble_gapc.h>`

## Data Fields
int8_t | rssi
gap_chnl_map_t | chnl_map
gap_le_phy_ind_t | phy
uint8_t | chan_sel_algo

## Detailed Description

Connection info.

## Field Documentation

## ◆ chan_sel_algo

uint8_t gap_conn_info_t::chan_sel_algo

Chanel Selection algorithm, 0x00: LE Channel Selection Algorithm #1 is used. 0x01: LE Channel Selection Algorithm #2 is used.
0x02-0xFF: reserved.

## ◆ chnl_map

gap_chnl_map_t gap_conn_info_t::chnl_map

channel map.

## ◆ phy

gap_le_phy_ind_t gap_conn_info_t::phy

PHY indicaiton.

## ◆ rssi

int8_t gap_conn_info_t::rssi

RSSI.

The documentation for this union was generated from the following file:

- ble_gapc.h