Enumerations
Enumerations
BLE Services » Phone Alert Status Service (PASS)

## Enumerations
enum | pass_ringer_ctrl_pt_t { PASS_CTRL_PT_SILENT_MODE = 0x01, PASS_CTRL_PT_MUTE_ONCE, PASS_CTRL_PT_CANCEL_SLIENT_MODE }
| Phone Alert Status Service Ringer Control Point. More...
enum | pass_evt_type_t { PASS_EVT_INVALID, PASS_EVT_ALERT_STATUS_NTF_ENABLE, PASS_EVT_ALERT_STATUS_NTF_DISABLE, PASS_EVT_RINGER_SET_NTF_ENABLE, PASS_EVT_RINGER_SET_NTF_DISABLE, PASS_EVT_SILENT_MODE_SET, PASS_EVT_MUTE_ONCE_SET, PASS_EVT_SILENT_MODE_CANCEL }
| Phone Alert Status Service event type. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ pass_evt_type_t

enum pass_evt_type_t

Phone Alert Status Service event type.

Enumerator
PASS_EVT_INVALID | Invalid PASS event type.
PASS_EVT_ALERT_STATUS_NTF_ENABLE | Alert Status notification is enabled.
PASS_EVT_ALERT_STATUS_NTF_DISABLE | Alert Status notification is disabled.
PASS_EVT_RINGER_SET_NTF_ENABLE | Ringer Setting notification is enabled.
PASS_EVT_RINGER_SET_NTF_DISABLE | Ringer Setting notification is disabled.
PASS_EVT_SILENT_MODE_SET | Set silent mode.
PASS_EVT_MUTE_ONCE_SET | Set mute once.
PASS_EVT_SILENT_MODE_CANCEL | Cancel silent mode.

## ◆ pass_ringer_ctrl_pt_t

enum pass_ringer_ctrl_pt_t

Phone Alert Status Service Ringer Control Point.

Enumerator
PASS_CTRL_PT_SILENT_MODE | Silent Mode.
PASS_CTRL_PT_MUTE_ONCE | Mute Once.
PASS_CTRL_PT_CANCEL_SLIENT_MODE | Cancel Silent Mode.