Enumerations
HAL ISO7816 State
Peripheral Driver » HAL Driver » ISO7816 » Enumerations

## Enumerations
enum | hal_iso7816_state_t { HAL_ISO7816_STATE_RESET = 0x00U, HAL_ISO7816_STATE_READY = 0x20U, HAL_ISO7816_STATE_BUSY = 0x24U, HAL_ISO7816_STATE_BUSY_TX = 0x21U, HAL_ISO7816_STATE_BUSY_RX = 0x22U, HAL_ISO7816_STATE_BUSY_TX_RX = 0x23U, HAL_ISO7816_STATE_ABORT = 0x08U, HAL_ISO7816_STATE_TIMEOUT = 0xA0U, HAL_ISO7816_STATE_ERROR = 0xE0U }
| HAL ISO7816 State Enumerations definition. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ hal_iso7816_state_t

enum hal_iso7816_state_t

HAL ISO7816 State Enumerations definition.

Enumerator
HAL_ISO7816_STATE_RESET | Peripheral not initialized
HAL_ISO7816_STATE_READY | Peripheral initialized and ready for use
HAL_ISO7816_STATE_BUSY | An internal process is ongoing
HAL_ISO7816_STATE_BUSY_TX | Data Transmission process is ongoing
HAL_ISO7816_STATE_BUSY_RX | Data Reception process is ongoing
HAL_ISO7816_STATE_BUSY_TX_RX | Data Transmission and Reception process is ongoing
HAL_ISO7816_STATE_ABORT | Peripheral with abort request ongoing
HAL_ISO7816_STATE_TIMEOUT | Timeout state
HAL_ISO7816_STATE_ERROR | Peripheral in error