Macros
GAP PHY OPTIONS (bitmask)
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Defines

## Macros
#define | PHY_OPT_NO_CODING 0x00
#define | PHY_OPT_S2_CODING 0x01
#define | PHY_OPT_S8_CODING 0x02

## Detailed Description

## Macro Definition Documentation

## ◆ PHY_OPT_NO_CODING

#define PHY_OPT_NO_CODING 0x00

The Host has no preferred coding when transmitting on the LE Coded PHY.

## ◆ PHY_OPT_S2_CODING

#define PHY_OPT_S2_CODING 0x01

The Host prefers that S=2 coding be used when transmitting on the LE Coded PHY.

## ◆ PHY_OPT_S8_CODING

#define PHY_OPT_S8_CODING 0x02

The Host prefers that S=8 coding be used when transmitting on the LE Coded PHY.