Here is a list of all documented struct and union fields with links to the struct/union documentation for each field:

### - m -

- major : sdk_version_t
- manager_cbs : prf_client_info_t , prf_server_info_t
- mantissa : ieee_float16_t , ieee_float32_t
- manuf_name : gap_dev_version_ind_t
- manufact_name_str : dis_init_t
- manufacturer_id : dis_c_sys_id_t , dis_sys_id_t
- map : gap_chnl_map_t
- master_ack_count : _i2c_handle
- max : gls_racp_filter_t
- max_adv_data_len : gap_dev_info_t
- max_adv_evt : gap_adv_time_param_t
- max_connection_nb : prf_client_info_t , prf_server_info_t
- max_data_len : gap_dev_info_t
- max_meas_interval_sup : hts_init_t
- max_nb_attr : gatts_create_db_t
- max_rx_octets : gap_le_pkt_size_ind_t
- max_rx_time : gap_le_pkt_size_ind_t
- max_size : attm_desc_128_t , attm_desc_t
- max_skip : gap_adv_second_cfg_t
- max_tx_octets : gap_le_pkt_size_ind_t
- max_tx_pwr : gap_adv_param_t , gap_dev_tx_power_t , gap_ext_adv_param_t
- max_tx_time : gap_le_pkt_size_ind_t
- meal : gls_meas_ctx_t
- mean_arterial_pr : bps_meas_t
- meas_ctx : gls_rec_t
- meas_interval : hts_init_t
- meas_status : bps_meas_t
- meas_status_present : bps_meas_t
- meas_val : gls_rec_t
- medication : gls_meas_ctx_t
- medication_id : gls_meas_ctx_t
- min : _calendar_alarm , _calendar_time , gls_racp_filter_t , prf_date_time_t
- min_meas_interval_sup : hts_init_t
- min_tx_pwr : gap_dev_tx_power_t
- minor : sdk_version_t
- miso : app_spi_pin_cfg_t
- mks_flag : gap_lepsm_register_t
- mode : _aon_gpio_init , _calendar_handle , _dma_init , _gpio_init , _hmac_init , _i2c_handle , _ll_aon_gpio_init , _ll_dma_init , _ll_gpio_init , _ll_msio_init , _ll_pwm_init_t , _ll_xqspi_init_t , _msio_init , app_gpiote_param_t , app_io_init_t , gdx_lcp_config_t , pwm_init_t
- model_num_str : dis_init_t
- mon : _calendar_time
- month : birth_date_t , prf_date_time_t
- mosi : app_spi_pin_cfg_t
- mps : lecb_cfm_conn_t , lecb_conn_req_t
- ms : _calendar_handle , _calendar_time
- msg_ret : stack_heaps_table_t
- msg_ret_size : stack_heaps_table_t
- msp_deinit : _hal_callback
- msp_init : _hal_callback
- mtu : lecb_cfm_conn_t , lecb_conn_req_t
- muscle_mass : bcs_meas_val_t
- muscle_mass_present : bcs_meas_flag_t
- muscle_percentage : bcs_meas_val_t
- muscle_percentage_present : bcs_meas_flag_t
- mux : _aon_gpio_init , _gpio_init , _ll_aon_gpio_init , _ll_gpio_init , _ll_msio_init , _msio_init , app_adc_pin_t , app_comp_pin_t , app_i2c_pin_t , app_i2s_pin_t , app_io_init_t , app_pwm_pin_t , app_qspi_pin_t , app_spi_pin_t , app_uart_pin_t