Macros
Master Addressing Mode
Peripheral Driver » LL Driver » I2C » Defines » I2C Exported Constants

## Macros
#define | LL_I2C_ADDRESSING_MODE_7BIT 0x00000000U
#define | LL_I2C_ADDRESSING_MODE_10BIT I2C_CON_10BITADDR_MST

## Detailed Description

## Macro Definition Documentation

## ◆ LL_I2C_ADDRESSING_MODE_10BIT

#define LL_I2C_ADDRESSING_MODE_10BIT I2C_CON_10BITADDR_MST

Master operates in 10-bit addressing mode.

## ◆ LL_I2C_ADDRESSING_MODE_7BIT

#define LL_I2C_ADDRESSING_MODE_7BIT 0x00000000U

Master operates in 7-bit addressing mode.