Data Fields
gap_dev_info_t Union Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

Device info. More...

`#include <ble_gapc.h>`

## Data Fields
gap_dev_version_ind_t | dev_version
gap_get_bd_addr_t | get_bd_addr
gap_dev_adv_tx_power_t | adv_tx_power
gap_sugg_dflt_data_len_t | sugg_dflt_data_len
gap_max_data_len_t | max_data_len
gap_nb_adv_sets_t | nb_adv_sets
gap_max_adv_data_len_ind_t | max_adv_data_len
gap_dev_tx_power_t | dev_tx_power
gap_dev_rf_path_comp_ind_t | dev_rf_path_comp

## Detailed Description

Device info.

## Field Documentation

## ◆ adv_tx_power

gap_dev_adv_tx_power_t gap_dev_info_t::adv_tx_power

Advertising TX power info.

## ◆ dev_rf_path_comp

gap_dev_rf_path_comp_ind_t gap_dev_info_t::dev_rf_path_comp

RF path compensation values.

## ◆ dev_tx_power

gap_dev_tx_power_t gap_dev_info_t::dev_tx_power

Device TX power info.

## ◆ dev_version

gap_dev_version_ind_t gap_dev_info_t::dev_version

Version info.

## ◆ get_bd_addr

gap_get_bd_addr_t gap_dev_info_t::get_bd_addr

Device BD address info.

## ◆ max_adv_data_len

gap_max_adv_data_len_ind_t gap_dev_info_t::max_adv_data_len

Maximum advertising data length info.

## ◆ max_data_len

gap_max_data_len_t gap_dev_info_t::max_data_len

Suggested MAX data length info.

## ◆ nb_adv_sets

gap_nb_adv_sets_t gap_dev_info_t::nb_adv_sets

Number of available advertising sets.

## ◆ sugg_dflt_data_len

gap_sugg_dflt_data_len_t gap_dev_info_t::sugg_dflt_data_len

Suggested default data length info.

The documentation for this union was generated from the following file:

- ble_gapc.h