Modules
Current Time Service (CTS)
BLE Services

Current Time Service module. More...

## Modules
| Defines
| Enumerations
| Structures
| Typedefs
| Functions

## Detailed Description

Current Time Service module.

The Current Time Service exposes Current Time characteristic. It optionally exposes Local Time Information characteristic and Reference Time Information characteristic.

After cts_init_t variable is intialized, the application must call cts_service_init() to add Current Time Service and Current Time, Local Time Information and Reference Time Information characteristics to the BLE Stack database according to cts_init_t::char_mask.