Data Fields
hids_hid_info_t Struct Reference
BLE Services » Human Input Device Service (HIDS) » Typedefs

HID Information characteristic value. More...

`#include <hids.h>`

## Data Fields
uint16_t | bcd_hid
uint8_t | b_country_code
uint8_t | flags

## Detailed Description

HID Information characteristic value.

## Field Documentation

## ◆ b_country_code

uint8_t hids_hid_info_t::b_country_code

Identifies which country the hardware is localized for. Most hardware is not localized and thus this value would be zero (0).

## ◆ bcd_hid

uint16_t hids_hid_info_t::bcd_hid

16-bit unsigned integer representing version number of base USB HID Specification implemented by HID Device

## ◆ flags

uint8_t hids_hid_info_t::flags

See http://developer.bluetooth.org/gatt/characteristics/Pages/CharacteristicViewer.aspx?u=org.bluetooth.characteristic.hid_information.xml

The documentation for this struct was generated from the following file:

- hids.h