Data Fields
ancs_ntf_flags_t Struct Reference
BLE Services » Apple Notification Center Service (ANCS) » Structures

notification flags that can be performed for iOS notifications. More...

`#include <ancs_protocol.h>`

## Data Fields
uint8_t | silent: 1
uint8_t | important: 1
uint8_t | pre_existing: 1
uint8_t | positive_action: 1
uint8_t | negative_action: 1

## Detailed Description

notification flags that can be performed for iOS notifications.

## Field Documentation

## ◆ important

uint8_t ancs_ntf_flags_t::important

If this flag is set, the notification has a high priority.

## ◆ negative_action

uint8_t ancs_ntf_flags_t::negative_action

If this flag is set, the notification has a negative action that can be taken.

## ◆ positive_action

uint8_t ancs_ntf_flags_t::positive_action

If this flag is set, the notification has a positive action that can be taken.

## ◆ pre_existing

uint8_t ancs_ntf_flags_t::pre_existing

If this flag is set, the notification is pre-existing.

## ◆ silent

uint8_t ancs_ntf_flags_t::silent

If this flag is set, the notification has a low priority.

The documentation for this struct was generated from the following file:

- ancs_protocol.h