Modules | Macros
Defines
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control

## Modules
| GAP Address types
| GAP PHY OPTIONS (bitmask)

## Macros
#define | GAP_CHNL_MAP_LEN 0x05
#define | GAP_FEATS_LEN 0x08
#define | GAP_ADDR_LEN 0x06
#define | GAP_INVALID_CONN_INDEX 0xFF

## Detailed Description

## Macro Definition Documentation

## ◆ GAP_ADDR_LEN

#define GAP_ADDR_LEN 0x06

The length of address.

## ◆ GAP_CHNL_MAP_LEN

#define GAP_CHNL_MAP_LEN 0x05

The length of channel map.

## ◆ GAP_FEATS_LEN

#define GAP_FEATS_LEN 0x08

The length of features.

## ◆ GAP_INVALID_CONN_INDEX

#define GAP_INVALID_CONN_INDEX 0xFF

Invalid connection index.