Data Fields
wechat_pedo_meas_t Struct Reference
BLE Services » Wechat (WECHAT) » Structures

WeChat current pedometer measurement variable. More...

`#include <wechat.h>`

## Data Fields
uint8_t | flag
uint8_t | step_count [3]
uint8_t | step_dist [3]
uint8_t | step_calorie [3]

## Detailed Description

WeChat current pedometer measurement variable.

## Field Documentation

## ◆ flag

uint8_t wechat_pedo_meas_t::flag

Flag for WeChat current pedometer measurement.

## ◆ step_calorie

uint8_t wechat_pedo_meas_t::step_calorie[3]

Step Calorie of pedometer measurement.

## ◆ step_count

uint8_t wechat_pedo_meas_t::step_count[3]

Step counts of pedometer measurement.

## ◆ step_dist

uint8_t wechat_pedo_meas_t::step_dist[3]

Step distance of pedometer measurement.

The documentation for this struct was generated from the following file:

- wechat.h