Data Fields
ieee_float16_t Struct Reference
BLE Services » Blood Pressure Service (BPS) » Structures | BLE Services » Glucose Service (GLS) » Structures

SFLOAT format (IEEE-11073 16-bit FLOAT, defined as a 16-bit value with 12-bit mantissa and 4-bit exponent. More...

`#include <bps.h>`

## Data Fields
int8_t | exponent
int16_t | mantissa

## Detailed Description

SFLOAT format (IEEE-11073 16-bit FLOAT, defined as a 16-bit value with 12-bit mantissa and 4-bit exponent.

SFLOAT format (IEEE-11073 16-bit FLOAT, defined as a 16-bit value with 12-bit mantissa and 4-bit exponent).

## Field Documentation

## ◆ exponent

int8_t ieee_float16_t::exponent

Base 10 exponent, only 4 bits

Base 10 exponent, only 4 bits.

## ◆ mantissa

int16_t ieee_float16_t::mantissa

Mantissa, only 12 bits

Mantissa, only 12 bits.

The documentation for this struct was generated from the following files:

- bps.h
- gls.h