Data Fields
app_qspi_pin_t Struct Reference
Peripheral Driver » APP DRIVER » QSPI » Structures

QSPI IO configuration Structures. More...

`#include <app_qspi.h>`

## Data Fields
app_io_type_t | type
app_io_mux_t | mux
uint32_t | pin
app_io_pull_t | pull
uint8_t | enable

## Detailed Description

QSPI IO configuration Structures.

## Field Documentation

## ◆ enable

uint8_t app_qspi_pin_t::enable

Enable or disable the pin.

## ◆ mux

app_io_mux_t app_qspi_pin_t::mux

Specifies the Peripheral to be connected to the selected pins.

## ◆ pin

uint32_t app_qspi_pin_t::pin

Specifies the IO pins to be configured. This parameter can be any value of IO pins.

## ◆ pull

app_io_pull_t app_qspi_pin_t::pull

Specifies the Pull-up or Pull-Down activation for the selected pins.

## ◆ type

app_io_type_t app_qspi_pin_t::type

Specifies the type of QSPI IO.

The documentation for this struct was generated from the following file:

- app_qspi.h