Data Fields
tps_c_handles_t Struct Reference
BLE Services » Tx Power Service Client (TPS_C) » Structures

Handles on the connected peer device needed to interact with it. More...

`#include <tps_c.h>`

## Data Fields
uint16_t | tps_srvc_start_handle
uint16_t | tps_srvc_end_handle
uint16_t | tps_tx_power_level_handle

## Detailed Description

Handles on the connected peer device needed to interact with it.

## Field Documentation

## ◆ tps_srvc_end_handle

uint16_t tps_c_handles_t::tps_srvc_end_handle

TPS Service end handle.

## ◆ tps_srvc_start_handle

uint16_t tps_c_handles_t::tps_srvc_start_handle

TPS Service start handle.

## ◆ tps_tx_power_level_handle

uint16_t tps_c_handles_t::tps_tx_power_level_handle

TPS Tx Power Level characteristic Value handle which has been got from peer.

The documentation for this struct was generated from the following file:

- tps_c.h