Data Fields
dfu_uart_info_t Struct Reference
SYSTEM » Device Firmware Update » Structures

DFU uart config definition. More...

`#include <gr55xx_dfu.h>`

## Data Fields
dfu_info_state | state
dfu_uart_baudrate_t | baud_rate
dfu_uart_data_bit_t | data_bit
dfu_uart_stop_bit_t | stop_bits
dfu_uart_parity_bit_t | parity
dfu_uart_pin_group_t | pin_group

## Detailed Description

DFU uart config definition.

## Field Documentation

## ◆ baud_rate

dfu_uart_baudrate_t dfu_uart_info_t::baud_rate

UART communication baudrate. This parameter can be a value of dfu_uart_baudrate_t.

## ◆ data_bit

dfu_uart_data_bit_t dfu_uart_info_t::data_bit

The number of data bits transmitted or received in a frame. This parameter can be a value of dfu_uart_data_bit_t.

## ◆ parity

dfu_uart_parity_bit_t dfu_uart_info_t::parity

Specify the parity mode. This parameter can be a value of dfu_uart_parity_bit_t.

## ◆ pin_group

dfu_uart_pin_group_t dfu_uart_info_t::pin_group

Uart pin group. This parameter can be a value of dfu_uart_pin_group_t.

## ◆ state

dfu_info_state dfu_uart_info_t::state

DFU UART Enable or Disable. This parameter can be a value of dfu_info_state.

## ◆ stop_bits

dfu_uart_stop_bit_t dfu_uart_info_t::stop_bits

The number of stop bits transmitted. This parameter can be a value of dfu_uart_stop_bit_t.

The documentation for this struct was generated from the following file:

- gr55xx_dfu.h