Data Fields
_xqspi_init_t Struct Reference
Peripheral Driver » HAL Driver » XQSPI » Structures » XQSPI Configuration

XQSPI init Structure definition. More...

`#include <gr55xx_hal_xqspi.h>`

## Data Fields
uint32_t | work_mode
uint32_t | cache_mode
uint32_t | read_cmd
uint32_t | baud_rate
uint32_t | clock_mode

## Detailed Description

XQSPI init Structure definition.

## Field Documentation

## ◆ baud_rate

uint32_t _xqspi_init_t::baud_rate

Specifies the serial clock speed for transmit in both XIP and QSPI mode. This parameter can be a value of XQSPI Clock Speed

## ◆ cache_mode

uint32_t _xqspi_init_t::cache_mode

Specifies the cache mode for XIP mode. This parameter can be a value of XQSPI Cache Mode in XIP mode

## ◆ clock_mode

uint32_t _xqspi_init_t::clock_mode

Specifies the Clock Mode. It indicates the level that clock takes between commands. This parameter can be a value of XQSPI Clock Mode

## ◆ read_cmd

uint32_t _xqspi_init_t::read_cmd

Specifies the read command for transmit in XIP mode. This parameter can be a value of XQSPI Read Command in XIP mode

## ◆ work_mode

uint32_t _xqspi_init_t::work_mode

Specifies the work mode for XQSPI. This parameter can be a value of XQSPI Work Mode

The documentation for this struct was generated from the following file:

- gr55xx_hal_xqspi.h