Enumerations
Enumerations
BLE Services » HRS RSCS Relay Control Point Service (HRRCPS)

## Enumerations
enum | hrrcps_ctrl_pt_id_t { HRRCPS_CTRL_PT_SCAN_HRS = 0x01, HRRCPS_CTRL_PT_SCAN_RSCS, HRRCPS_CTRL_PT_HRS_SEN_LOC_READ, HRRCPS_CTRL_PT_RSCS_SEN_LOC_READ, HRRCPS_CTRL_PT_HRS_NTF_ENABLE, HRRCPS_CTRL_PT_HRS_NTF_DISABLE, HRRCPS_CTRL_PT_RSCS_NTF_ENABLE, HRRCPS_CTRL_PT_RSCS_NTF_DISABLE, HRRCPS_CTRL_PT_HRS_CONN_STA_REPORT, HRRCPS_CTRL_PT_RSCS_CONN_STA_REPORT, HRRCPS_CTRL_PT_HRS_DISCONN, HRRCPS_CTRL_PT_RSCS_DISCONN, HRRCPS_CTRL_PT_RSP_CODE = 0xff }
| HRS RSCS Relay Control Point Service Control Point IDs. More...
enum | hrrcps_rsp_id_t { HRRCPS_RSP_ID_OK = 0x01, HRRCPS_RSP_ID_ERROR }
| HRS RSCS Relay Control Point Service Response IDs of Control Point. More...
enum | hrrcps_evt_type_t { HRRCPS_EVT_INVALID, HRRCPS_EVT_CTRL_PT_IND_ENABLE, HRRCPS_EVT_CTRL_PT_IND_DISABLE, HRRCPS_EVT_SCAN_HRS, HRRCPS_EVT_SCAN_RSCS, HRRCPS_EVT_ENABLE_HRS_NTF, HRRCPS_EVT_DISABLE_HRS_NTF, HRRCPS_EVT_ENABLE_RSCS_NTF, HRRCPS_EVT_DISABLE_RSCS_NTF, HRRCPS_EVT_HRS_SENSOR_LOC_READ, HRRCPS_EVT_RSCS_SENSOR_LOC_READ, HRRCPS_EVT_DISCONN_HRS_LINK, HRRCPS_EVT_DISCONN_RSCS_LINK }
| HRS RSCS Relay Control Point Service event type. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ hrrcps_ctrl_pt_id_t

enum hrrcps_ctrl_pt_id_t

HRS RSCS Relay Control Point Service Control Point IDs.

Enumerator
HRRCPS_CTRL_PT_SCAN_HRS | Scan HRS device.
HRRCPS_CTRL_PT_SCAN_RSCS | Scan RSCS device.
HRRCPS_CTRL_PT_HRS_SEN_LOC_READ | Read HRS sensor location.
HRRCPS_CTRL_PT_RSCS_SEN_LOC_READ | Read RSCS sensor location.
HRRCPS_CTRL_PT_HRS_NTF_ENABLE | Enable HRS notification.
HRRCPS_CTRL_PT_HRS_NTF_DISABLE | Disable HRS notification.
HRRCPS_CTRL_PT_RSCS_NTF_ENABLE | Enable RSCS notification.
HRRCPS_CTRL_PT_RSCS_NTF_DISABLE | Disable RSCS notification.
HRRCPS_CTRL_PT_HRS_CONN_STA_REPORT | Report HRS connection state.
HRRCPS_CTRL_PT_RSCS_CONN_STA_REPORT | Report RSCS connecntion state.
HRRCPS_CTRL_PT_HRS_DISCONN | Disconnect HRS link.
HRRCPS_CTRL_PT_RSCS_DISCONN | Disconnect RSCS link.
HRRCPS_CTRL_PT_RSP_CODE | Response code.

## ◆ hrrcps_evt_type_t

enum hrrcps_evt_type_t

HRS RSCS Relay Control Point Service event type.

Enumerator
HRRCPS_EVT_INVALID | Invalid HRRCPS event type.
HRRCPS_EVT_CTRL_PT_IND_ENABLE | HRR Control Point indicaiton is enabled.
HRRCPS_EVT_CTRL_PT_IND_DISABLE | HRR Control Point indicaiton is disabled.
HRRCPS_EVT_SCAN_HRS | Scan HRS device.
HRRCPS_EVT_SCAN_RSCS | Scan RSCS device.
HRRCPS_EVT_ENABLE_HRS_NTF | Enable HRS notification.
HRRCPS_EVT_DISABLE_HRS_NTF | Disable HRS notification.
HRRCPS_EVT_ENABLE_RSCS_NTF | Enable RSCS notificaiton.
HRRCPS_EVT_DISABLE_RSCS_NTF | Disable RSCS notificaiton.
HRRCPS_EVT_HRS_SENSOR_LOC_READ | Read HRS sensor location.
HRRCPS_EVT_RSCS_SENSOR_LOC_READ | Read RSCS sensor location.
HRRCPS_EVT_DISCONN_HRS_LINK | Disconnect HRS link.
HRRCPS_EVT_DISCONN_RSCS_LINK | Disconnect RSCS link.

## ◆ hrrcps_rsp_id_t

enum hrrcps_rsp_id_t

HRS RSCS Relay Control Point Service Response IDs of Control Point.

Enumerator
HRRCPS_RSP_ID_OK | Success.
HRRCPS_RSP_ID_ERROR | Fail.