Macros
Interrupt Trigger
Peripheral Driver » LL Driver » AON_GPIO » Defines » AON_GPIO Exported Constants

## Macros
#define | LL_AON_GPIO_TRIGGER_NONE ((uint32_t)0x00U)
#define | LL_AON_GPIO_TRIGGER_RISING ((uint32_t)0x01U)
#define | LL_AON_GPIO_TRIGGER_FALLING ((uint32_t)0x02U)
#define | LL_AON_GPIO_TRIGGER_HIGH ((uint32_t)0x03U)
#define | LL_AON_GPIO_TRIGGER_LOW ((uint32_t)0x04U)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_AON_GPIO_TRIGGER_FALLING

#define LL_AON_GPIO_TRIGGER_FALLING ((uint32_t)0x02U)

Trigger Falling Mode

## ◆ LL_AON_GPIO_TRIGGER_HIGH

#define LL_AON_GPIO_TRIGGER_HIGH ((uint32_t)0x03U)

Trigger High Mode

## ◆ LL_AON_GPIO_TRIGGER_LOW

#define LL_AON_GPIO_TRIGGER_LOW ((uint32_t)0x04U)

Trigger Low Mode

## ◆ LL_AON_GPIO_TRIGGER_NONE

#define LL_AON_GPIO_TRIGGER_NONE ((uint32_t)0x00U)

No Trigger Mode

## ◆ LL_AON_GPIO_TRIGGER_RISING

#define LL_AON_GPIO_TRIGGER_RISING ((uint32_t)0x01U)

Trigger Rising Mode