Data Fields
gus_init_t Struct Reference
BLE Services » Goodix UART Service (GUS) » Structures

Goodix UART Service init stucture. This contains all option and data needed for initialization of the service. More...

`#include <gus.h>`

## Data Fields
gus_evt_handler_t | evt_handler

## Detailed Description

Goodix UART Service init stucture. This contains all option and data needed for initialization of the service.

## Field Documentation

## ◆ evt_handler

gus_evt_handler_t gus_init_t::evt_handler

Goodix UART Service event handler which must be provided by the application to send and receive the data.

The documentation for this struct was generated from the following file:

- gus.h