Data Fields
_exflash_handle Struct Reference
Peripheral Driver » HAL Driver » EXFLASH » Structures » EXFLASH handle

exFlash handle Structure definition More...

`#include <gr55xx_hal_exflash.h>`

## Data Fields
xqspi_handle_t * | p_xqspi
__IO uint32_t | fw_mode
__IO hal_lock_t | lock
__IO hal_exflash_state_t | state
__IO hal_eflash_security | security
__IO uint32_t | flash_id
__IO uint32_t | flash_size
__IO uint32_t | count
__IO uint32_t | error_code
uint32_t | retry

## Detailed Description

exFlash handle Structure definition

## Field Documentation

## ◆ count

__IO uint32_t _exflash_handle::count

exFlash count for suspend and resume

## ◆ error_code

__IO uint32_t _exflash_handle::error_code

exFlash Error code

## ◆ flash_id

__IO uint32_t _exflash_handle::flash_id

exFlash ID

## ◆ flash_size

__IO uint32_t _exflash_handle::flash_size

exFlash Size

## ◆ fw_mode

__IO uint32_t _exflash_handle::fw_mode

exFlash firmware mode

## ◆ lock

__IO hal_lock_t _exflash_handle::lock

Locking object

## ◆ p_xqspi

xqspi_handle_t* _exflash_handle::p_xqspi

exFlash XQSPI Handle parameters

## ◆ retry

uint32_t _exflash_handle::retry

Repeat times for the exFlash memory access

## ◆ security

__IO hal_eflash_security _exflash_handle::security

exFlash data security

## ◆ state

__IO hal_exflash_state_t _exflash_handle::state

exFlash communication state

The documentation for this struct was generated from the following file:

- gr55xx_hal_exflash.h