### - p -

- PASS_ALERT_STATUS_VAL_LEN : pass.h
- PASS_ALL_STATE_ACTIVE : pass.h
- PASS_C_ALL_STATE_ACTIVE : pass_c.h
- PASS_C_CONNECTION_MAX : pass_c.h
- PASS_C_DISPLAY_ALERT_ACTIVE : pass_c.h
- PASS_C_NO_STATE_ACTIVE : pass_c.h
- PASS_C_RINGER_ACTIVE : pass_c.h
- PASS_C_RINGER_CTRL_PT_VAL_LEN : pass_c.h
- PASS_C_RINGER_SET_NORMAL : pass_c.h
- PASS_C_RINGER_SET_SILENT : pass_c.h
- PASS_C_VIBRATE_ACTIVE : pass_c.h
- PASS_CHAR_FULL : pass.h
- PASS_CHAR_MANDATORY : pass.h
- PASS_CHAR_RING_CTRL_PT_SUP : pass.h
- PASS_CONNECTION_MAX : pass.h
- PASS_DISPLAY_ALERT_ACTIVE : pass.h
- PASS_NO_STATE_ACTIVE : pass.h
- PASS_RINGER_ACTIVE : pass.h
- PASS_RINGER_CTRL_PT_VAL_LEN : pass.h
- PASS_RINGER_SET_NORMAL : pass.h
- PASS_RINGER_SET_SILENT : pass.h
- PASS_RINGER_SET_VAL_LEN : pass.h
- PASS_VIBRATE_ACTIVE : pass.h
- PCS_CONNECTION_MAX : pcs.h
- PCS_MAX_DATA_LEN : pcs.h
- PCS_SERVICE_UUID : pcs.h
- PCS_SET_ADV_DATA_10B : pcs.h
- PCS_SET_ADV_DATA_17B : pcs.h
- PCS_SET_ADV_DATA_24B : pcs.h
- PCS_SET_ADV_DATA_31B : pcs.h
- PCS_SET_ADV_DATA_3B : pcs.h
- PCS_SET_PARAM_FAIL : pcs.h
- PCS_SET_PARAM_SUCCESS : pcs.h
- PHY_OPT_NO_CODING : ble_gapc.h
- PHY_OPT_S2_CODING : ble_gapc.h
- PHY_OPT_S8_CODING : ble_gapc.h
- PKC_BIGMULTI_BITS_LENGTH_MAX : gr55xx_hal_pkc.h
- PKC_BITS_LENGTH_MAX : gr55xx_hal_pkc.h
- PKC_BITS_LENGTH_MIN : gr55xx_hal_pkc.h
- PKC_FLAG_BUSY : gr55xx_hal_pkc.h
- PKC_IT_DONE : gr55xx_hal_pkc.h
- PKC_IT_ERR : gr55xx_hal_pkc.h
- PKC_IT_OVF : gr55xx_hal_pkc.h
- PKC_OPERATION_MODE_ADD : gr55xx_hal_pkc.h
- PKC_OPERATION_MODE_BIGADD : gr55xx_hal_pkc.h
- PKC_OPERATION_MODE_BIGMULTI : gr55xx_hal_pkc.h
- PKC_OPERATION_MODE_CMP : gr55xx_hal_pkc.h
- PKC_OPERATION_MODE_INVER : gr55xx_hal_pkc.h
- PKC_OPERATION_MODE_LSHIFT : gr55xx_hal_pkc.h
- PKC_OPERATION_MODE_MULTI : gr55xx_hal_pkc.h
- PKC_OPERATION_MODE_SUB : gr55xx_hal_pkc.h
- PKC_SECURE_MODE_DISABLE : gr55xx_hal_pkc.h
- PKC_SECURE_MODE_ENABLE : gr55xx_hal_pkc.h
- PRF_CHAR_PRES_FMT_SIZE : ble_prf_types.h
- PRF_INVALID_HANDLE : ble_prf_types.h
- PWM_ALIGNED_CENTER : gr55xx_hal_pwm.h
- PWM_ALIGNED_EDGE : gr55xx_hal_pwm.h
- PWM_DRIVEPOLARITY_NEGATIVE : gr55xx_hal_pwm.h
- PWM_DRIVEPOLARITY_POSITIVE : gr55xx_hal_pwm.h
- PWM_MODE_BREATH : gr55xx_hal_pwm.h
- PWM_MODE_FLICKER : gr55xx_hal_pwm.h
- PWR_COMM_CORE_MODE_RESET : gr55xx_hal_pwr.h
- PWR_COMM_CORE_MODE_RUNNING : gr55xx_hal_pwr.h
- PWR_COMM_CORE_POWER_DOWN : gr55xx_hal_pwr.h
- PWR_COMM_CORE_POWER_UP : gr55xx_hal_pwr.h
- PWR_COMM_TIMER_MODE_RESET : gr55xx_hal_pwr.h
- PWR_COMM_TIMER_MODE_RUNNING : gr55xx_hal_pwr.h
- PWR_COMM_TIMER_POWER_DOWN : gr55xx_hal_pwr.h
- PWR_COMM_TIMER_POWER_UP : gr55xx_hal_pwr.h
- PWR_EXTWKUP_PIN0 : gr55xx_hal_pwr.h
- PWR_EXTWKUP_PIN1 : gr55xx_hal_pwr.h
- PWR_EXTWKUP_PIN2 : gr55xx_hal_pwr.h
- PWR_EXTWKUP_PIN3 : gr55xx_hal_pwr.h
- PWR_EXTWKUP_PIN4 : gr55xx_hal_pwr.h
- PWR_EXTWKUP_PIN5 : gr55xx_hal_pwr.h
- PWR_EXTWKUP_PIN6 : gr55xx_hal_pwr.h
- PWR_EXTWKUP_PIN7 : gr55xx_hal_pwr.h
- PWR_EXTWKUP_PIN_ALL : gr55xx_hal_pwr.h
- PWR_EXTWKUP_TYPE_FALLING : gr55xx_hal_pwr.h
- PWR_EXTWKUP_TYPE_HIGH : gr55xx_hal_pwr.h
- PWR_EXTWKUP_TYPE_LOW : gr55xx_hal_pwr.h
- PWR_EXTWKUP_TYPE_RISING : gr55xx_hal_pwr.h
- PWR_MEM_POWER_FULL : gr55xx_hal_pwr.h
- PWR_MEM_POWER_OFF : gr55xx_hal_pwr.h
- PWR_MEM_POWER_RETENTION : gr55xx_hal_pwr.h
- PWR_SLP_TIMER_MODE_DISABLE : gr55xx_hal_pwr.h
- PWR_SLP_TIMER_MODE_NORMAL : gr55xx_hal_pwr.h
- PWR_SLP_TIMER_MODE_RELOAD : gr55xx_hal_pwr.h
- PWR_SLP_TIMER_MODE_SINGLE : gr55xx_hal_pwr.h
- PWR_TIMER_TYPE_AON_WDT : gr55xx_hal_pwr.h
- PWR_TIMER_TYPE_CAL_ALARM : gr55xx_hal_pwr.h
- PWR_TIMER_TYPE_CAL_TIMER : gr55xx_hal_pwr.h
- PWR_TIMER_TYPE_SLP_TIMER : gr55xx_hal_pwr.h
- PWR_WKUP_COND_ALL : gr55xx_hal_pwr.h
- PWR_WKUP_COND_BLE : gr55xx_hal_pwr.h
- PWR_WKUP_COND_BOD_FEDGE : gr55xx_hal_pwr.h
- PWR_WKUP_COND_CALENDAR : gr55xx_hal_pwr.h
- PWR_WKUP_COND_EXT : gr55xx_hal_pwr.h
- PWR_WKUP_COND_MSIO_COMP : gr55xx_hal_pwr.h
- PWR_WKUP_COND_TIMER : gr55xx_hal_pwr.h