Macros
Power States Defines
Peripheral Driver » LL Driver » ISO7816 » Defines » ISO7816 Exported Constants

## Macros
#define | LL_ISO7816_PWR_STATE_OFF (0x0UL << ISO7816_STAT_PWR_STAT_POS)
#define | LL_ISO7816_PWR_STATE_PWRUP_VCC (0x1UL << ISO7816_STAT_PWR_STAT_POS)
#define | LL_ISO7816_PWR_STATE_PWRUP_RST (0x2UL << ISO7816_STAT_PWR_STAT_POS)
#define | LL_ISO7816_PWR_STATE_PWRDN_RST (0x3UL << ISO7816_STAT_PWR_STAT_POS)
#define | LL_ISO7816_PWR_STATE_PWRDN_VCC (0x4UL << ISO7816_STAT_PWR_STAT_POS)
#define | LL_ISO7816_PWR_STATE_STOP_PRE (0x5UL << ISO7816_STAT_PWR_STAT_POS)
#define | LL_ISO7816_PWR_STATE_STOP (0x6UL << ISO7816_STAT_PWR_STAT_POS)
#define | LL_ISO7816_PWR_STATE_STOP_POST (0x7UL << ISO7816_STAT_PWR_STAT_POS)
#define | LL_ISO7816_PWR_STATE_IDLE (0x8UL << ISO7816_STAT_PWR_STAT_POS)
#define | LL_ISO7816_PWR_STATE_RX_TS0 (0x9UL << ISO7816_STAT_PWR_STAT_POS)
#define | LL_ISO7816_PWR_STATE_RX_TS1 (0xAUL << ISO7816_STAT_PWR_STAT_POS)
#define | LL_ISO7816_PWR_STATE_RX (0xBUL << ISO7816_STAT_PWR_STAT_POS)
#define | LL_ISO7816_PWR_STATE_TX (0xCUL << ISO7816_STAT_PWR_STAT_POS)
#define | LL_ISO7816_PWR_STATE_TX_RX (0xDUL << ISO7816_STAT_PWR_STAT_POS)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_ISO7816_PWR_STATE_IDLE

#define LL_ISO7816_PWR_STATE_IDLE (0x8UL << ISO7816_STAT_PWR_STAT_POS)

Idle

## ◆ LL_ISO7816_PWR_STATE_OFF

#define LL_ISO7816_PWR_STATE_OFF (0x0UL << ISO7816_STAT_PWR_STAT_POS)

Off

## ◆ LL_ISO7816_PWR_STATE_PWRDN_RST

#define LL_ISO7816_PWR_STATE_PWRDN_RST (0x3UL << ISO7816_STAT_PWR_STAT_POS)

Power Down reset

## ◆ LL_ISO7816_PWR_STATE_PWRDN_VCC

#define LL_ISO7816_PWR_STATE_PWRDN_VCC (0x4UL << ISO7816_STAT_PWR_STAT_POS)

Power Down VCC

## ◆ LL_ISO7816_PWR_STATE_PWRUP_RST

#define LL_ISO7816_PWR_STATE_PWRUP_RST (0x2UL << ISO7816_STAT_PWR_STAT_POS)

Power up reset

## ◆ LL_ISO7816_PWR_STATE_PWRUP_VCC

#define LL_ISO7816_PWR_STATE_PWRUP_VCC (0x1UL << ISO7816_STAT_PWR_STAT_POS)

Power up VCC

## ◆ LL_ISO7816_PWR_STATE_RX

#define LL_ISO7816_PWR_STATE_RX (0xBUL << ISO7816_STAT_PWR_STAT_POS)

Receive

## ◆ LL_ISO7816_PWR_STATE_RX_TS0

#define LL_ISO7816_PWR_STATE_RX_TS0 (0x9UL << ISO7816_STAT_PWR_STAT_POS)

RX TS Character

## ◆ LL_ISO7816_PWR_STATE_RX_TS1

#define LL_ISO7816_PWR_STATE_RX_TS1 (0xAUL << ISO7816_STAT_PWR_STAT_POS)

RX TS Character

## ◆ LL_ISO7816_PWR_STATE_STOP

#define LL_ISO7816_PWR_STATE_STOP (0x6UL << ISO7816_STAT_PWR_STAT_POS)

Clock Stopped

## ◆ LL_ISO7816_PWR_STATE_STOP_POST

#define LL_ISO7816_PWR_STATE_STOP_POST (0x7UL << ISO7816_STAT_PWR_STAT_POS)

Exiting Clock Stop

## ◆ LL_ISO7816_PWR_STATE_STOP_PRE

#define LL_ISO7816_PWR_STATE_STOP_PRE (0x5UL << ISO7816_STAT_PWR_STAT_POS)

Preparing Clock Stop

## ◆ LL_ISO7816_PWR_STATE_TX

#define LL_ISO7816_PWR_STATE_TX (0xCUL << ISO7816_STAT_PWR_STAT_POS)

Transmit

## ◆ LL_ISO7816_PWR_STATE_TX_RX

#define LL_ISO7816_PWR_STATE_TX_RX (0xDUL << ISO7816_STAT_PWR_STAT_POS)

Transmit and Receive