Data Structures
Structures
BLE Services » Health Thermometer Service (HTS)

## Data Structures
struct | hts_evt_t
| Health Thermometer Service event. More...
struct | ieee_float32_t
| SFLOAT format (IEEE-11073 32-bit FLOAT, defined as a 32-bit vlue with 24-bit mantissa and 8-bit exponent. More...
struct | hts_meas_val_t
| Health Theromometer Measurement Character value structure. More...
struct | hts_init_t
| Health Thermometer Service init stucture. This contains all option and data needed for initialization of the service. More...

## Detailed Description