Data Fields
cscs_meas_val_t Struct Reference
BLE Services » Cycling Speed and Cadence Service (CSCS) » Structures

Cycling Speed and Cadence Measurement Character value structure. More...

`#include <cscs.h>`

## Data Fields
bool | wheel_rev_data_present
bool | crank_rev_data_present
uint32_t | cumulative_wheel_revs
uint16_t | last_wheel_event_time
uint16_t | cumulative_crank_revs
uint16_t | last_crank_event_time

## Detailed Description

Cycling Speed and Cadence Measurement Character value structure.

## Field Documentation

## ◆ crank_rev_data_present

bool cscs_meas_val_t::crank_rev_data_present

If Crank Revolution Data is present.

## ◆ cumulative_crank_revs

uint16_t cscs_meas_val_t::cumulative_crank_revs

Cumulative Crank Revolutions.

## ◆ cumulative_wheel_revs

uint32_t cscs_meas_val_t::cumulative_wheel_revs

Cumulative Wheel Revolutions.

## ◆ last_crank_event_time

uint16_t cscs_meas_val_t::last_crank_event_time

Last Crank Event Time.

## ◆ last_wheel_event_time

uint16_t cscs_meas_val_t::last_wheel_event_time

Last Wheel Event Time.

## ◆ wheel_rev_data_present

bool cscs_meas_val_t::wheel_rev_data_present

If Wheel Revolution Data is present.

The documentation for this struct was generated from the following file:

- cscs.h