Macros
PIN
Peripheral Driver » LL Driver » GPIO » Defines » GPIO Exported Constants

## Macros
#define | LL_GPIO_PIN_0 ((uint32_t)0x0001U)
#define | LL_GPIO_PIN_1 ((uint32_t)0x0002U)
#define | LL_GPIO_PIN_2 ((uint32_t)0x0004U)
#define | LL_GPIO_PIN_3 ((uint32_t)0x0008U)
#define | LL_GPIO_PIN_4 ((uint32_t)0x0010U)
#define | LL_GPIO_PIN_5 ((uint32_t)0x0020U)
#define | LL_GPIO_PIN_6 ((uint32_t)0x0040U)
#define | LL_GPIO_PIN_7 ((uint32_t)0x0080U)
#define | LL_GPIO_PIN_8 ((uint32_t)0x0100U)
#define | LL_GPIO_PIN_9 ((uint32_t)0x0200U)
#define | LL_GPIO_PIN_10 ((uint32_t)0x0400U)
#define | LL_GPIO_PIN_11 ((uint32_t)0x0800U)
#define | LL_GPIO_PIN_12 ((uint32_t)0x1000U)
#define | LL_GPIO_PIN_13 ((uint32_t)0x2000U)
#define | LL_GPIO_PIN_14 ((uint32_t)0x4000U)
#define | LL_GPIO_PIN_15 ((uint32_t)0x8000U)
#define | LL_GPIO_PIN_ALL ((uint32_t)0xFFFFU)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_GPIO_PIN_0

#define LL_GPIO_PIN_0 ((uint32_t)0x0001U)

Select pin 0

## ◆ LL_GPIO_PIN_1

#define LL_GPIO_PIN_1 ((uint32_t)0x0002U)

Select pin 1

## ◆ LL_GPIO_PIN_10

#define LL_GPIO_PIN_10 ((uint32_t)0x0400U)

Select pin 10

## ◆ LL_GPIO_PIN_11

#define LL_GPIO_PIN_11 ((uint32_t)0x0800U)

Select pin 11

## ◆ LL_GPIO_PIN_12

#define LL_GPIO_PIN_12 ((uint32_t)0x1000U)

Select pin 12

## ◆ LL_GPIO_PIN_13

#define LL_GPIO_PIN_13 ((uint32_t)0x2000U)

Select pin 13

## ◆ LL_GPIO_PIN_14

#define LL_GPIO_PIN_14 ((uint32_t)0x4000U)

Select pin 14

## ◆ LL_GPIO_PIN_15

#define LL_GPIO_PIN_15 ((uint32_t)0x8000U)

Select pin 15

## ◆ LL_GPIO_PIN_2

#define LL_GPIO_PIN_2 ((uint32_t)0x0004U)

Select pin 2

## ◆ LL_GPIO_PIN_3

#define LL_GPIO_PIN_3 ((uint32_t)0x0008U)

Select pin 3

## ◆ LL_GPIO_PIN_4

#define LL_GPIO_PIN_4 ((uint32_t)0x0010U)

Select pin 4

## ◆ LL_GPIO_PIN_5

#define LL_GPIO_PIN_5 ((uint32_t)0x0020U)

Select pin 5

## ◆ LL_GPIO_PIN_6

#define LL_GPIO_PIN_6 ((uint32_t)0x0040U)

Select pin 6

## ◆ LL_GPIO_PIN_7

#define LL_GPIO_PIN_7 ((uint32_t)0x0080U)

Select pin 7

## ◆ LL_GPIO_PIN_8

#define LL_GPIO_PIN_8 ((uint32_t)0x0100U)

Select pin 8

## ◆ LL_GPIO_PIN_9

#define LL_GPIO_PIN_9 ((uint32_t)0x0200U)

Select pin 9

## ◆ LL_GPIO_PIN_ALL

#define LL_GPIO_PIN_ALL ((uint32_t)0xFFFFU)

Select all pins