Data Fields
gap_sec_key_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Management » Structures

Security key. More...

`#include <ble_gapm.h>`

## Data Fields
uint8_t | key [MAX_KEY_LEN]

## Detailed Description

Security key.

## Field Documentation

## ◆ key

uint8_t gap_sec_key_t::key[MAX_KEY_LEN]

Key value MSB -> LSB (MSB followed by LSB).

The documentation for this struct was generated from the following file:

- ble_gapm.h