Macros
THS UUIDs
BLE Services » Throughput Service Client (THS_C) » Defines

THS service and characteristcs UUID. More...

## Macros
#define | THS_C_CONNECTION_MAX
#define | THS_SVC_UUID
#define | THS_TX_CHAR_UUID
#define | THS_RX_CHAR_UUID
#define | THS_SETTING_CHAR_UUID
#define | THS_TOGGLE_CHAR_UUID

## Detailed Description

THS service and characteristcs UUID.

## Macro Definition Documentation

## ◆ THS_C_CONNECTION_MAX

#define THS_C_CONNECTION_MAX

Value:
(10 < CFG_MAX_CONNECTIONS ?\
10 : CFG_MAX_CONNECTIONS)

Maximum number of THS Client connections.

## ◆ THS_RX_CHAR_UUID

#define THS_RX_CHAR_UUID

Value:
{0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x03, 0x03, 0xED, 0xA6}

UUID of THS Rx Characteristic.

## ◆ THS_SETTING_CHAR_UUID

#define THS_SETTING_CHAR_UUID

Value:
{0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x04, 0x03, 0xED, 0xA6}

UUID of THS Setting Characteristic.

## ◆ THS_SVC_UUID

#define THS_SVC_UUID

Value:
{0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x01, 0x03, 0xED, 0xA6}

UUID of THS Service.

## ◆ THS_TOGGLE_CHAR_UUID

#define THS_TOGGLE_CHAR_UUID

Value:
{0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x05, 0x03, 0xED, 0xA6}

UUID of THS Toggle Characteristic.

## ◆ THS_TX_CHAR_UUID

#define THS_TX_CHAR_UUID

Value:
{0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
0x0A, 0x46, 0x44, 0xD3, 0x02, 0x03, 0xED, 0xA6}

UUID of THS Tx Characteristic.