Here is a list of all documented struct and union fields with links to the struct/union documentation for each field:

### - s -

- sample_location : gls_meas_val_t
- scan_dup_filt : gap_scan_param_t
- scan_intv : gap_scan_wd_op_param_t
- scan_mode : gap_scan_param_t
- scan_param_1m : gap_ext_init_param_t , gap_ext_scan_param_t
- scan_param_coded : gap_ext_init_param_t , gap_ext_scan_param_t
- scan_req_ind_en : gap_adv_param_t
- scan_type : gap_scan_param_t
- scan_wd : gap_scan_wd_op_param_t
- scl : app_i2c_pin_cfg_t
- sclk : app_i2s_pin_cfg_t
- sda : app_i2c_pin_cfg_t
- sdi : app_i2s_pin_cfg_t
- sdo : app_i2s_pin_cfg_t
- sec : _calendar_handle , _calendar_time , prf_date_time_t
- sec_lvl : gap_lepsm_register_t
- second_cfg : gap_ext_adv_param_t
- secure_mode : pkc_init_t
- security : _exflash_handle
- seed : _ll_rng_init
- seed_mode : _rng_init
- segm_num : uds_regi_user_data_stream_t
- segm_offset : uds_regi_user_data_stream_t
- sensor_loc : hrs_c_evt_t , hrs_init_t
- sensor_location : cscs_init_t , rscs_init_t
- sensor_status_annunciation : gls_meas_val_t
- seq_num : gls_racp_filter_t
- sequence_number : gls_meas_val_t
- serial_num_str : dis_init_t
- services : ble_gattc_srvc_disc_t
- setting_type : ths_evt_t
- shdl : gatts_create_db_t
- shift_bits : _pkc_modular_shift
- shift_count : _pkc_handle
- signed_write : gattc_write_no_resp_t
- silent : ancs_ntf_flags_t
- single_tx : gap_set_pref_slave_evt_dur_param_t
- size : app_i2c_evt_t , app_i2s_evt_t , app_qspi_evt_t , app_spi_evt_t , app_uart_evt_t
- skip : gap_per_sync_param_t
- slave_latency : gap_conn_param_t , gap_conn_update_param_t , gap_init_param_t , gap_slv_pref_t
- slave_select : _ll_spim_init_t , _spi_init
- sleep_algo_dur : ble_slp_config_t
- sleep_enable : ble_slp_config_t
- slope_ext_1p0 : adc_trim_info_t
- slope_int_0p8 : adc_trim_info_t
- slope_int_1p2 : adc_trim_info_t
- slope_int_1p6 : adc_trim_info_t
- slope_int_2p0 : adc_trim_info_t
- soft_lean_mass : bcs_meas_val_t
- soft_lean_mass_present : bcs_meas_flag_t
- source : cts_c_ref_time_info_t , cts_ref_time_info_t
- speed : _i2c_init , _ll_i2c_init
- spi_abort_cplt_callback : _hal_spi_callback
- spi_error_callback : _hal_spi_callback
- spi_msp_deinit : _hal_spi_callback
- spi_msp_init : _hal_spi_callback
- spi_rx_cplt_callback : _hal_spi_callback
- spi_tx_cplt_callback : _hal_spi_callback
- spi_tx_rx_cplt_callback : _hal_spi_callback
- src_address : _ll_dma_init
- src_data_alignment : _dma_init
- src_data_width : _ll_dma_init
- src_increment : _dma_init
- src_increment_mode : _ll_dma_init
- src_peripheral : _ll_dma_init
- src_request : _dma_init
- srvc_perm : gatts_create_db_t
- start_address : dfu_nvds_info_t
- start_hdl : ble_gattc_browse_srvc_t , ble_gattc_include_t , ble_gattc_service_t , gattc_browse_inc_srvc_t , gattc_disc_char_t , gattc_prf_reg_peer_evt_t , gattc_read_by_uuid_t
- state : _adc_handle , _aes_handle , _calendar_handle , _comp_handle , _dma_handle , _dual_timer_handle , _efuse_handle , _exflash_handle , _hmac_handle , _i2c_handle , _i2s_handle , _iso7816_handle_t , _pkc_handle , _qspi_handle , _rng_handle , _spi_handle , _timer_handle , _xqspi_handle_t , dfu_adv_name_info_t , dfu_cmd_disable_t , dfu_nvds_info_t , dfu_uart_info_t , pwm_handle_t
- status : gatts_prep_write_cfm_t , gatts_read_cfm_t , gatts_write_cfm_t , gls_racp_rsp_t , prf_att_info_t
- step_calorie : wechat_pedo_meas_t
- step_count : wechat_pedo_meas_t , wechat_pedo_target_t
- step_count_target : wechat_init_t
- step_dist : wechat_pedo_meas_t
- stop_bits : _ll_uart_init_t , _uart_init , dfu_uart_info_t
- str_info : ans_c_new_alert_t , ans_new_alert_t
- string_data : ble_dis_c_read_rsp_t
- sugg_dflt_data_len : gap_dev_info_t
- suggted_max_tx_octets : gap_sugg_dflt_data_len_t
- suggted_max_tx_time : gap_sugg_dflt_data_len_t
- sup_new_alert_cat : ans_init_t
- sup_new_alert_cat_ids : ans_c_evt_t
- sup_timeout : gap_conn_param_t , gap_conn_update_cmp_t , gap_conn_update_param_t , gap_init_param_t
- sup_to : gap_conn_cmp_t
- sup_unread_alert_cat_ids : ans_c_evt_t
- sup_unread_alert_sta : ans_init_t
- supervision_to : gap_ext_conn_param_t
- suppted_max_rx_octets : gap_max_data_len_t
- suppted_max_rx_time : gap_max_data_len_t
- suppted_max_tx_octets : gap_max_data_len_t
- suppted_max_tx_time : gap_max_data_len_t
- sw_rev_str : dis_init_t
- sync_hdl : gap_sync_established_ind_t
- sync_to : gap_per_sync_param_t
- sys_id : ble_dis_c_read_rsp_t
- system_clk : boot_info_t
- systolic : bps_meas_t