Data Fields
gap_ral_dev_info_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Management » Structures

RPA list item info. More...

`#include <ble_gapm.h>`

## Data Fields
gap_bdaddr_t | bd_addr
uint8_t | priv_mode
uint8_t | peer_irk [MAX_KEY_LEN]
uint8_t | local_irk [MAX_KEY_LEN]

## Detailed Description

RPA list item info.

## Field Documentation

## ◆ bd_addr

gap_bdaddr_t gap_ral_dev_info_t::bd_addr

Peer device identity.

## ◆ local_irk

uint8_t gap_ral_dev_info_t::local_irk[MAX_KEY_LEN]

Local IRK.

## ◆ peer_irk

uint8_t gap_ral_dev_info_t::peer_irk[MAX_KEY_LEN]

Peer IRK.

## ◆ priv_mode

uint8_t gap_ral_dev_info_t::priv_mode

Privacy mode, see enum privacy_mode_t.

The documentation for this struct was generated from the following file:

- ble_gapm.h