Data Fields
gattc_read_by_uuid_t Struct Reference
BLE » Generic Attribute Profile (GATT) » Generic Attribute Profile (GATT) Client » Structures

GATTC read by characteristic UUID structure. More...

`#include <ble_gattc.h>`

## Data Fields
uint16_t | start_hdl
uint16_t | end_hdl
ble_uuid_t * | p_uuid

## Detailed Description

GATTC read by characteristic UUID structure.

## Field Documentation

## ◆ end_hdl

uint16_t gattc_read_by_uuid_t::end_hdl

End handle.

## ◆ p_uuid

ble_uuid_t* gattc_read_by_uuid_t::p_uuid

Characteristic UUID.

## ◆ start_hdl

uint16_t gattc_read_by_uuid_t::start_hdl

Start handle.

The documentation for this struct was generated from the following file:

- ble_gattc.h